<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.9.3b" moduleId="DFRobot_DFPlayer_Mini">
 <version>1</version>
 <author>Mike Causer</author>
 <title>DFRobot DFPlayer Mini</title>
 <label>DFRobot DFPlayer Mini</label>
 <date>Fri Feb 12 2016</date>
 <url>http://www.dfrobot.com/index.php?route=product/product&amp;product_id=1121</url>
 <tags>
  <tag>MP3</tag>
  <tag>WAV</tag>
  <tag>WMA</tag>
  <tag>Mini Player</tag>
  <tag>Arduino Player</tag>
  <tag>MP3 Player</tag>
  <tag>DFPlayer</tag>
  <tag>DFR0299</tag>
  <tag>Serial</tag>
  <tag>24-bit DAC</tag>
 </tags>
 <properties>
  <property name="family">DFRobot DFPlayer Mini</property>
  <property name="variant">variant 1</property>
  <property name="part number">DFR0299</property>
  <property name="layer"></property>
 </properties>
 <description>The DFPlayer Mini is a small and low cost MP3 module with an simplified output directly to the speaker. The module can be used as a stand alone module with attached battery, speaker and push buttons or used in combination with an Arduino UNO or any other with RX/TX capabilities.</description>
 <views>
  <iconView>
   <layers image="breadboard/DFRobot-DFPlayer-Mini_breadboard.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/DFRobot-DFPlayer-Mini_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/DFRobot-DFPlayer-Mini_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/DFRobot-DFPlayer-Mini_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" type="male" name="VCC">
   <description>Input voltage, Min: DC3.2V; Max: DC5.0V; Typ: DC4.2V</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" terminalId="connector0terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pad" layer="copper0"/>
     <p svgId="connector0pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" type="male" name="RX">
   <description>UART serial input</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" terminalId="connector1terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pad" layer="copper0"/>
     <p svgId="connector1pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" type="male" name="TX">
   <description>UART serial output</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" terminalId="connector2terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pad" layer="copper0"/>
     <p svgId="connector2pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector3" type="male" name="DAC_R">
   <description>Audio output right channel</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" terminalId="connector3terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pad" layer="copper0"/>
     <p svgId="connector3pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector4" type="male" name="DAC_L">
   <description>Audio output left channel</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" terminalId="connector4terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pad" layer="copper0"/>
     <p svgId="connector4pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector5" type="male" name="SPK_1">
   <description>Speaker 1 (less than 3W)</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" terminalId="connector5terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pad" layer="copper0"/>
     <p svgId="connector5pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector6" type="male" name="GND-1">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" terminalId="connector6terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pad" layer="copper0"/>
     <p svgId="connector6pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector7" type="male" name="SPK_2">
   <description>Speaker 2 (less than 3W)</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" terminalId="connector7terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pad" layer="copper0"/>
     <p svgId="connector7pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector8" type="male" name="IO_1">
   <description>Trigger port 1 - Short press to play previous, long press to decrease volume</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" terminalId="connector8terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pad" layer="copper0"/>
     <p svgId="connector8pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector9" type="male" name="GND-2">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" terminalId="connector9terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pad" layer="copper0"/>
     <p svgId="connector9pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector10" type="male" name="IO_2">
   <description>Trigger port 2 - Short press to play next, long press to increase volume</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" terminalId="connector10terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pad" layer="copper0"/>
     <p svgId="connector10pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector11" type="male" name="ADKEY_1">
   <description>AD port 1 - Trigger play first segment</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" terminalId="connector11terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pad" layer="copper0"/>
     <p svgId="connector11pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector12" type="male" name="ADKEY_2">
   <description>AD port 2 - Trigger play fifth segment</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" terminalId="connector12terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pad" layer="copper0"/>
     <p svgId="connector12pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector13" type="male" name="USB_POS">
   <description>USB+DP</description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector13pin" terminalId="connector13terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pad" layer="copper0"/>
     <p svgId="connector13pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector14" type="male" name="USB_NEG">
   <description>USB-DM</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" terminalId="connector14terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pad" layer="copper0"/>
     <p svgId="connector14pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector15" type="male" name="BUSY">
   <description>Busy - Low means playing, high means not</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" terminalId="connector15terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pad" layer="copper0"/>
     <p svgId="connector15pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
  <bus id="internal1">
   <nodeMember connectorId="connector6"/>
   <nodeMember connectorId="connector9"/>
  </bus>
 </buses>
</module>
