<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='Arduino-Fio-v22(icsp+)_bottom'>
<version>6</version>
<date>2013-04-11</date>
<author>althaus</author>
<description>The Arduino Funnel I/O (Fio) is a board designed by Shigeru Kobayashi, based on the original design from LilyPad.

Funnel is a toolkit to sketch your idea physically, and consists of software libraries and hardware. By using Funnel, the user can interface to sensors and/or actuators with various programming languages such as ActionScript 3, Processing, and Ruby.

Arduino Fio is compatible with Funnel. It has connections for a Lithium Polymer battery and includes a charge circuit over USB. An XBee socket is available on the bottom of the board. The Fio has been designed to be wirelessly reprogrammable. Checkout our tutorial on wireless bootloading!</description>
<title>Arduino Fio (Funnel I/O)</title>
<url>http://arduino.cc/en/Main/ArduinoBoardFio</url>
<tags>
<tag>Arduino Fio</tag>
<tag>ATmega328V</tag>
<tag>microcontrollerboard</tag>
</tags>
<properties>
<property name='family'>microcontroller board (arduino)</property>
<property name='type'>Arduino Fio (v22)(iscp)</property>
<property name='view'>bottom-view</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/Arduino-Fio-v22_bottom_breadboard.svg'>
<layer layerId='breadboardbreadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/Arduino-Fio-v22_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/Arduino-Fio-v22(icsp+)_bottom_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/Arduino-Fio-v22_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector22' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector22pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector22pin' terminalId='connector22terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector22pad'/><p layer='copper1' svgId='connector22pad'/></pcbView>
</views>
</connector>
<connector id='connector23' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector23pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector23pin' terminalId='connector23terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector23pad'/><p layer='copper1' svgId='connector23pad'/></pcbView>
</views>
</connector>
<connector id='connector24' type='male' name='D2'>
<description>D2</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector24pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector24pin' terminalId='connector24terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector24pad'/><p layer='copper1' svgId='connector24pad'/></pcbView>
</views>
</connector>
<connector id='connector25' type='male' name='D3 PWM'>
<description>D3 PWM</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector25pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector25pin' terminalId='connector25terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector25pad'/><p layer='copper1' svgId='connector25pad'/></pcbView>
</views>
</connector>
<connector id='connector26' type='male' name='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector26pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector26pin' terminalId='connector26terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector26pad'/><p layer='copper1' svgId='connector26pad'/></pcbView>
</views>
</connector>
<connector id='connector27' type='male' name='D5 PWM'>
<description>D5 PWM</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector27pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector27pin' terminalId='connector27terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector27pad'/><p layer='copper1' svgId='connector27pad'/></pcbView>
</views>
</connector>
<connector id='connector28' type='male' name='D6 PWM'>
<description>D6 PWM</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector28pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector28pin' terminalId='connector28terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector28pad'/><p layer='copper1' svgId='connector28pad'/></pcbView>
</views>
</connector>
<connector id='connector29' type='male' name='D7'>
<description>D7</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector29pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector29pin' terminalId='connector29terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector29pad'/><p layer='copper1' svgId='connector29pad'/></pcbView>
</views>
</connector>
<connector id='connector30' type='male' name='D8'>
<description>D8</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector30pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector30pin' terminalId='connector30terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector30pad'/><p layer='copper1' svgId='connector30pad'/></pcbView>
</views>
</connector>
<connector id='connector31' type='male' name='D9 PWM'>
<description>D9 PWM</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector31pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector31pin' terminalId='connector31terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector31pad'/><p layer='copper1' svgId='connector31pad'/></pcbView>
</views>
</connector>
<connector id='connector32' type='male' name='D10 PWM/SS'>
<description>D10 PWM/SS</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector32pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector32pin' terminalId='connector32terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector32pad'/><p layer='copper1' svgId='connector32pad'/></pcbView>
</views>
</connector>
<connector id='connector33' type='male' name='D11 PWM/MOSI'>
<description>D11 PWM/MOSI</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector33pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector33pin' terminalId='connector33terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector33pad'/><p layer='copper1' svgId='connector33pad'/></pcbView>
</views>
</connector>
<connector id='connector34' type='male' name='D12/MISO'>
<description>D12/MISO</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector34pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector34pin' terminalId='connector34terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector34pad'/><p layer='copper1' svgId='connector34pad'/></pcbView>
</views>
</connector>
<connector id='connector35' type='male' name='D13/SCK'>
<description>D13/SCK</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector35pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector35pin' terminalId='connector35terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector35pad'/><p layer='copper1' svgId='connector35pad'/></pcbView>
</views>
</connector>
<connector id='connector36' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector36pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector36pin' terminalId='connector36terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector36pad'/>
<p layer='copper1' svgId='connector36pad'/>
</pcbView>
</views>
</connector>
<connector id='connector37' type='male' name='VBATT'>
<description>VBATT</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector37pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector37pin' terminalId='connector37terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector37pad'/>
<p layer='copper1' svgId='connector37pad'/>
</pcbView>
</views>
</connector>
<connector id='connector42' type='male' name='MISO'>
<description>MISO</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector42pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector42pin' terminalId='connector42terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector42pad'/>
<p layer='copper1' svgId='connector42pad'/>
</pcbView>
</views>
</connector>
<connector id='connector43' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector43pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector43pin' terminalId='connector43terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector43pad'/>
<p layer='copper1' svgId='connector43pad'/>
</pcbView>
</views>
</connector>
<connector id='connector44' type='male' name='SCK'>
<description>SCK</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector44pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector44pin' terminalId='connector44terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector44pad'/>
<p layer='copper1' svgId='connector44pad'/>
</pcbView>
</views>
</connector>
<connector id='connector45' type='male' name='MOSI'>
<description>MOSI</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector45pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector45pin' terminalId='connector45terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector45pad'/>
<p layer='copper1' svgId='connector45pad'/>
</pcbView>
</views>
</connector>
<connector id='connector46' type='male' name='Reset'>
<description>Reset</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector46pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector46pin' terminalId='connector46terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector46pad'/>
<p layer='copper1' svgId='connector46pad'/>
</pcbView>
</views>
</connector>
<connector id='connector47' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector47pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector47pin' terminalId='connector47terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector47pad'/>
<p layer='copper1' svgId='connector47pad'/>
</pcbView>
</views>
</connector>
<connector id='connector48' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector48pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector48pin' terminalId='connector48terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector48pad'/>
<p layer='copper1' svgId='connector48pad'/></pcbView>
</views>
</connector>
<connector id='connector49' type='male' name='AREF'>
<description>AREF</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector49pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector49pin' terminalId='connector49terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector49pad'/>
<p layer='copper1' svgId='connector49pad'/></pcbView>
</views>
</connector>
<connector id='connector50' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector50pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector50pin' terminalId='connector50terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector50pad'/>
<p layer='copper1' svgId='connector50pad'/></pcbView>
</views>
</connector>
<connector id='connector51' type='male' name='D0/RXI'>
<description>D0/RXI</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector51pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector51pin' terminalId='connector51terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector51pad'/>
<p layer='copper1' svgId='connector51pad'/></pcbView>
</views>
</connector>
<connector id='connector52' type='male' name='D1/TXO'>
<description>D1/TXO</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector52pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector52pin' terminalId='connector52terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector52pad'/>
<p layer='copper1' svgId='connector52pad'/></pcbView>
</views>
</connector>
<connector id='connector53' type='male' name='DTR (Reset)'>
<description>DTR (Reset)</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector53pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector53pin' terminalId='connector53terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector53pad'/><p layer='copper1' svgId='connector53pad'/></pcbView>
</views>
</connector>
<connector id='connector54' type='male' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector54pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector54pin' terminalId='connector54terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector54pad'/><p layer='copper1' svgId='connector54pad'/></pcbView>
</views>
</connector>
<connector id='connector55' type='male' name='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector55pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector55pin' terminalId='connector55terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector55pad'/><p layer='copper1' svgId='connector55pad'/></pcbView>
</views>
</connector>
<connector id='connector56' type='male' name='A2'>
<description>A2</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector56pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector56pin' terminalId='connector56terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector56pad'/><p layer='copper1' svgId='connector56pad'/></pcbView>
</views>
</connector>
<connector id='connector57' type='male' name='A3'>
<description>A3</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector57pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector57pin' terminalId='connector57terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector57pad'/><p layer='copper1' svgId='connector57pad'/></pcbView>
</views>
</connector>
<connector id='connector58' type='male' name='A4/SDA'>
<description>A4/SDA</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector58pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector58pin' terminalId='connector58terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector58pad'/><p layer='copper1' svgId='connector58pad'/></pcbView>
</views>
</connector>
<connector id='connector59' type='male' name='A5/SCL'>
<description>A5/SCL</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector59pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector59pin' terminalId='connector59terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector59pad'/><p layer='copper1' svgId='connector59pad'/></pcbView>
</views>
</connector>
<connector id='connector60' type='male' name='A6'>
<description>A6</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector60pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector60pin' terminalId='connector60terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector60pad'/>
<p layer='copper1' svgId='connector60pad'/>
</pcbView>
</views>
</connector>
<connector id='connector61' type='male' name='A7'>
<description>A7</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector61pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector61pin' terminalId='connector61terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector61pad'/>
<p layer='copper1' svgId='connector61pad'/>
</pcbView>
</views>
</connector>
<connector id='connector62' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector62pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector62pin' terminalId='connector62terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector62pad'/>
<p layer='copper1' svgId='connector62pad'/>
</pcbView>
</views>
</connector>
<connector id='connector63' type='male' name='USB_VIN'>
<description>USB_VIN</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector63pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector63pin' terminalId='connector63terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector63pad'/>
<p layer='copper1' svgId='connector63pad'/>
</pcbView>
</views>
</connector>
<connector id='connector64' type='male' name='Off'>
<description>Off</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector64pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector64pin' terminalId='connector64terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector64pad'/>
<p layer='copper1' svgId='connector64pad'/>
</pcbView>
</views>
</connector>
<connector id='connector65' type='male' name='On'>
<description>On</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector65pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector65pin' terminalId='connector65terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector65pad'/>
<p layer='copper1' svgId='connector65pad'/>
</pcbView>
</views>
</connector>
<connector id='connector66' type='male' name='CTS'>
<description>CTS</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector66pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector66pin' terminalId='connector66terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector66pad'/>
<p layer='copper1' svgId='connector66pad'/>
</pcbView>
</views>
</connector>
<connector id='connector67' type='male' name='SLEEP_RQ'>
<description>SLEEP_RQ</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector67pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector67pin' terminalId='connector67terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector67pad'/>
<p layer='copper1' svgId='connector67pad'/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector23'/>
<nodeMember connectorId='connector36'/>
<nodeMember connectorId='connector47'/>
<nodeMember connectorId='connector48'/>
<nodeMember connectorId='connector62'/>
</bus>
<bus id='miso'>
<nodeMember connectorId='connector34'/>
<nodeMember connectorId='connector42'/>
</bus>
<bus id='vcc'>
<nodeMember connectorId='connector22'/>
<nodeMember connectorId='connector43'/>
<nodeMember connectorId='connector50'/>
</bus>
<bus id='sck'>
<nodeMember connectorId='connector35'/>
<nodeMember connectorId='connector44'/>
</bus>
<bus id='mosi'>
<nodeMember connectorId='connector33'/>
<nodeMember connectorId='connector45'/>
</bus>
</buses>
</module>
