<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Connectors-MMA_ACCEL_CONNECTOR-">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Connectors' MMA_ACCEL_CONNECTOR  -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description/>
<title>MMA_ACCEL_CONNECTOR</title>
<tags>
<tag>MMA_ACCEL_CONNECTOR</tag>
<tag>1X08</tag>
</tags>
<properties>
<property name="package">1x08</property>
<property name="family">sparkfun mma_accel_connector</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/generic_female_pin_header_8_100mil_bread.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-connectors_mma_con_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/nsjumper_8_100mil_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
<layer layerId="copper0"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/1X08.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector1" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector1pin"/>
<p layer="copper1" svgId="connector1pin"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="GS1" type="male">
<description>GS1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector5pin"/>
<p layer="copper1" svgId="connector5pin"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="GS2" type="male">
<description>GS2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector6pin"/>
<p layer="copper1" svgId="connector6pin"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="SLP" type="male">
<description>SLP</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector7pin"/>
<p layer="copper1" svgId="connector7pin"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="VCC" type="male">
<description>VCC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector0pin"/>
<p layer="copper1" svgId="connector0pin"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="X" type="male">
<description>X</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector2pin"/>
<p layer="copper1" svgId="connector2pin"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="Y" type="male">
<description>Y</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector3pin"/>
<p layer="copper1" svgId="connector3pin"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="Z" type="male">
<description>Z</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector4pin"/>
<p layer="copper1" svgId="connector4pin"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>