<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.9.0b.02.18.4756' moduleId='pinoccio_board'>
<version>4</version>
<date>2014-09-10</date>
<author>f.althaus</author>
<description>The Arduino-compatible atomic unit of Pinoccio: Every Field Scout can talk to any other Field Scout via radio (up to about 100m away). The built-in temperature sensor and RGB LED are perfect for starter projects.</description>
<title>pinocc.io scout</title>
<url>https://pinocc.io/</url>
<tags>
<tag>pinocc.io</tag>
<tag>scout</tag>
<tag>atmega</tag>
<tag>mega16u2</tag>
</tags>
<properties>
<property name='family'>pinocc.io</property>
<property name='type'>scout</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/pinoccio_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/pinoccio_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/pinoccio_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='icon/pinoccio_icon.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector62' type='female' name='Switch2'>
<description>Switch2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector62pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector62pin' terminalId='connector62terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector62pad'/><p layer='copper1' svgId='connector62pad'/></pcbView>
</views>
</connector>
<connector id='connector63' type='female' name='Switch1'>
<description>Switch1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector63pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector63pin' terminalId='connector63terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector63pad'/><p layer='copper1' svgId='connector63pad'/></pcbView>
</views>
</connector>
<connector id='connector64' type='female' name='VBAT-'>
<description>VBAT-</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector64pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector64pin' terminalId='connector64terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector64pad'/><p layer='copper1' svgId='connector64pad'/></pcbView>
</views>
</connector>
<connector id='connector65' type='female' name='VBAT+'>
<description>VBAT+</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector65pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector65pin' terminalId='connector65terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector65pad'/><p layer='copper1' svgId='connector65pad'/></pcbView>
</views>
</connector>
<connector id='connector66' type='female' name='VUSB'>
<description>VUSB</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector66pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector66pin' terminalId='connector66terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector66pad'/><p layer='copper1' svgId='connector66pad'/></pcbView>
</views>
</connector>
<connector id='connector67' type='female' name='BKPK-BUS'>
<description>BKPK-BUS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector67pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector67pin' terminalId='connector67terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector67pad'/><p layer='copper1' svgId='connector67pad'/></pcbView>
</views>
</connector>
<connector id='connector68' type='female' name='RESET-EN'>
<description>RESET-EN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector68pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector68pin' terminalId='connector68terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector68pad'/><p layer='copper1' svgId='connector68pad'/></pcbView>
</views>
</connector>
<connector id='connector69' type='female' name='SCK'>
<description>SCK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector69pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector69pin' terminalId='connector69terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector69pad'/><p layer='copper1' svgId='connector69pad'/></pcbView>
</views>
</connector>
<connector id='connector70' type='female' name='MISO'>
<description>MISO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector70pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector70pin' terminalId='connector70terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector70pad'/><p layer='copper1' svgId='connector70pad'/></pcbView>
</views>
</connector>
<connector id='connector71' type='female' name='MOSI'>
<description>MOSI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector71pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector71pin' terminalId='connector71terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector71pad'/><p layer='copper1' svgId='connector71pad'/></pcbView>
</views>
</connector>
<connector id='connector72' type='female' name='SS'>
<description>SS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector72pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector72pin' terminalId='connector72terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector72pad'/><p layer='copper1' svgId='connector72pad'/></pcbView>
</views>
</connector>
<connector id='connector73' type='female' name='RX0'>
<description>RX0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector73pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector73pin' terminalId='connector73terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector73pad'/><p layer='copper1' svgId='connector73pad'/></pcbView>
</views>
</connector>
<connector id='connector74' type='female' name='TX0'>
<description>TX0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector74pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector74pin' terminalId='connector74terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector74pad'/><p layer='copper1' svgId='connector74pad'/></pcbView>
</views>
</connector>
<connector id='connector75' type='female' name='D2'>
<description>D2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector75pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector75pin' terminalId='connector75terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector75pad'/><p layer='copper1' svgId='connector75pad'/></pcbView>
</views>
</connector>
<connector id='connector76' type='female' name='D3'>
<description>D3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector76pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector76pin' terminalId='connector76terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector76pad'/><p layer='copper1' svgId='connector76pad'/></pcbView>
</views>
</connector>
<connector id='connector77' type='female' name='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector77pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector77pin' terminalId='connector77terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector77pad'/><p layer='copper1' svgId='connector77pad'/></pcbView>
</views>
</connector>
<connector id='connector78' type='female' name='D5'>
<description>D5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector78pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector78pin' terminalId='connector78terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector78pad'/><p layer='copper1' svgId='connector78pad'/></pcbView>
</views>
</connector>
<connector id='connector79' type='female' name='D6'>
<description>D6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector79pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector79pin' terminalId='connector79terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector79pad'/><p layer='copper1' svgId='connector79pad'/></pcbView>
</views>
</connector>
<connector id='connector80' type='female' name='D7'>
<description>D7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector80pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector80pin' terminalId='connector80terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector80pad'/><p layer='copper1' svgId='connector80pad'/></pcbView>
</views>
</connector>
<connector id='connector81' type='female' name='D8'>
<description>D8</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector81pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector81pin' terminalId='connector81terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector81pad'/><p layer='copper1' svgId='connector81pad'/></pcbView>
</views>
</connector>
<connector id='connector82' type='female' name='3V3'>
<description>3V3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector82pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector82pin' terminalId='connector82terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector82pad'/><p layer='copper1' svgId='connector82pad'/></pcbView>
</views>
</connector>
<connector id='connector83' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector83pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector83pin' terminalId='connector83terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector83pad'/><p layer='copper1' svgId='connector83pad'/></pcbView>
</views>
</connector>
<connector id='connector84' type='female' name='VBAT'>
<description>VBAT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector84pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector84pin' terminalId='connector84terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector84pad'/><p layer='copper1' svgId='connector84pad'/></pcbView>
</views>
</connector>
<connector id='connector85' type='female' name='RX1'>
<description>RX1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector85pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector85pin' terminalId='connector85terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector85pad'/><p layer='copper1' svgId='connector85pad'/></pcbView>
</views>
</connector>
<connector id='connector86' type='female' name='TX1'>
<description>TX1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector86pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector86pin' terminalId='connector86terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector86pad'/><p layer='copper1' svgId='connector86pad'/></pcbView>
</views>
</connector>
<connector id='connector87' type='female' name='SCL'>
<description>SCL</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector87pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector87pin' terminalId='connector87terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector87pad'/><p layer='copper1' svgId='connector87pad'/></pcbView>
</views>
</connector>
<connector id='connector88' type='female' name='SDA'>
<description>SDA</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector88pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector88pin' terminalId='connector88terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector88pad'/><p layer='copper1' svgId='connector88pad'/></pcbView>
</views>
</connector>
<connector id='connector89' type='female' name='AREF'>
<description>AREF</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector89pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector89pin' terminalId='connector89terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector89pad'/><p layer='copper1' svgId='connector89pad'/></pcbView>
</views>
</connector>
<connector id='connector90' type='female' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector90pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector90pin' terminalId='connector90terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector90pad'/><p layer='copper1' svgId='connector90pad'/></pcbView>
</views>
</connector>
<connector id='connector91' type='female' name='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector91pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector91pin' terminalId='connector91terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector91pad'/><p layer='copper1' svgId='connector91pad'/></pcbView>
</views>
</connector>
<connector id='connector92' type='female' name='A2'>
<description>A2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector92pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector92pin' terminalId='connector92terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector92pad'/><p layer='copper1' svgId='connector92pad'/></pcbView>
</views>
</connector>
<connector id='connector93' type='female' name='A3'>
<description>A3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector93pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector93pin' terminalId='connector93terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector93pad'/><p layer='copper1' svgId='connector93pad'/></pcbView>
</views>
</connector>
<connector id='connector94' type='female' name='A4'>
<description>A4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector94pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector94pin' terminalId='connector94terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector94pad'/><p layer='copper1' svgId='connector94pad'/></pcbView>
</views>
</connector>
<connector id='connector95' type='female' name='A5'>
<description>A5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector95pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector95pin' terminalId='connector95terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector95pad'/><p layer='copper1' svgId='connector95pad'/></pcbView>
</views>
</connector>
<connector id='connector96' type='female' name='A6'>
<description>A6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector96pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector96pin' terminalId='connector96terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector96pad'/><p layer='copper1' svgId='connector96pad'/></pcbView>
</views>
</connector>
<connector id='connector97' type='female' name='A7'>
<description>A7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector97pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector97pin' terminalId='connector97terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector97pad'/><p layer='copper1' svgId='connector97pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector64'/>
<nodeMember connectorId='connector83'/>
</bus>
<bus id='vbat'>
<nodeMember connectorId='connector65'/>
<nodeMember connectorId='connector84'/>
</bus>
</buses>
</module>
