<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.9.3b" moduleId="optical_jack_orj-8">
    <version>4</version>
    <author>f.althaus</author>
    <title>optical jack orj-8</title>
    <label>ORJ-8</label>
    <date>09.02.2017</date>
    <tags>
           <tag>optical</tag>
        <tag>orj-8</tag>
        <tag>jack</tag>
        <tag>receiver</tag>
      <tag>orj</tag>
    </tags>
    <properties>
        <property name="family">Optical Jack</property>
        <property name="Form">receiver</property>
        <property name="package">tht</property>
      </properties>
    <description>Optical Jacks from CLIFF Receiver ORJ-8</description>
    <views>
        <iconView>
            <layers image="breadboard/optical_jack_orj-8_breadoard.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/optical_jack_orj-8_breadoard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView fliphorizontal="true">
            <layers image="schematic/optical_jack_orj-8_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/optical_jack_orj-8_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
	      <layer layerId="copper1"/>
	</layers>
        </pcbView>
    </views>
    <connectors>
   <connector id="connector0" name="pin1" type="male">
   <description>pin 1</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pin"/>
    <p layer="copper1" svgId="connector0pin"/></pcbView>
   </views>
  </connector>
   <connector id="connector0" name="pin1" type="male">
   <description>Vcc</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pin"/>
    <p layer="copper1" svgId="connector0pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector1" name="pin2" type="male">
   <description>GND</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pin"/>
    <p layer="copper1" svgId="connector1pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector2" name="pin3" type="male">
   <description>Vout</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector2pin"/>
    <p layer="copper1" svgId="connector2pin"/></pcbView>
   </views>
  </connector>

      <connector id="connector3" name="pin4" type="male">
   <description>pin 4</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector3pin"/>
    <p layer="copper1" svgId="connector3pin"/></pcbView>
   </views>
  </connector>

      <connector id="connector4" name="pin5" type="male">
   <description>pin 5</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector4pin"/>
    <p layer="copper1" svgId="connector4pin"/></pcbView>
   </views>
  </connector>
  
    </connectors>
</module>