<?xml version='1.0' encoding='UTF-8' standalone='no'?>
<module referenceFile="router_1.fzp" moduleId="router_1" fritzingVersion="0.9.3b">
  <version>4</version>
  <author>Nitay Megides (modified by vanepp July 2019)</author>
  <title>Rounter OpenMesh</title>
  <label>Router</label>
  <date>Sat Jan 12 2019</date>
  <url>https://www.andymark.com/products/open-mesh-om5p-ac-dual-band-1-17-gbps-access-point-radio</url>
  <tags>
    <tag>Router</tag>
    <tag>OpenMesh</tag>
    <tag>FRC</tag>
  </tags>
  <properties>
    <property name="family">FRC</property>
    <property name="editable pin labels">false</property>
    <property name="layer"/>
    <property name="part number"/>
    <property name="variant">variant 1</property>
  </properties>
  <description>Open-Mesh OM5P-AC Dual Band 1.17 Gbps Access Point aka: FRC Radio. Note pcb view is supressed as this device will not fit on a pcb.</description>
  <views>
    <iconView>
      <layers image="icon/router_1_icon.svg">
        <layer layerId="icon"/>
      </layers>
    </iconView>
    <breadboardView>
      <layers image="breadboard/router_1_breadboard.svg">
        <layer layerId="breadboard"/>
      </layers>
    </breadboardView>
    <schematicView>
      <layers image="schematic/router_1_schematic.svg">
        <layer layerId="schematic"/>
      </layers>
    </schematicView>
  </views>
  <connectors>
    <connector type="male" id="connector0" name="V_neg">
      <description>Negative 12V power connection</description>
      <views>
        <breadboardView>
          <p svgId="connector0pin" layer="breadboard"/>
        </breadboardView>
        <schematicView>
          <p svgId="connector0pin" terminalId="connector0terminal" layer="schematic"/>
        </schematicView>
      </views>
    </connector>
    <connector type="male" id="connector1" name="V_pos">
      <description>Positive 12V power connection</description>
      <views>
        <breadboardView>
          <p svgId="connector1pin" layer="breadboard"/>
        </breadboardView>
        <schematicView>
          <p svgId="connector1pin" terminalId="connector1terminal" layer="schematic"/>
        </schematicView>
      </views>
    </connector>
    <connector type="male" id="connector2" name="ETH_right">
      <description>Right Ethernet connection 18-24V POE</description>
      <views>
        <breadboardView>
          <p svgId="connector2pin" layer="breadboard"/>
        </breadboardView>
        <schematicView>
          <p svgId="connector2pin" terminalId="connector2terminal" layer="schematic"/>
        </schematicView>
      </views>
    </connector>
    <connector type="male" id="connector3" name="ETH_left">
      <description>Left Ethernet connection 802.3af POE</description>
      <views>
        <breadboardView>
          <p svgId="connector3pin" layer="breadboard"/>
        </breadboardView>
        <schematicView>
          <p svgId="connector3pin" terminalId="connector3terminal" layer="schematic"/>
        </schematicView>
      </views>
    </connector>
  </connectors>
</module>
