<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.5.2b.02.18.4756" moduleId="arduino_uno(rev3)-icsp_only" referenceFile="arduino_uno(rev3)-icsp(1).fzp">
    <version>5</version>
    <date>Mon Nov 18 2013</date>
    <author>althaus</author>
    <description>The Arduino Uno is a microcontroller board based on the ATmega328 (datasheet). It has 14 digital input/output pins (of which 6 can be used as PWM outputs), 6 analog inputs, a 16 MHz ceramic resonator, a USB connection, a power jack, an ICSP header, and a reset button. It contains everything needed to support the microcontroller; simply connect it to a computer with a USB cable or power it with a AC-to-DC adapter or battery to get started.
The Uno differs from all preceding boards in that it does not use the FTDI USB-to-serial driver chip. Instead, it features the Atmega16U2 (Atmega8U2 up to version R2) programmed as a USB-to-serial converter.
Revision 2 of the Uno board has a resistor pulling the 8U2 HWB line to ground, making it easier to put into DFU mode.
Revision 3 of the board has the following new features:
1.0 pinout: added SDA and SCL pins that are near to the AREF pin and two other new pins placed near to the RESET pin, the IOREF that allow the shields to adapt to the voltage provided from the board. In future, shields will be compatible both with the board that use the AVR, which operate with 5V and with the Arduino Due that operate with 3.3V. The second one is a not connected pin, that is reserved for future purposes.
Stronger RESET circuit.
Atmega 16U2 replace the 8U2.
"Uno" means one in Italian and is named to mark the upcoming release of Arduino 1.0. The Uno and version 1.0 will be the reference versions of Arduino, moving forward. The Uno is the latest in a series of USB Arduino boards, and the reference model for the Arduino platform; for a comparison with previous versions, see the index of Arduino boards.</description>
    <title>Arduino Uno (Rev3) - ICSP</title>
    <url>http://arduino.cc/en/Main/ArduinoBoardUno</url>
    <tags>
        <tag>rev3</tag>
        <tag>uno</tag>
        <tag>arduino</tag>
        <tag>ATmega328</tag>
    </tags>
    <properties>
        <property name="family">microcontroller board (arduino)</property>
        <property name="part number"/>
        <property name="type">Arduino UNO (Rev3) - ICSP (w/o icsp2)</property>
        <property name="layer"/>
    </properties>
    <views>
        <breadboardView>
            <layers image="breadboard/arduino_uno(rev3)-icsp(1)_breadboard.svg">
                <layer layerId="breadboardbreadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/arduino_uno(rev3)-icsp(1)_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/arduino_uno(rev3)-icsp(1)_pcb.svg">
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper0"/>
            </layers>
        </pcbView>
        <iconView>
            <layers image="breadboard/arduino_uno(rev3)-icsp_breadboard.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
    </views>
    <connectors>
        <connector type="female" id="connector0" name="A0">
            <description>A0</description>
            <views>
                <breadboardView>
                    <p svgId="connector0pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector0pad" layer="copper0"/>
                    <p svgId="connector0pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector1" name="A1">
            <description>A1</description>
            <views>
                <breadboardView>
                    <p svgId="connector1pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1pad" layer="copper0"/>
                    <p svgId="connector1pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector2" name="A2">
            <description>A2</description>
            <views>
                <breadboardView>
                    <p svgId="connector2pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2pad" layer="copper0"/>
                    <p svgId="connector2pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector3" name="A3">
            <description>A3</description>
            <views>
                <breadboardView>
                    <p svgId="connector3pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3pad" layer="copper0"/>
                    <p svgId="connector3pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector4" name="A4/SDA">
            <description>A4/SDA</description>
            <views>
                <breadboardView>
                    <p svgId="connector4pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector4pad" layer="copper0"/>
                    <p svgId="connector4pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector5" name="A5/SCL">
            <description>A5/SCL</description>
            <views>
                <breadboardView>
                    <p svgId="connector5pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector5pad" layer="copper0"/>
                    <p svgId="connector5pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector39" name="ICSP MISO">
            <description>ICSP MISO</description>
            <views>
                <breadboardView>
                    <p svgId="connector39pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector39pin" layer="schematic" terminalId="connector39terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector39pad" layer="copper0"/>
                    <p svgId="connector39pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector40" name="5V">
            <description>5V</description>
            <views>
                <breadboardView>
                    <p svgId="connector40pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector40pin" layer="schematic" terminalId="connector40terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector40pad" layer="copper0"/>
                    <p svgId="connector40pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector41" name="ICSP SCK">
            <description>ICSP SCK</description>
            <views>
                <breadboardView>
                    <p svgId="connector41pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector41pin" layer="unknown" terminalId="connector41terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector41pad" layer="copper0"/>
                    <p svgId="connector41pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector42" name="ICSP MOSI">
            <description>ICSP MOSI</description>
            <views>
                <breadboardView>
                    <p svgId="connector42pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector42pin" layer="schematic" terminalId="connector42terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector42pad" layer="copper0"/>
                    <p svgId="connector42pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector43" name="RESET">
            <description>RESET</description>
            <views>
                <breadboardView>
                    <p svgId="connector43pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector43pin" layer="schematic" terminalId="connector43terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector43pad" layer="copper0"/>
                    <p svgId="connector43pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector44" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector44pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector44pin" layer="schematic" terminalId="connector44terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector44pad" layer="copper0"/>
                    <p svgId="connector44pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>

        <connector type="female" id="connector51" name="D8">
            <description>D8</description>
            <views>
                <breadboardView>
                    <p svgId="connector51pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector51pin" layer="schematic" terminalId="connector51terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector51pad" layer="copper0"/>
                    <p svgId="connector51pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector52" name="D9 PWM">
            <description>D9 PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector52pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector52pin" layer="schematic" terminalId="connector52terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector52pad" layer="copper0"/>
                    <p svgId="connector52pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector53" name="D10 PWM/SS">
            <description>D10 PWM/SS</description>
            <views>
                <breadboardView>
                    <p svgId="connector53pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector53pin" layer="schematic" terminalId="connector53terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector53pad" layer="copper0"/>
                    <p svgId="connector53pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector54" name="D11 PWM/MOSI">
            <description>D11 PWM/MOSI</description>
            <views>
                <breadboardView>
                    <p svgId="connector54pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector54pin" layer="schematic" terminalId="connector54terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector54pad" layer="copper0"/>
                    <p svgId="connector54pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector55" name="D12/MISO">
            <description>D12/MISO</description>
            <views>
                <breadboardView>
                    <p svgId="connector55pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector55pin" layer="schematic" terminalId="connector55terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector55pad" layer="copper0"/>
                    <p svgId="connector55pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector56" name="D13/SCK">
            <description>D13/SCK</description>
            <views>
                <breadboardView>
                    <p svgId="connector56pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector56pin" layer="schematic" terminalId="connector56terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector56pad" layer="copper0"/>
                    <p svgId="connector56pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector57" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector57pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector57pin" layer="schematic" terminalId="connector57terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector57pad" layer="copper0"/>
                    <p svgId="connector57pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector58" name="AREF">
            <description>AREF</description>
            <views>
                <breadboardView>
                    <p svgId="connector58pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector58pin" layer="schematic" terminalId="connector58terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector58pad" layer="copper0"/>
                    <p svgId="connector58pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector59" name="A4/SDA">
            <description>A4/SDA</description>
            <views>
                <breadboardView>
                    <p svgId="connector59pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector59pin" layer="schematic" terminalId="connector59terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector59pad" layer="copper0"/>
                    <p svgId="connector59pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector60" name="A5/SCL">
            <description>A5/SCL</description>
            <views>
                <breadboardView>
                    <p svgId="connector60pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector60pin" layer="schematic" terminalId="connector60terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector60pad" layer="copper0"/>
                    <p svgId="connector60pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector61" name="D0/RX">
            <description>D0/RX</description>
            <views>
                <breadboardView>
                    <p svgId="connector61pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector61pin" layer="schematic" terminalId="connector61terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector61pad" layer="copper0"/>
                    <p svgId="connector61pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector62" name="D1/TX">
            <description>D1/TX</description>
            <views>
                <breadboardView>
                    <p svgId="connector62pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector62pin" layer="schematic" terminalId="connector62terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector62pad" layer="copper0"/>
                    <p svgId="connector62pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector63" name="D2">
            <description>D2</description>
            <views>
                <breadboardView>
                    <p svgId="connector63pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector63pin" layer="schematic" terminalId="connector63terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector63pad" layer="copper0"/>
                    <p svgId="connector63pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector64" name="D3 PWM">
            <description>D3 PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector64pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector64pin" layer="schematic" terminalId="connector64terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector64pad" layer="copper0"/>
                    <p svgId="connector64pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector65" name="D4">
            <description>D4</description>
            <views>
                <breadboardView>
                    <p svgId="connector65pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector65pin" layer="schematic" terminalId="connector65terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector65pad" layer="copper0"/>
                    <p svgId="connector65pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector66" name="D5 PWM">
            <description>D5 PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector66pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector66pin" layer="schematic" terminalId="connector66terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector66pad" layer="copper0"/>
                    <p svgId="connector66pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector67" name="D6 PWM">
            <description>D6 PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector67pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector67pin" layer="schematic" terminalId="connector67terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector67pad" layer="copper0"/>
                    <p svgId="connector67pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector68" name="D7">
            <description>D7</description>
            <views>
                <breadboardView>
                    <p svgId="connector68pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector68pin" layer="schematic" terminalId="connector68terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector68pad" layer="copper0"/>
                    <p svgId="connector68pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector84" name="IOREF">
            <description>IOREF</description>
            <views>
                <breadboardView>
                    <p svgId="connector84pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector84pin" layer="schematic" terminalId="connector84terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector84pad" layer="copper0"/>
                    <p svgId="connector84pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector85" name="RESET">
            <description>RESET</description>
            <views>
                <breadboardView>
                    <p svgId="connector85pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector85pin" layer="schematic" terminalId="connector85terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector85pad" layer="copper0"/>
                    <p svgId="connector85pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector86" name="3V3">
            <description>3V3</description>
            <views>
                <breadboardView>
                    <p svgId="connector86pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector86pin" layer="schematic" terminalId="connector86terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector86pad" layer="copper0"/>
                    <p svgId="connector86pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector87" name="5V">
            <description>5V</description>
            <views>
                <breadboardView>
                    <p svgId="connector87pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector87pin" layer="schematic" terminalId="connector87terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector87pad" layer="copper0"/>
                    <p svgId="connector87pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector88" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector88pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector88pin" layer="schematic" terminalId="connector88terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector88pad" layer="copper0"/>
                    <p svgId="connector88pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector89" name="GND">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p svgId="connector89pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector89pin" layer="schematic" terminalId="connector89terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector89pad" layer="copper0"/>
                    <p svgId="connector89pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector90" name="VIN">
            <description>VIN</description>
            <views>
                <breadboardView>
                    <p svgId="connector90pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector90pin" layer="schematic" terminalId="connector90terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector90pad" layer="copper0"/>
                    <p svgId="connector90pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="female" id="connector91" name="N/C">
            <description>not connected</description>
            <views>
                <breadboardView>
                    <p svgId="connector91pin" layer="breadboardbreadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector91pin" layer="schematic" terminalId="connector91terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector91pin" layer="copper0"/>
                    <p svgId="connector91pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
    <buses>
        <bus id="+5v">
            <nodeMember connectorId="connector40"/>

            <nodeMember connectorId="connector87"/>
        </bus>
        <bus id="gnd">
            <nodeMember connectorId="connector44"/>
            <nodeMember connectorId="connector57"/>
            <nodeMember connectorId="connector88"/>
            <nodeMember connectorId="connector89"/>
        </bus>
        <bus id="mosi">
            <nodeMember connectorId="connector42"/>

        </bus>
        <bus id="miso">
            <nodeMember connectorId="connector39"/>

        </bus>
        <bus id="sck">
            <nodeMember connectorId="connector41"/>

        </bus>
        <bus id="ad4/sda">
            <nodeMember connectorId="connector4"/>
            <nodeMember connectorId="connector59"/>
        </bus>
        <bus id="ad5/scl">
            <nodeMember connectorId="connector5"/>
            <nodeMember connectorId="connector60"/>
        </bus>
        <bus id="reset">
            <nodeMember connectorId="connector43"/>
            <nodeMember connectorId="connector85"/>
        </bus>
    </buses>
</module>
