<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.7.1b.03.10.5908" moduleId="PCF8574A_f92705dc5bbcb278fb8f55ff08c7872a_1" referenceFile="PCF8574.fzp">
 <version>5</version>
 <author>D&amp;C</author>
 <title>PCF8574</title>
 <label>U</label>
 <date>2019-09-14</date>
 <tags>
  <tag>DIP</tag>
  <tag>I2C</tag>
  <tag>Expander Port</tag>
 </tags>
 <properties>
  <property name="package">DIP16 [THT]</property>
  <property name="family">pcf8574</property>
  <property name="type">PCF8574</property>
  <property name="part number"></property>
  <property name="layer"></property>
  <property name="variant">variant 1</property>
 </properties>
 <description>8-bit parallel-load shift registers</description>
 <views>
  <pcbView>
   <layers image="pcb/PCF8574A_2.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/PCF8574A_2.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/PCF8574A_2.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/PCF8574A_2.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
 </views>
 <connectors>
  <connector id="connector15" name="VCC" type="male">
   <description>Positive supply voltage</description>
   <views>
    <breadboardView>
     <p terminalId="connector15terminal" layer="breadboard" svgId="connector15pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector15terminal" layer="schematic" svgId="connector15pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector15pin"/>
     <p layer="copper0" svgId="connector15pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector3" name="P0" type="male">
   <description>Output pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector3terminal" layer="breadboard" svgId="connector3pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector3terminal" layer="schematic" svgId="connector3pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector3pin"/>
     <p layer="copper0" svgId="connector3pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector4" name="P1" type="male">
   <description>Output pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector4terminal" layer="breadboard" svgId="connector4pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector4terminal" layer="schematic" svgId="connector4pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector4pin"/>
     <p layer="copper0" svgId="connector4pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector5" name="P2" type="male">
   <description>Output pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector5terminal" layer="breadboard" svgId="connector5pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector5terminal" layer="schematic" svgId="connector5pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector5pin"/>
     <p layer="copper0" svgId="connector5pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector6" name="P3" type="male">
   <description>Output pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector6terminal" layer="breadboard" svgId="connector6pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector6terminal" layer="schematic" svgId="connector6pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector6pin"/>
     <p layer="copper0" svgId="connector6pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector7" name="GND" type="male">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p terminalId="connector7terminal" layer="breadboard" svgId="connector7pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector7terminal" layer="schematic" svgId="connector7pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector7pin"/>
     <p layer="copper0" svgId="connector7pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector8" name="P4" type="male">
   <description>Output pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector8terminal" layer="breadboard" svgId="connector8pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector8terminal" layer="schematic" svgId="connector8pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector8pin"/>
     <p layer="copper0" svgId="connector8pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector9" name="P5" type="male">
   <description>Output pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector9terminal" layer="breadboard" svgId="connector9pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector9terminal" layer="schematic" svgId="connector9pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector9pin"/>
     <p layer="copper0" svgId="connector9pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector10" name="P6" type="male">
   <description>Output pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector10terminal" layer="breadboard" svgId="connector10pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector10terminal" layer="schematic" svgId="connector10pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector10pin"/>
     <p layer="copper0" svgId="connector10pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector11" name="P7" type="male">
   <description>Output pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector11terminal" layer="breadboard" svgId="connector11pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector11terminal" layer="schematic" svgId="connector11pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector11pin"/>
     <p layer="copper0" svgId="connector11pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector12" name="INT" type="male">
   <description>Interrupt pin, (active low)</description>
   <views>
    <breadboardView>
     <p terminalId="connector12terminal" layer="breadboard" svgId="connector12pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector12terminal" layer="schematic" svgId="connector12pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector12pin"/>
     <p layer="copper0" svgId="connector12pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector0" name="A0" type="male">
   <description>Address pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector0terminal" layer="breadboard" svgId="connector0pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector0terminal" layer="schematic" svgId="connector0pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector0pin"/>
     <p layer="copper0" svgId="connector0pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" name="A1" type="male">
   <description>Address pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector1terminal" layer="breadboard" svgId="connector1pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector1terminal" layer="schematic" svgId="connector1pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector1pin"/>
     <p layer="copper0" svgId="connector1pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector13" name="SCL" type="male">
   <description>Serial Clock pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector13terminal" layer="breadboard" svgId="connector13pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector13terminal" layer="schematic" svgId="connector13pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector13pin"/>
     <p layer="copper0" svgId="connector13pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector14" name="SDA" type="male">
   <description>Serial Data pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector14terminal" layer="breadboard" svgId="connector14pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector14terminal" layer="schematic" svgId="connector14pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector14pin"/>
     <p layer="copper0" svgId="connector14pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" name="A2" type="male">
   <description>Output Pin</description>
   <views>
    <breadboardView>
     <p terminalId="connector2terminal" layer="breadboard" svgId="connector2pin"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector2terminal" layer="schematic" svgId="connector2pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper1" svgId="connector2pin"/>
     <p layer="copper0" svgId="connector2pin"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>
