<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.9.3" moduleId="PocketBeagle" referenceFile="PocketBeagle.fzp">
 <version>4</version>
 <date>Di Dez 5 2017</date>
 <author>Jason Kridner + F.Althaus</author>
 <description>PocketBeagle® is an ultra-tiny-yet-complete Linux-enabled, community-supported, open-source USB-key-fob computer. PocketBeagle features an incredible low cost, slick design and simple usage, making PocketBeagle® the ideal development board for beginners and professionals alike. You develop directly in a web browser and PocketBeagle® can easily be set back to factory conditions, leaving you free to experiment.<br />
 512MB DDR3 RAM integrated<br />
Integrated power management<br />
2×32-bit 200-MHz programmable real-time units (PRUs)<br />
ARM Cortex-M3<br />
</description>
 <title>PocketBeagle</title>
 <url>https://beagleboard.org/pocket</url>
 <tags>
  <tag>Beagle</tag>
  <tag>mint-tin</tag>
  <tag>Linux</tag>
  <tag>SBC</tag>
  <tag>PocketBeagle</tag>
 </tags>
 <properties>
  <property name="family">Computer</property>
  <property name="variant">A2</property>
  <property name="part number"></property>
 </properties>
 <views>
  <breadboardView>
   <layers image="breadboard/PocketBeagle_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/PocketBeagle_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/PocketBeagle_pcb.svg">
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/PocketBeagle_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector id="connector5" type="pad" name="VIN">
   <description>VIN</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector5terminal" svgId="connector5pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector5pad"/>
     <p layer="copper1" svgId="connector5pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector18" type="pad" name="3.3V">
   <description>3.3V</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector18terminal" svgId="connector18pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector18pad"/>
     <p layer="copper1" svgId="connector18pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector28" type="pad" name="VOUT">
   <description>VOUT</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector28pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector28terminal" svgId="connector28pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector28pad"/>
     <p layer="copper1" svgId="connector28pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector53" type="pad" name="VOUT">
   <description>VOUT</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector53pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector53terminal" svgId="connector53pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector53pad"/>
     <p layer="copper1" svgId="connector53pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector63" type="pad" name="3.3V">
   <description>3.3V</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector63pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector63terminal" svgId="connector63pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector63pad"/>
     <p layer="copper1" svgId="connector63pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector52" type="pad" name="POWER.BUTTON">
   <description>POWER.BUTTON</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector52pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector52terminal" svgId="connector52pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector52pad"/>
     <p layer="copper1" svgId="connector52pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector21" type="pad" name="AIN.VREFN">
   <description>AIN.VREFN</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector21terminal" svgId="connector21pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector21pad"/>
     <p layer="copper1" svgId="connector21pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector22" type="pad" name="AIN.VREFP">
   <description>AIN.VREFP</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector22terminal" svgId="connector22pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector22pad"/>
     <p layer="copper1" svgId="connector22pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector23" type="pad" name="AIN0(1.8V)">
   <description>AIN0(1.8V)</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector23terminal" svgId="connector23pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector23pad"/>
     <p layer="copper1" svgId="connector23pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector25" type="pad" name="AIN1(1.8V)">
   <description>AIN1(1.8V)</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector25terminal" svgId="connector25pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector25pad"/>
     <p layer="copper1" svgId="connector25pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector27" type="pad" name="AIN2(1.8V)">
   <description>AIN2(1.8V)</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector27terminal" svgId="connector27pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector27pad"/>
     <p layer="copper1" svgId="connector27pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector29" type="pad" name="AIN3(1.8V)">
   <description>AIN3(1.8V)</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector29pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector29terminal" svgId="connector29pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector29pad"/>
     <p layer="copper1" svgId="connector29pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector31" type="pad" name="AIN4(1.8V)">
   <description>AIN4(1.8V)</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector31pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector31terminal" svgId="connector31pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector31pad"/>
     <p layer="copper1" svgId="connector31pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector75" type="pad" name="AIN5/GPIO86">
   <description>AIN5/GPIO86</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector75pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector75terminal" svgId="connector75pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector75pad"/>
     <p layer="copper1" svgId="connector75pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector6" type="pad" name="AIN6/GPIO87">
   <description>AIN6/GPIO87</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector6terminal" svgId="connector6pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector6pad"/>
     <p layer="copper1" svgId="connector6pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector76" type="pad" name="AIN7(1.8V)">
   <description>AIN7(1.8V)</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector76pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector76terminal" svgId="connector76pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector76pad"/>
     <p layer="copper1" svgId="connector76pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector56" type="pad" name="BAT.TEMP">
   <description>BAT.TEMP</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector56pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector56terminal" svgId="connector56pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector56pad"/>
     <p layer="copper1" svgId="connector56pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector24" type="pad" name="GPIO20">
   <description>GPIO20</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector24terminal" svgId="connector24pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector24pad"/>
     <p layer="copper1" svgId="connector24pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector43" type="pad" name="GPIO23">
   <description>GPIO23</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector43pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector43terminal" svgId="connector43pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector43pad"/>
     <p layer="copper1" svgId="connector43pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector38" type="pad" name="GPIO26">
   <description>GPIO26</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector38pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector38terminal" svgId="connector38pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector38pad"/>
     <p layer="copper1" svgId="connector38pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector59" type="pad" name="GPIO27">
   <description>GPIO27</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector59pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector59terminal" svgId="connector59pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector59pad"/>
     <p layer="copper1" svgId="connector59pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector73" type="pad" name="GPIO45">
   <description>GPIO45</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector73pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector73terminal" svgId="connector73pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector73pad"/>
     <p layer="copper1" svgId="connector73pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector62" type="pad" name="GPIO46">
   <description>GPIO46</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector62pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector62terminal" svgId="connector62pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector62pad"/>
     <p layer="copper1" svgId="connector62pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector58" type="pad" name="GPIO47">
   <description>GPIO47</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector58pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector58terminal" svgId="connector58pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector58pad"/>
     <p layer="copper1" svgId="connector58pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector64" type="pad" name="GPIO48">
   <description>GPIO48</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector64pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector64terminal" svgId="connector64pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector64pad"/>
     <p layer="copper1" svgId="connector64pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector50" type="pad" name="GPIO52">
   <description>GPIO52</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector50pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector50terminal" svgId="connector50pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector50pad"/>
     <p layer="copper1" svgId="connector50pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector46" type="pad" name="GPIO57">
   <description>GPIO57</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector46pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector46terminal" svgId="connector46pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector46pad"/>
     <p layer="copper1" svgId="connector46pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector44" type="pad" name="GPIO58">
   <description>GPIO58</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector44pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector44terminal" svgId="connector44pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector44pad"/>
     <p layer="copper1" svgId="connector44pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector42" type="pad" name="GPIO59">
   <description>GPIO59</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector42pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector42terminal" svgId="connector42pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector42pad"/>
     <p layer="copper1" svgId="connector42pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector48" type="pad" name="GPIO60">
   <description>GPIO60</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector48pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector48terminal" svgId="connector48pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector48pad"/>
     <p layer="copper1" svgId="connector48pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector60" type="pad" name="GPIO64">
   <description>GPIO64</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector60pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector60terminal" svgId="connector60pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector60pad"/>
     <p layer="copper1" svgId="connector60pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector57" type="pad" name="GPIO65">
   <description>GPIO65</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector57pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector57terminal" svgId="connector57pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector57pad"/>
     <p layer="copper1" svgId="connector57pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector8" type="pad" name="GPIO89">
   <description>GPIO89</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector8terminal" svgId="connector8pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector8pad"/>
     <p layer="copper1" svgId="connector8pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector11" type="pad" name="USB1.VIN">
   <description>USB1.VIN</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector11terminal" svgId="connector11pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector11pad"/>
     <p layer="copper1" svgId="connector11pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector9" type="pad" name="USB1.VBUS">
   <description>USB1.VBUS</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector9terminal" svgId="connector9pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector9pad"/>
     <p layer="copper1" svgId="connector9pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector17" type="pad" name="USB1.ID">
   <description>USB1.ID</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector17terminal" svgId="connector17pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector17pad"/>
     <p layer="copper1" svgId="connector17pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector7" type="pad" name="USB1.DRVVBUS">
   <description>USB1.DRVVBUS</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector7terminal" svgId="connector7pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector7pad"/>
     <p layer="copper1" svgId="connector7pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector15" type="pad" name="USB1.DP">
   <description>USB1.DP</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector15terminal" svgId="connector15pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector15pad"/>
     <p layer="copper1" svgId="connector15pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector13" type="pad" name="USB1.DN">
   <description>USB1.DN</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector13terminal" svgId="connector13pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector13pad"/>
     <p layer="copper1" svgId="connector13pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector47" type="pad" name="UART4.TX">
   <description>UART4.TX</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector47pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector47terminal" svgId="connector47pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector47pad"/>
     <p layer="copper1" svgId="connector47pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector45" type="pad" name="UART4.RX">
   <description>UART4.RX</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector45pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector45terminal" svgId="connector45pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector45pad"/>
     <p layer="copper1" svgId="connector45pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector34" type="pad" name="UART0.TX">
   <description>UART0.TX</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector34terminal" svgId="connector34pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector34pad"/>
     <p layer="copper1" svgId="connector34pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector36" type="pad" name="UART0.RX">
   <description>UART0.RX</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector36pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector36terminal" svgId="connector36pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector36pad"/>
     <p layer="copper1" svgId="connector36pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector65" type="pad" name="SPI1.MOSI">
   <description>SPI1.MOSI</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector65pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector65terminal" svgId="connector65pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector65pad"/>
     <p layer="copper1" svgId="connector65pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector67" type="pad" name="SPI1.MISO">
   <description>SPI1.MISO</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector67pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector67terminal" svgId="connector67pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector67pad"/>
     <p layer="copper1" svgId="connector67pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector71" type="pad" name="SPI1.CS">
   <description>SPI1.CS</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector71pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector71terminal" svgId="connector71pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector71pad"/>
     <p layer="copper1" svgId="connector71pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector69" type="pad" name="SPI1.CLK">
   <description>SPI1.CLK</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector69pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector69terminal" svgId="connector69pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector69pad"/>
     <p layer="copper1" svgId="connector69pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector16" type="pad" name="SPI0.MOSI">
   <description>SPI0.MOSI</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector16terminal" svgId="connector16pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector16pad"/>
     <p layer="copper1" svgId="connector16pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector14" type="pad" name="SPI0.MISO">
   <description>SPI0.MISO</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector14terminal" svgId="connector14pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector14pad"/>
     <p layer="copper1" svgId="connector14pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector10" type="pad" name="SPI0.CS">
   <description>SPI0.CS</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector10terminal" svgId="connector10pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector10pad"/>
     <p layer="copper1" svgId="connector10pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector12" type="pad" name="SPI0.CLK">
   <description>SPI0.CLK</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector12terminal" svgId="connector12pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector12pad"/>
     <p layer="copper1" svgId="connector12pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector66" type="pad" name="RESET#">
   <description>RESET#</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector66pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector66terminal" svgId="connector66pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector66pad"/>
     <p layer="copper1" svgId="connector66pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector41" type="pad" name="PWM1A">
   <description>PWM1A</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector41pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector41terminal" svgId="connector41pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector41pad"/>
     <p layer="copper1" svgId="connector41pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector40" type="pad" name="PWM0A">
   <description>PWM0A</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector40pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector40terminal" svgId="connector40pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector40pad"/>
     <p layer="copper1" svgId="connector40pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector39" type="pad" name="PRU1.10">
   <description>PRU1.10</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector39pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector39terminal" svgId="connector39pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector39pad"/>
     <p layer="copper1" svgId="connector39pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector33" type="pad" name="PRU0.7">
   <description>PRU0.7</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector33pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector33terminal" svgId="connector33pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector33pad"/>
     <p layer="copper1" svgId="connector33pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector68" type="pad" name="PRU0.6">
   <description>PRU0.6</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector68pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector68terminal" svgId="connector68pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector68pad"/>
     <p layer="copper1" svgId="connector68pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector74" type="pad" name="PRU0.5">
   <description>PRU0.5</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector74pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector74terminal" svgId="connector74pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector74pad"/>
     <p layer="copper1" svgId="connector74pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector35" type="pad" name="PRU0.4">
   <description>PRU0.4</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector35terminal" svgId="connector35pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector35pad"/>
     <p layer="copper1" svgId="connector35pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector70" type="pad" name="PRU0.3">
   <description>PRU0.3</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector70pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector70terminal" svgId="connector70pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector70pad"/>
     <p layer="copper1" svgId="connector70pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector72" type="pad" name="PRU0.2">
   <description>PRU0.2</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector72pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector72terminal" svgId="connector72pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector72pad"/>
     <p layer="copper1" svgId="connector72pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector37" type="pad" name="PRU0.1">
   <description>PRU0.1</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector37pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector37terminal" svgId="connector37pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector37pad"/>
     <p layer="copper1" svgId="connector37pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector32" type="pad" name="I2C2.SCL">
   <description>I2C2.SCL</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector32pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector32terminal" svgId="connector32pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector32pad"/>
     <p layer="copper1" svgId="connector32pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector30" type="pad" name="I2C2.SDA">
   <description>I2C2.SDA</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector30pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector30terminal" svgId="connector30pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector30pad"/>
     <p layer="copper1" svgId="connector30pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector49" type="pad" name="I2C1.SCL">
   <description>I2C1.SCL</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector49pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector49terminal" svgId="connector49pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector49pad"/>
     <p layer="copper1" svgId="connector49pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector51" type="pad" name="I2C1.SDA">
   <description>I2C1.SDA</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector51pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector51terminal" svgId="connector51pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector51pad"/>
     <p layer="copper1" svgId="connector51pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector19" type="pad" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector19terminal" svgId="connector19pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector19pad"/>
     <p layer="copper1" svgId="connector19pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector20" type="pad" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector20terminal" svgId="connector20pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector20pad"/>
     <p layer="copper1" svgId="connector20pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector26" type="pad" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector26terminal" svgId="connector26pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector26pad"/>
     <p layer="copper1" svgId="connector26pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector55" type="pad" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector55pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector55terminal" svgId="connector55pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector55pad"/>
     <p layer="copper1" svgId="connector55pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector61" type="pad" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector61pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector61terminal" svgId="connector61pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector61pad"/>
     <p layer="copper1" svgId="connector61pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector90" type="pad" name="BAT.VIN">
   <description>BAT.VIN</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector90pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector90pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector90pin"/>
     <p layer="copper1" svgId="connector90pin"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
  <bus id="gnd">
   <nodeMember connectorId="connector19"/>
   <nodeMember connectorId="connector20"/>
   <nodeMember connectorId="connector26"/>
   <nodeMember connectorId="connector55"/>
   <nodeMember connectorId="connector61"/>
  </bus>
  <bus id="vout">
   <nodeMember connectorId="connector28"/>
   <nodeMember connectorId="connector53"/>
  </bus>
  <bus id="3.3v">
   <nodeMember connectorId="connector18"/>
   <nodeMember connectorId="connector63"/>
  </bus>
 </buses>
</module>
