<?xml version='1.0' encoding='UTF-8' standalone='no'?>
<module referenceFile="STM32F103C8T6 blue mini board.fzp" fritzingVersion="0.9.3b" moduleId="STM32F103C8T6_blue_mini_db4c63b0e434949d3cc651e6f45c9298_3">
  <version>4</version>
  <author>Jungho Park (modified by vanepp jan 2019)</author>
  <title>STM32F103C8T6 blue mini board</title>
  <label>M</label>
  <date>Fri Jun 8 2018</date>
  <tags>
    <tag>Blue Pill</tag>
    <tag>STM32F103C8T6</tag>
    <tag>STM32</tag>
    <tag>Microprocessor board</tag>
    <tag>Arduino</tag>
  </tags>
  <properties>
    <property name="family">microcontroller board (blue pill)</property>
    <property name="variant">variant 2</property>
    <property name="editable pin labels">false</property>
    <property name="part number"/>
    <property name="layer"/>
  </properties>
  <description>Generic Blue Pill microcomputer module, available from Ebay and others. CPU STM32F103C8 72Mhz Flash: 64 KB/128 KB RAM: 20KB. 
</description>
  <views>
    <iconView>
      <layers image="icon/STM32F103C8T6_blue_mini_2.svg">
        <layer layerId="icon"/>
      </layers>
    </iconView>
    <breadboardView>
      <layers image="breadboard/STM32F103C8T6_blue_mini_2.svg">
        <layer layerId="breadboard"/>
      </layers>
    </breadboardView>
    <schematicView>
      <layers image="schematic/STM32F103C8T6_blue_mini_2.svg">
        <layer layerId="schematic"/>
      </layers>
    </schematicView>
    <pcbView>
      <layers image="pcb/STM32F103C8T6_blue_mini_2.svg">
        <layer layerId="copper0"/>
        <layer layerId="copper1"/>
        <layer layerId="silkscreen"/>
      </layers>
    </pcbView>
  </views>
  <connectors>
    <connector name="B12" type="male" id="connector0">
      <description>5V ck3 T1BKIN NSS2 SMBA12 PB12 25</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector0pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector0terminal" layer="schematic" svgId="connector0pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector0pin"/>
          <p layer="copper1" svgId="connector0pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B13" type="male" id="connector1">
      <description>5V CTS3 T1CIN SCK2 PB13 26</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector1pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector1terminal" layer="schematic" svgId="connector1pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector1pin"/>
          <p layer="copper1" svgId="connector1pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B14" type="male" id="connector2">
      <description>5V RTS3 T1C2N MISO2 PB14 14</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector2pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector2terminal" layer="schematic" svgId="connector2pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector2pin"/>
          <p layer="copper1" svgId="connector2pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B15" type="male" id="connector3">
      <description>5V T1C3N MOSI2 PB15 28</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector3pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector3terminal" layer="schematic" svgId="connector3pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector3pin"/>
          <p layer="copper1" svgId="connector3pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A8" type="male" id="connector4">
      <description>5V PWM MCO T1C1 CK1 PA8 29</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector4pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector4terminal" layer="schematic" svgId="connector4pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector4pin"/>
          <p layer="copper1" svgId="connector4pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A9" type="male" id="connector5">
      <description>5V PWM T1C2 TX1 PA9 30</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector5pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector5terminal" layer="schematic" svgId="connector5pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector5pin"/>
          <p layer="copper1" svgId="connector5pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A10" type="male" id="connector6">
      <description>5V PWM T1C3 RX1 PA10 31</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector6pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector6terminal" layer="schematic" svgId="connector6pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector6pin"/>
          <p layer="copper1" svgId="connector6pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A11" type="male" id="connector7">
      <description>5V PWM CANRX T1C4 CTS1 USB- PA11 32</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector7pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector7terminal" layer="schematic" svgId="connector7pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector7pin"/>
          <p layer="copper1" svgId="connector7pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A12" type="male" id="connector8">
      <description>5V CANTX T1ETR RTS1 USB+ PA12 33 </description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector8pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector8terminal" layer="schematic" svgId="connector8pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector8pin"/>
          <p layer="copper1" svgId="connector8pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A15" type="male" id="connector9">
      <description>5V T2C1E NSS1 JTDI PA15 38</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector9pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector9terminal" layer="schematic" svgId="connector9pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector9pin"/>
          <p layer="copper1" svgId="connector9pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B3" type="male" id="connector10">
      <description>5V TRACE T2C2 SCKI JTDO PB3 39</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector10pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector10terminal" layer="schematic" svgId="connector10pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector10pin"/>
          <p layer="copper1" svgId="connector10pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B4" type="male" id="connector11">
      <description>5V SWO T3C1 MISO1 JTRST PB4 40</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector11pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector11terminal" layer="schematic" svgId="connector11pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector11pin"/>
          <p layer="copper1" svgId="connector11pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B5" type="male" id="connector12">
      <description>3.3V T2C2 MOSI1 SMBAI1 PB5 41</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector12pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector12terminal" layer="schematic" svgId="connector12pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector12pin"/>
          <p layer="copper1" svgId="connector12pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B6" type="male" id="connector13">
      <description>5V PWM TX1 T4C1 SCL1 PB6 42</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector13pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector13terminal" layer="schematic" svgId="connector13pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector13pin"/>
          <p layer="copper1" svgId="connector13pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B7" type="male" id="connector14">
      <description>5V PWM RX1 T4C2 SDA1 PB7 43</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector14pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector14terminal" layer="schematic" svgId="connector14pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector14pin"/>
          <p layer="copper1" svgId="connector14pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B8" type="male" id="connector15">
      <description>5V PWM CANRX SCL1 T4C3 PB8 45</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector15pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector15terminal" layer="schematic" svgId="connector15pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector15pin"/>
          <p layer="copper1" svgId="connector15pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B9" type="male" id="connector16">
      <description>5V PWM CANTX SDA1 T4c4 PB9 46</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector16pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector16terminal" layer="schematic" svgId="connector16pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector16pin"/>
          <p layer="copper1" svgId="connector16pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="5V" type="male" id="connector17">
      <description>5V Power Connection</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector17pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector17terminal" layer="schematic" svgId="connector17pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector17pin"/>
          <p layer="copper1" svgId="connector17pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="G" type="male" id="connector18">
      <description>GND Ground</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector18pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector18terminal" layer="schematic" svgId="connector18pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector18pin"/>
          <p layer="copper1" svgId="connector18pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="3.3V" type="male" id="connector19">
      <description>3.3V Power Connection</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector19pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector19terminal" layer="schematic" svgId="connector19pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector19pin"/>
          <p layer="copper1" svgId="connector19pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="VBAT" type="male" id="connector20">
      <description>3.3V VBAT</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector20pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector20terminal" layer="schematic" svgId="connector20pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector20pin"/>
          <p layer="copper1" svgId="connector20pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="C13" type="male" id="connector21">
      <description>3.3V Sink 3ma source 0ma PC13_LED TAMPER_RTC PC13 2</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector21pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector21terminal" layer="schematic" svgId="connector21pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector21pin"/>
          <p layer="copper1" svgId="connector21pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="C14" type="male" id="connector22">
      <description>3.3V Sink 3ma source 0ma OSC32_IN PC14 3</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector22pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector22terminal" layer="schematic" svgId="connector22pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector22pin"/>
          <p layer="copper1" svgId="connector22pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="C15" type="male" id="connector23">
      <description>3.3V Sink 3ma source 0ma OSC32_OUT PC15 4</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector23pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector23terminal" layer="schematic" svgId="connector23pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector23pin"/>
          <p layer="copper1" svgId="connector23pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A0" type="male" id="connector24">
      <description>3.3V PWM WKUP T2C1E CTS2 ADC0 PA0 10</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector24pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector24terminal" layer="schematic" svgId="connector24pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector24pin"/>
          <p layer="copper1" svgId="connector24pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A1" type="male" id="connector25">
      <description>3.3V PWM T2C2 RTS2 ADC1 PA1 11</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector25pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector25terminal" layer="schematic" svgId="connector25pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector25pin"/>
          <p layer="copper1" svgId="connector25pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A2" type="male" id="connector26">
      <description>3.3V PWM T2C3 TX2 ADC2 PA2 12</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector26pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector26terminal" layer="schematic" svgId="connector26pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector26pin"/>
          <p layer="copper1" svgId="connector26pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A3" type="male" id="connector27">
      <description>3.3V PWM T2C4 RX2 ADC3 PA3 13</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector27pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector27terminal" layer="schematic" svgId="connector27pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector27pin"/>
          <p layer="copper1" svgId="connector27pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A4" type="male" id="connector28">
      <description>3.3V CK2 NSS1 ADC4 PA4 14</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector28pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector28terminal" layer="schematic" svgId="connector28pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector28pin"/>
          <p layer="copper1" svgId="connector28pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A5" type="male" id="connector29">
      <description>3.3V SCK1 ADC5 PA5 15</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector29pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector29terminal" layer="schematic" svgId="connector29pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector29pin"/>
          <p layer="copper1" svgId="connector29pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A6" type="male" id="connector30">
      <description>3.3V PWM T1BKIN T3C1 MISO1 ADC6 PA6 16</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector30pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector30terminal" layer="schematic" svgId="connector30pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector30pin"/>
          <p layer="copper1" svgId="connector30pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="A7" type="male" id="connector31">
      <description>3.3V PWM T1C1N T3C3 MOSI1 ADC7 PA7 17</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector31pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector31terminal" layer="schematic" svgId="connector31pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector31pin"/>
          <p layer="copper1" svgId="connector31pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B0" type="male" id="connector32">
      <description>3.3V PWM T1C2N T3C3 ADC8 PB0</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector32pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector32terminal" layer="schematic" svgId="connector32pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector32pin"/>
          <p layer="copper1" svgId="connector32pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B1" type="male" id="connector33">
      <description>3.3V PWM T1C3N T3C4 ADC9 PB1 19</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector33pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector33terminal" layer="schematic" svgId="connector33pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector33pin"/>
          <p layer="copper1" svgId="connector33pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B10" type="male" id="connector34">
      <description>5V T2C3N TX3 SCL2 PB10 21</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector34pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector34terminal" layer="schematic" svgId="connector34pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector34pin"/>
          <p layer="copper1" svgId="connector34pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="B11" type="male" id="connector35">
      <description>5V T2CAN RX3 SDA2 PB11 22</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector35pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector35terminal" layer="schematic" svgId="connector35pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector35pin"/>
          <p layer="copper1" svgId="connector35pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="RST" type="male" id="connector36">
      <description>3.3V RESET_BUTTON NRST 7</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector36pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector36terminal" layer="schematic" svgId="connector36pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector36pin"/>
          <p layer="copper1" svgId="connector36pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="3.3V" type="male" id="connector37">
      <description>3.3V Power connection</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector37pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector37terminal" layer="schematic" svgId="connector37pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector37pin"/>
          <p layer="copper1" svgId="connector37pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="G" type="male" id="connector38">
      <description>GND Ground Connection</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector38pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector38terminal" layer="schematic" svgId="connector38pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector38pin"/>
          <p layer="copper1" svgId="connector38pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="G" type="male" id="connector39">
      <description>GND Ground Connection</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector39pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector39terminal" layer="schematic" svgId="connector39pin"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector39pin"/>
          <p layer="copper1" svgId="connector39pin"/>
        </pcbView>
      </views>
    </connector>
    <connector name="3.3" type="female" id="connector40">
      <description>3.3V Jtag connector</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector40pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector40terminal" layer="schematic" svgId="connector40pin"/>
        </schematicView>
        <pcbView>
    </pcbView>
      </views>
    </connector>
    <connector name="DIO" type="female" id="connector41">
      <description>5V SWDIO JTMS PA13 34 jtag connector</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector41pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector41terminal" layer="schematic" svgId="connector41pin"/>
        </schematicView>
        <pcbView>
    </pcbView>
      </views>
    </connector>
    <connector name="CLK" type="female" id="connector42">
      <description>5V SWCLK JTCLK PA14 37 Jtag Connector</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector42pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector42terminal" layer="schematic" svgId="connector42pin"/>
        </schematicView>
        <pcbView>
    </pcbView>
      </views>
    </connector>
    <connector name="GND" type="female" id="connector43">
      <description>Ground Jtag Connector</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector43pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector43terminal" layer="schematic" svgId="connector43pin"/>
        </schematicView>
        <pcbView>
    </pcbView>
      </views>
    </connector>
    <connector name="GND" type="female" id="connector44">
      <description>Ground Boot1 connector</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector44pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector44terminal" layer="schematic" svgId="connector44pin"/>
        </schematicView>
        <pcbView>
    </pcbView>
      </views>
    </connector>
    <connector name="" type="female" id="connector45">
      <description>5V Boot1 PB2 20</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector45pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector45terminal" layer="schematic" svgId="connector45pin"/>
        </schematicView>
        <pcbView>
    </pcbView>
      </views>
    </connector>
    <connector name="3.3V" type="female" id="connector46">
      <description>3.3V  Power Connection Boot1 Connector</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector46pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector46terminal" layer="schematic" svgId="connector46pin"/>
        </schematicView>
        <pcbView>
    </pcbView>
      </views>
    </connector>
    <connector name="GND" type="female" id="connector47">
      <description>Ground Boot0 Connector</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector47pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector47terminal" layer="schematic" svgId="connector47pin"/>
        </schematicView>
        <pcbView>
    </pcbView>
      </views>
    </connector>
    <connector name="Boot0" type="female" id="connector48">
      <description>3.3V Boot0 44</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector48pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector48terminal" layer="schematic" svgId="connector48pin"/>
        </schematicView>
        <pcbView>
    </pcbView>
      </views>
    </connector>
    <connector name="3.3V" type="female" id="connector49">
      <description>3.3V Power Connection Boot0 Connector</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector49pin"/>
        </breadboardView>
        <schematicView>
          <p terminalId="connector49terminal" layer="schematic" svgId="connector49pin"/>
        </schematicView>
        <pcbView>
    </pcbView>
      </views>
    </connector>
  </connectors>
  <buses>
    <bus id="GND">
      <nodeMember connectorId="connector18"/>
      <nodeMember connectorId="connector38"/>
      <nodeMember connectorId="connector39"/>
      <nodeMember connectorId="connector43"/>
      <nodeMember connectorId="connector44"/>
      <nodeMember connectorId="connector47"/>
    </bus>
    <bus id="3.3V">
      <nodeMember connectorId="connector19"/>
      <nodeMember connectorId="connector37"/>
      <nodeMember connectorId="connector40"/>
      <nodeMember connectorId="connector46"/>
      <nodeMember connectorId="connector49"/>
    </bus>
  </buses>
  <url>https://wiki.stm32duino.com/index.php?title=Blue_Pill</url>
</module>
