<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.9.2b" moduleId="Sparkfun_TiltaWhirl">
 <version>5</version>
 <date>Dec 1 2015</date>
 <author>SparkFun and Fritzing toolkit</author>
 <description></description>
 <title>SparkFun RPI-1031 Tilt-a-Whirl Breakout</title>
 <url>https://www.sparkfun.com/products/10621</url>
 <tags>
  <tag>Breakout Board</tag>
  <tag>tilt sensor</tag>
  <tag>RPI-1031</tag>
  <tag>sensor</tag>
  <tag>SparkFun</tag>
 </tags>
 <properties>
  <property name="family">SparkFun Breakout Boards</property>
  <property name="variant"></property>
  <property name="layer"></property>
  <property name="part number">SEN-10621</property>
 </properties>
 <views>
  <breadboardView>
   <layers image="breadboard/Sparkfun_Tilt-a-Whirl_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/Sparkfun_Tilt-a-Whirl_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/Sparkfun_Tilt-a-Whirl_pcb.svg">
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/Sparkfun_Tilt-a-Whirl_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector type="male" id="connector6" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pad" layer="copper0"/>
     <p svgId="connector6pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector7" name="VCC">
   <description>VCC</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pad" layer="copper0"/>
     <p svgId="connector7pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector8" name="S1">
   <description>SDA</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pad" layer="copper0"/>
     <p svgId="connector8pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector9" name="S2">
   <description>S2</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pad" layer="copper0"/>
     <p svgId="connector9pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses/>
</module>
