<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.5.4b.05.18.4914" moduleId="CathodeLEDRGBSuperfluxModuleID">
    <version>4</version>
    <author>stefanhermann</author>
    <title>Super Flux RGB LED (com. cathode)</title>
    <label>LED</label>
    <date>2011-09-21</date>
    <tags>
				<tag>rgb</tag>
				<tag>led</tag>
        <tag>super flux</tag>
        <tag>full color</tag>
        <tag>indicator</tag>
    </tags>
    <properties>
        <property name="family">SuperFlux LED</property>
        <property name="type">RGB</property>
        <property name="polarity">common cathode</property>
    </properties>
    <description>A full color SuperFlux LED.</description>
    <views>
        <iconView>
            <layers image="icon/LED-SuperFlux-rgb.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/led-superFlux-rgb.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/led-rbg-flux-4pin-cathode.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/led-superFlux.svg">
                <layer layerId="copper0"/>
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" type="male" name="red anode">
            <description>anode pin for red LED</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin"  terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pad"/>
                    <p layer="copper0" svgId="connector0pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" type="male" name="common cathode">
            <description>cathode pin for every color, supply +voltage</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pad"/>
                    <p layer="copper0" svgId="connector3pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="blue anode">
            <description>anode pin for blue LED</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"  terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pad"/>
                    <p layer="copper0" svgId="connector1pad"/>
                </pcbView>
            </views>
        </connector>
         <connector id="connector2" type="male" name="green anode">
            <description>anode pin for green LED</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"  terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pad"/>
                    <p layer="copper0" svgId="connector2pad"/>
                </pcbView>
            </views>
        </connector>
   </connectors>
</module>
