<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Sensors-LIS3LV02DQ-SMD">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Sensors' LIS3LV02DQ SMD -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>3-axis 2/6g I2C/SPI accelerometer</description>
<title>LIS3LV02DQ</title>
<tags>
<tag>SMD</tag>
<tag>QFN-28</tag>
<tag>LIS3LV02DQ</tag>
</tags>
<properties>
<property name="package">qfn-28</property>
<property name="family">sparkfun Accelerometer</property>
<property name="interface">I2C/SPI</property>
<property name="variant">smd</property>
<property name="axis">3</property>
<property name="sensitivity">2/6g</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/QFN-28_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-sensors_lis3lv02dq_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-sensors_qfn-28_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/QFN-28_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector16" name="CK" type="male">
<description>CK</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector16pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector16pad"/>
</pcbView>
</views>
</connector>
<connector id="connector13" name="CS" type="male">
<description>CS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector13pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector13pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector17" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector17pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector17pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="INT" type="male">
<description>INT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector12" name="SCL_SPC" type="male">
<description>SCL_SPC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector12pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector12pad"/>
</pcbView>
</views>
</connector>
<connector id="connector10" name="SDA_SDI" type="male">
<description>SDA_SDI</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector10pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector10pad"/>
</pcbView>
</views>
</connector>
<connector id="connector9" name="SDO" type="male">
<description>SDO</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector19" name="VDD" type="male">
<description>VDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector19pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector19pad"/>
</pcbView>
</views>
</connector>
<connector id="connector20" name="VDD" type="male">
<description>VDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector20pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector20pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="VDD" type="male">
<description>VDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector11" name="VDD_IO" type="male">
<description>VDD_IO</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector11pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector11pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id="VDD">
<nodeMember connectorId="connector3"/>
<nodeMember connectorId="connector20"/>
<nodeMember connectorId="connector19"/>
</bus>
<bus id="GND">
<nodeMember connectorId="connector5"/>
<nodeMember connectorId="connector2"/>
<nodeMember connectorId="connector17"/>
<nodeMember connectorId="connector0"/>
</bus>
</buses>
</module>