<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="ds1809_ic_dip" referenceFile="generic_ic_dip_8_300mil.fzp" fritzingVersion="0.12.34">
 <version>4</version>
 <author>Fritzing Part-o-matic</author>
 <title>DS1809</title>
 <label>DS1809</label>
 <date>So Jan 15 2017</date>
 <tags>
  <tag>DIP</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="family">DS1806</property>
  <property name="package">DS1806</property>
  <property name="part number">DS1809</property>
  <property name="variant">variant 1</property>
 </properties>
 <description>The DS1809 Dallastat is a nonvolatile digitally controlled potentiometer that provides 64 uniform wiper
positions over the entire resistor range; including the high-end and low-end terminals of the device. The
DS1809 is a low-power device capable of operating from power supplies of +4.5V to +5.5V. The device
is ideal for low-power, portable, or battery powered applications.</description>
 <views>
  <iconView>
   <layers image="icon/ds2809_ic_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/ds2809_ic_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/ds2809_ic_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/ds2809_ic_pcb.svg">
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" type="male" name="RH">
   <description>pin 1</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" terminalId="connector0terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" terminalId="connector0terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" type="male" name="UC">
   <description>pin 2</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" terminalId="connector1terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" terminalId="connector1terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" type="male" name="STR">
   <description>pin 3</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" terminalId="connector2terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" terminalId="connector2terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector3" type="male" name="RL">
   <description>pin 4</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" terminalId="connector3terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" terminalId="connector3terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper0"/>
     <p svgId="connector3pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector4" type="male" name="GND">
   <description>pin 5</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" terminalId="connector4terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" terminalId="connector4terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper0"/>
     <p svgId="connector4pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector5" type="male" name="RW">
   <description>pin 6</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" terminalId="connector5terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" terminalId="connector5terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper0"/>
     <p svgId="connector5pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector6" type="male" name="DC">
   <description>pin 7</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" terminalId="connector6terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" terminalId="connector6terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper0"/>
     <p svgId="connector6pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector7" type="male" name="VCC">
   <description>pin 8</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" terminalId="connector7terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" terminalId="connector7terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper0"/>
     <p svgId="connector7pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>
