<?xml version='1.0' encoding='UTF-8' standalone='no'?>
<module fritzingVersion="0.1.1255" moduleId="1238DBDC00-voltage-reg_lm317">
  <version>5</version>
  <author>Jenny</author>
  <title>Voltage Regulator - Variable</title>
  <label>U</label>
  <date>2018-4-24</date>
  <tags>
    <tag>regulator</tag>
    <tag>lm317</tag>
    <tag>power</tag>
    <tag>fritzing core</tag>
  </tags>
  <properties>
    <property name="package">TO220 [THT]</property>
    <property name="voltage">Variable V</property>
    <property name="family">Voltage Regulator</property>
  </properties>
  <description>Variable DC Voltage Regulator</description>
  <views>
    <iconView>
      <layers image="icon/voltage_regulator_vreg_icon.svg">
        <layer layerId="icon"/>
      </layers>
    </iconView>
    <breadboardView>
      <layers image="breadboard/voltage_regulator_vreg.svg">
        <layer layerId="breadboard"/>
      </layers>
    </breadboardView>
    <schematicView>
      <layers image="schematic/voltage_regulator_LM317.svg">
        <layer layerId="schematic"/>
      </layers>
    </schematicView>
    <pcbView>
      <layers image="pcb/TO-220.svg">
        <layer layerId="copper0"/>
        <layer layerId="silkscreen"/>
        <layer layerId="copper1"/>
      </layers>
    </pcbView>
  </views>
  <connectors>
    <connector id="connector0" name="ADJ" type="male">
      <description>Adjust</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector0pin" legId="connector0leg"/>
        </breadboardView>0
    <schematicView>
          <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector0pad"/>
          <p layer="copper1" svgId="connector0pad"/>
        </pcbView>
      </views>
    </connector>
    <connector id="connector1" name="OUT" type="male">
      <description>Output</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector1pin" legId="connector1leg"/>
        </breadboardView>
        <schematicView>
          <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector1pad"/>
          <p layer="copper1" svgId="connector1pad"/>
        </pcbView>
      </views>
    </connector>
    <connector id="connector2" name="IN" type="male">
      <description>Input Voltage</description>
      <views>
        <breadboardView>
          <p layer="breadboard" svgId="connector2pin" legId="connector2leg"/>
        </breadboardView>
        <schematicView>
          <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
        </schematicView>
        <pcbView>
          <p layer="copper0" svgId="connector2pad"/>
          <p layer="copper1" svgId="connector2pad"/>
        </pcbView>
      </views>
    </connector>
  </connectors>
</module>
