<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='ArduinoBluetoothMatev13'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;b&gt;Description: &lt;/b&gt;The Bluetooth Mate is very similar to our BlueSMiRF modem, but it is designed specifically to be used with our &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9219&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;Arduino Pros&lt;/a&gt; and &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9266&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;LilyPad Arduinos&lt;/a&gt;. These modems work as a serial (RX/TX) pipe, and are a great wireless replacement for serial cables. Any serial stream from 9600 to 115200bps can be passed seamlessly from your computer to your target.&lt;/p&gt;


&lt;p&gt;


	Bluetooth Mate has the same pin out as the FTDI Basic, and is meant to plug directly into an Arduino Pro, Pro Mini, or LilyPad Mainboard. Because we&amp;#39;ve arranged the pins to do this, you cannot directly plug the Bluetooth Mate to an FTDI Basic board (you&amp;#39;ll have to swap TX and RX).&lt;/p&gt;


&lt;p&gt;


	The RN-42 is perfect for short range, battery powered applications.&amp;nbsp; The RN-42 uses only 26uA in sleep mode while still being discoverable and connectable.&amp;nbsp; Multiple user configurable power modes allow the user to dial in the lowest power profile for a given application. If you need longer range, check out the Bluetooth Mate Gold.&lt;/p&gt;


&lt;p&gt;


	The Bluetooth Mate has on-board voltage regulators, so it can be powered from any 3.3 to 6VDC power supply. We&amp;#39;ve got level shifting all set up so the RX and TX pins on the remote unit are 3-6VDC tolerant. &lt;span style=&quot;font-weight: bold;&quot;&gt;Do not&lt;/span&gt; attach this device directly to a serial port. You will need an &lt;a href=&quot;http://www.sparkfun.com/products/449&quot; target=&quot;_blank&quot;&gt;RS232 to TTL converter circuit&lt;/a&gt; if you need to attach this to a computer.&lt;/p&gt;


&lt;p&gt;


	Unit comes without a connector; if you want to connect it to an Arduino Pro, we&amp;#39;d suggest the &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9429&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;6-pin right-angle female header&lt;/a&gt;.&lt;/p&gt;


&lt;p&gt;


	&lt;strong&gt;Note: &lt;/strong&gt;The hardware reset pin of the RN-42 module is broken out on the bottom side of the board. This pin is mislabeled as &amp;#39;PIO6&amp;#39;, it is actually PIO4. Should you need to reset the Mate, pull this pin high upon power-up, and then toggle it 3 times.&lt;/p&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Features&lt;/span&gt;&lt;b&gt;:&lt;/b&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		Designed to work directly with Arduino Pro&amp;#39;s and LilyPad main boards&lt;/li&gt;


	&lt;li&gt;


		FCC Approved Class 2 Bluetooth&lt;sup&gt;&lt;font face=&quot;Tahoma, sans-serif&quot;&gt;&lt;b&gt;&amp;reg; &lt;/b&gt;&lt;/font&gt;&lt;/sup&gt;Radio Modem!&lt;/li&gt;


	&lt;li&gt;


		Low power consumption : 25mA avg&lt;/li&gt;


	&lt;li&gt;


		Hardy frequency hopping scheme - operates in harsh RF environments like WiFi, 802.11g, and Zigbee&lt;/li&gt;


	&lt;li&gt;


		Encrypted connection&lt;/li&gt;


	&lt;li&gt;


		Frequency: 2.4~2.524 GHz&lt;/li&gt;


	&lt;li&gt;


		Operating Voltage: 3.3V-6V&lt;/li&gt;


	&lt;li&gt;


		Serial communications: 2400-115200bps&lt;/li&gt;


	&lt;li&gt;


		Operating Temperature: -40 ~ +70C&lt;/li&gt;


	&lt;li&gt;


		Built-in antenna&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Dimensions: &lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		Board: 1.75x0.65&amp;quot;&lt;br /&gt;


		&lt;span style=&quot;font-weight: bold;&quot;&gt; &lt;/span&gt;&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;b&gt;Documents:&lt;/b&gt; &lt;a href=&quot;http://www.sparkfun.com/datasheets/RF/BlueSMiRF_v1.pdf&quot; target=&quot;_blank&quot;&gt;&lt;br /&gt;


	&lt;/a&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Wireless/Bluetooth/ArduinoBluetoothMatev13.pdf&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/datasheets/Wireless/Bluetooth/ArduinoBluetoothMatev13.zip&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Wireless/Bluetooth/rn-bluetooth-um.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;RN-42 AT Command Set&lt;/a&gt;&lt;a href=&quot;http://www.sparkfun.com/datasheets/RF/RN_BlueportII-ref-guide.pdf&quot; id=&quot;Roving Networks Bluetooth Command Set&quot; name=&quot;Roving Networks Bluetooth Command Set&quot; target=&quot;_blank&quot;&gt;&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.rovingnetworks.com/documents/RN-41.pdf&quot; name=&quot;Roving Networks Bluetooth module datasheet&quot; target=&quot;_blank&quot;&gt;Roving Networks Bluetooth&lt;sup&gt;&lt;font face=&quot;Tahoma, sans-serif&quot;&gt;&lt;b&gt;&amp;reg;&lt;/b&gt;&lt;/font&gt;&lt;/sup&gt; module datasheet&lt;/a&gt;&lt;br /&gt;


		&lt;a href=&quot;http://www.sparkfun.com/datasheets/RF/RN-24-guide.pdf&quot; id=&quot;Roving Networks RN-24 Usage Guide&quot; name=&quot;Roving Networks RN-24 Usage Guide&quot; target=&quot;_blank&quot;&gt;&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/tutorials/67&quot; target=&quot;_blank&quot;&gt;Check out our Bluetooth Tutorial&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;</description>
<title>Bluetooth Mate Silver</title>
<url>http://www.sparkfun.com/products/10393</url>
<tags>
<tag>Bluetooth</tag>
<tag>Mate</tag>
<tag>Wireless</tag>
</tags>
<properties>
<property name='family'>Wireless</property>
<property name='Protocol'>Bluetooth</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/ArduinoBluetoothMatev13_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/ArduinoBluetoothMatev13_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/ArduinoBluetoothMatev13_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/ArduinoBluetoothMatev13_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector12' type='male' name='RTS_5V'>
<description>RTS_5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector12pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector12pin' terminalId='connector12terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector12pad'/><p layer='copper1' svgId='connector12pad'/></pcbView>
</views>
</connector>
<connector id='connector13' type='male' name='RX_5V'>
<description>RX_5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector13pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector13pin' terminalId='connector13terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector13pad'/><p layer='copper1' svgId='connector13pad'/></pcbView>
</views>
</connector>
<connector id='connector14' type='male' name='TX_5V'>
<description>TX_5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector14pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector14pin' terminalId='connector14terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector14pad'/><p layer='copper1' svgId='connector14pad'/></pcbView>
</views>
</connector>
<connector id='connector15' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector15pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector15pin' terminalId='connector15terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector15pad'/><p layer='copper1' svgId='connector15pad'/></pcbView>
</views>
</connector>
<connector id='connector16' type='male' name='CTS_5V'>
<description>CTS_5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector16pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector16pin' terminalId='connector16terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector16pad'/><p layer='copper1' svgId='connector16pad'/></pcbView>
</views>
</connector>
<connector id='connector17' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector17pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector17pin' terminalId='connector17terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector17pad'/><p layer='copper1' svgId='connector17pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
