<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.7.4b.04.10.5970" moduleId="Raspberry Pi" referenceFile="Raspberry_Pi.fzp">
 <version replacedby="Raspberry Pi (rev1)">4</version>
 <author>Fabian Althaus</author>
 <title>Raspberry Pi</title>
 <label>Raspberry Pi</label>
 <date>Mo Apr 15 2013</date>
 <tags>
  <tag>Raspberry</tag>
  <tag>Raspberry Pi</tag>
  <tag>RPi</tag>
 </tags>
 <properties>
  <property name="family">//obsolete//CPU Board (Raspberry Pi)</property>
  <property name="processor">Broadcom SoC BCM2835 ARMv6</property>
  <property name="variant">Raspberry Pi</property>
 </properties>
 <description>The awesome Raspberry Pi ARM Board</description>
 <views>
  <iconView>
   <layers image="icon/Raspberry_Pi_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/raspberry_pi_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/raspberry_pi_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/Raspberry_Pi_pcb.svg">
    <layer layerId="copper0"/>
	
    <layer layerId="copper1"/>
	  <layer layerId="silkscreen"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="male" id="connector15" name="GPIO4">
   <description>GPIO Pin 4</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" layer="schematic" terminalId="connector15terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pin" layer="copper1"/>
     <p svgId="connector15pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector7" name="TXD">
   <description>Serial TXD</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper1"/>
     <p svgId="connector7pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector17" name="GPIO5">
   <description>GPIO Pin 5</description>
   <views>
    <breadboardView>
     <p svgId="connector17pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector17pin" layer="schematic" terminalId="connector17terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector17pin" layer="copper1"/>
     <p svgId="connector17pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector9" name="RXD">
   <description>Serial RXD</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper1"/>
     <p svgId="connector9pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector18" name="SPI_MOSI">
   <description>SPI MOSI (Master Out, Slave In)</description>
   <views>
    <breadboardView>
     <p svgId="connector18pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector18pin" layer="schematic" terminalId="connector18terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector18pin" layer="copper1"/>
     <p svgId="connector18pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector20" name="SPI_MISO">
   <description>SPI MISO (Master In, Slave Out)</description>
   <views>
    <breadboardView>
     <p svgId="connector20pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector20pin" layer="schematic" terminalId="connector20terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector20pin" layer="copper1"/>
     <p svgId="connector20pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector21" name="GPIO6">
   <description>GPIO Pin 6</description>
   <views>
    <breadboardView>
     <p svgId="connector21pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector21pin" layer="schematic" terminalId="connector21terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector21pin" layer="copper1"/>
     <p svgId="connector21pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector22" name="SPI_SCLK">
   <description>SPI SCLK (Serial Clock)</description>
   <views>
    <breadboardView>
     <p svgId="connector22pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector22pin" layer="schematic" terminalId="connector22terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector22pin" layer="copper1"/>
     <p svgId="connector22pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector23" name="SPI_CE0_N">
   <description>SPI CE0 N (Cable Select Line 0)</description>
   <views>
    <breadboardView>
     <p svgId="connector23pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector23pin" layer="schematic" terminalId="connector23terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector23pin" layer="copper1"/>
     <p svgId="connector23pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector25" name="SPI_CE1_N">
   <description>SPI CE1 N (Cable Select Line 1)</description>
   <views>
    <breadboardView>
     <p svgId="connector25pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector25pin" layer="schematic" terminalId="connector25terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector25pin" layer="copper1"/>
     <p svgId="connector25pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector0" name="3V3">
   <description>Output Voltage 3V3</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper1"/>
     <p svgId="connector0pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector1" name="5V">
   <description>Output Voltage 5V</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper1"/>
     <p svgId="connector1pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector10" name="GPIO0">
   <description>GPIO Pin 0</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper1"/>
     <p svgId="connector10pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector2" name="I2C_SDA0">
   <description>I2C SDA 0 (Serial Data)</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper1"/>
     <p svgId="connector2pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector11" name="GPIO1">
   <description>GPIO Pin 1</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper1"/>
     <p svgId="connector11pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector4" name="I2C_SCL_0">
   <description>I2C SCL 0 (Serial Clock)</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper1"/>
     <p svgId="connector4pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector12" name="GPIO2">
   <description>GPIO Pin 2</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper1"/>
     <p svgId="connector12pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector5" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper1"/>
     <p svgId="connector5pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector6" name="GPIO7">
   <description>GPIO Pin 7</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper1"/>
     <p svgId="connector6pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector14" name="GPIO3">
   <description>GPIO Pin 3</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" layer="schematic" terminalId="connector14terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pin" layer="copper1"/>
     <p svgId="connector14pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector26" name="Pin 9 DNC">
   <description>Pin 9 DNC </description>
   <views>
    <breadboardView>
     <p svgId="connector26pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector26pin" layer="schematic" terminalId="connector26terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector26pin" layer="copper1"/>
     <p svgId="connector26pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector27" name="Pin 4 DNC ">
   <description>Pin 4 DNC </description>
   <views>
    <breadboardView>
     <p svgId="connector27pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector27pin" layer="schematic" terminalId="connector27terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector27pin" layer="copper1"/>
     <p svgId="connector27pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector28" name="Pin 14 DNC ">
   <description>Pin 14 DNC </description>
   <views>
    <breadboardView>
     <p svgId="connector28pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector28pin" layer="schematic" terminalId="connector28terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector28pin" layer="copper1"/>
     <p svgId="connector28pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector29" name="Pin 20 DNC ">
   <description>Pin 20 DNC </description>
   <views>
    <breadboardView>
     <p svgId="connector29pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector29pin" layer="schematic" terminalId="connector29terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector29pin" layer="copper1"/>
     <p svgId="connector29pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector30" name="Pin 17 DNC ">
   <description>Pin 17 DNC </description>
   <views>
    <breadboardView>
     <p svgId="connector30pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector30pin" layer="schematic" terminalId="connector30terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector30pin" layer="copper1"/>
     <p svgId="connector30pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector31" name="Pin 25 DNC ">
   <description>Pin 25 DNC </description>
   <views>
    <breadboardView>
     <p svgId="connector31pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector31pin" layer="schematic" terminalId="connector31terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector31pin" layer="copper1"/>
     <p svgId="connector31pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>
