<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.6.3b.08.16.5401" moduleId="4067 HCF">
    <version>4</version>
    <author>Alfonso Abelenda Escudero</author>
    <title>HCF 4067</title>
    <label>HCF 4067</label>
    <date>2001-09-23</date>
    <tags>
			<tag>DIP</tag>
      <tag>TTL</tag>
      <tag>Logic IC</tag>
      <tag>HCF</tag>
      <tag>Multiplexer</tag>
    </tags>
    <properties>
		 		<property name="family">4000 series</property>
        <property name="package">DIP24 [THT]</property>
				<property name="type">HF 4067</property>
        <property name="chip label">HF 4067</property>
        <property name="pins">24</property>
        <property name="spacing">600mil</property>
    </properties>
    <description>Analog multiplexer 16:1</description>
    <views>
        <iconView>
            <layers image="icon/HCF_4067397.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/HCF_4067397.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <pcbView>
            <layers image="pcb/HCF_4067397.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
        <schematicView>
            <layers image="schematic/HCF_406703c.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
    </views>
    <connectors>
        <connector id="connector15" type="male" name="16 TG15">
            <description>TG15</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin" terminalId="connector15terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector15pin"/>
                    <p layer="copper1" svgId="connector15pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" type="male" name="8 TG1">
            <description>TG1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin" terminalId="connector7terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector7pin"/>
                    <p layer="copper1" svgId="connector7pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector16" type="male" name="17 TG14">
            <description>TG14</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector16pin" terminalId="connector16terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector16pin"/>
                    <p layer="copper1" svgId="connector16pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" type="male" name="9 TG0">
            <description>TG0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin" terminalId="connector8terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector8pin"/>
                    <p layer="copper1" svgId="connector8pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector17" type="male" name="18 TG13">
            <description>TG13</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector17pin" terminalId="connector17terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector17pin"/>
                    <p layer="copper1" svgId="connector17pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" type="male" name="10 A">
            <description>Control Pin A</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin" terminalId="connector9terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector9pin"/>
                    <p layer="copper1" svgId="connector9pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector18" type="male" name="19 TG12">
            <description>TG12</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector18pin" terminalId="connector18terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector18pin"/>
                    <p layer="copper1" svgId="connector18pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector19" type="male" name="20 TG11">
            <description>TG11</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector19pin" terminalId="connector19terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector19pin"/>
                    <p layer="copper1" svgId="connector19pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector20" type="male" name="21 TG10">
            <description>TG10</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector20pin" terminalId="connector20terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector20pin"/>
                    <p layer="copper1" svgId="connector20pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector21" type="male" name="22 TG9">
            <description>TG9</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector21pin" terminalId="connector21terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector21pin"/>
                    <p layer="copper1" svgId="connector21pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector22" type="male" name="23 TG8">
            <description>TG8</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector22pin" terminalId="connector22terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector22pin"/>
                    <p layer="copper1" svgId="connector22pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector23" type="male" name="24 Vdd">
            <description>VDD</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector23pin" terminalId="connector23terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector23pin"/>
                    <p layer="copper1" svgId="connector23pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" type="male" name="1 O/I">
            <description>Common out/in</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                    <p layer="copper1" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="2 TG 7">
            <description>TG7</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                    <p layer="copper1" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" type="male" name="11 B">
            <description>Control Pin B</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin" terminalId="connector10terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector10pin"/>
                    <p layer="copper1" svgId="connector10pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="male" name="3 TG6">
            <description>TG6</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                    <p layer="copper1" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" type="male" name="4 TG5">
            <description>TG5</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pin"/>
                    <p layer="copper1" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" type="male" name="12 VSS">
            <description>Vss Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin" terminalId="connector11terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector11pin"/>
                    <p layer="copper1" svgId="connector11pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" type="male" name="5 TG4">
            <description>TG4</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector4pin"/>
                    <p layer="copper1" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector12" type="male" name="13 D">
            <description>Control Pin D</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin" terminalId="connector12terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector12pin"/>
                    <p layer="copper1" svgId="connector12pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" type="male" name="6 TG3">
            <description>TG3</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" terminalId="connector5terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector5pin"/>
                    <p layer="copper1" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector13" type="male" name="14 C">
            <description>Control Pin C</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin" terminalId="connector13terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector13pin"/>
                    <p layer="copper1" svgId="connector13pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" type="male" name="7 TG2">
            <description>TG2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin" terminalId="connector6terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector6pin"/>
                    <p layer="copper1" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector14" type="male" name="15 Inhibit">
            <description>Inhibit</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin" terminalId="connector14terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector14pin"/>
                    <p layer="copper1" svgId="connector14pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
