<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.2.2.b.03.04.2550" moduleId="a22e371d3e8c77a58fdfe4dd2799c449leg">
<version>4</version>
    <author>Peter Boman</author>
    <title>Stepper Motor - Unipolar</title>
    <label>M</label>
    <date>2009-10-23</date>
    <tags>
        <tag>Motor</tag>
        <tag>Stepper Motor</tag>
    </tags>
    <properties>
        <property name="family">Stepper Motor</property>
        <property name="Stepper Type">Unipolar</property>
    </properties>
    <description>A basic unipolar stepper motor</description>
    <views>
        <breadboardView>
            <layers image="breadboard/Stepper_Motor_Unipolar_breadboard_leg.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/Stepper_Motor_-_Unipolar__schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/jumper_6_100mil_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
            <layer layerId="copper1"/></layers>
        </pcbView>
        <iconView>
            <layers image="icon/Stepper_Motor_-_Unipolar__icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
    </views>
    <connectors>
        <connector id="connector3" name="B" type="male">
            <description>Terminal &quot;B&quot; - Coil Pair 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" legId="connector3leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pin"/>
                <p layer="copper1" svgId="connector3pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector4" name="COMMON_2" type="male">
            <description>Common Tap - Coil Pair 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" legId="connector4leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector4pin"/>
                <p layer="copper1" svgId="connector4pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector5" name="D" type="male">
            <description>Terminal &quot;D&quot; - Coil Pair 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" legId="connector5leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector5pin"/>
                <p layer="copper1" svgId="connector5pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector0" name="A" type="male">
            <description>Terminal &quot;A&quot; - Coil Pair 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" legId="connector0leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                <p layer="copper1" svgId="connector0pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector1" name="COMMON_1" type="male">
            <description>Common Tap - Coil Pair 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" legId="connector1leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                <p layer="copper1" svgId="connector1pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector2" name="C" type="male">
            <description>Terminal &quot;C&quot; - Coil Pair 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" legId="connector2leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                <p layer="copper1" svgId="connector2pin"/></pcbView>
            </views>
        </connector>
    </connectors>
</module>