<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="Blend_Micro_1.0" fritzingVersion="0.5.2b.02.18.4756">
 <version>7</version>
 <date>Mon Jun 27 2016</date>
 <author>Pawel Szymczykowski fixed by f.althaus</author>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'.Helvetica Neue DeskInterface'; font-size:13pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">Blend Micro is a RedBearLab Arduino at Heart integrated development board, they have &amp;quot;blend&amp;quot;ed Arduino with Bluetooth 4.0 Low Energy (aka BLE or Bluetooth Smart) into a single board. It is targeted for makers to develop low power Internet-Of-Things (IoT) projects quickly and easily.&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;br />&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">The micro-controller unit (MCU) is Atmel ATmega32u4 and the BLE chip is Nordic nRF8001. Blend Micro runs as BLE peripheral role only, it allows BLE central role devices to establish connection with.&lt;/p>&lt;/body>&lt;/html></description>
 <title>Blend Micro v1.0</title>
 <url>http://redbearlab.com/blendmicro/</url>
 <tags>
  <tag>ATmega32U4</tag>
  <tag>microcontrollerboard</tag>
  <tag>BLE</tag>
  <tag>ReadBearLabs</tag>
  <tag>Bluetooth</tag>
 </tags>
 <properties>
  <property name="variant">variant 1</property>
  <property name="family">Blend Micro</property>
  <property name="layer"></property>
  <property name="part number"></property>
  <property name="type">Blend Micro (1.0)</property>
 </properties>
 <views>
  <breadboardView>
   <layers image="breadboard/Blend_Micro_1.0_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/Blend_Micro_1.0_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/Blend_Micro_1.0_pcb.svg">
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/Blend_Micro_1.0_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector id="connector1" type="male" name="D8/A8">
   <description>D8/A8</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pin"/>
     <p layer="copper1" svgId="connector1pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" type="male" name="D5/PWM">
   <description>D5/PWM</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector2pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector2pin"/>
     <p layer="copper1" svgId="connector2pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector3" type="male" name="D3/SCL/PWM">
   <description>D3/SCL/PWM</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector3pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector3pin"/>
     <p layer="copper1" svgId="connector3pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector4" type="male" name="D2/SDA">
   <description>D2/SDA</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector4pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector4pin"/>
     <p layer="copper1" svgId="connector4pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector5" type="male" name="D1/TX">
   <description>D1/TX</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector5pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector5pin"/>
     <p layer="copper1" svgId="connector5pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector6" type="male" name="D0/RX">
   <description>D0/RX</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector6pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector6pin"/>
     <p layer="copper1" svgId="connector6pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector7" type="male" name="RST">
   <description>RST</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector7pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector7pin"/>
     <p layer="copper1" svgId="connector7pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector8" type="male" name="MISO">
   <description>MISO</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector8pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector8pin"/>
     <p layer="copper1" svgId="connector8pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector9" type="male" name="MOSI">
   <description>MOSI</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector9pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector9pin"/>
     <p layer="copper1" svgId="connector9pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector10" type="male" name="CLK">
   <description>CLK</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector10pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector10pin"/>
     <p layer="copper1" svgId="connector10pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector11" type="male" name="SS">
   <description>SS</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector11pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector11pin"/>
     <p layer="copper1" svgId="connector11pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector12" type="male" name="VIN">
   <description>VIN</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector12pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector12pin"/>
     <p layer="copper1" svgId="connector12pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector13" type="male" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector13pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector13pin"/>
     <p layer="copper1" svgId="connector13pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector15" type="male" name="D9/PWM/A9">
   <description>D9/PWM/A9</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector15pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector15pin"/>
     <p layer="copper1" svgId="connector15pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector16" type="male" name="D10/PWM/A10">
   <description>D10/PWM/A10</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector16pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector16pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector16pin"/>
     <p layer="copper1" svgId="connector16pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector17" type="male" name="D11/PWM">
   <description>D11/PWM</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector17pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector17pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector17pin"/>
     <p layer="copper1" svgId="connector17pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector18" type="male" name="D12/A11">
   <description>D12/A11</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector18pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector18pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector18pin"/>
     <p layer="copper1" svgId="connector18pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector19" type="male" name="D13/PWM/LED">
   <description>D13/PWM/LED</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector19pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector19pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector19pin"/>
     <p layer="copper1" svgId="connector19pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector20" type="male" name="A0">
   <description>A0</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector20pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector20pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector20pin"/>
     <p layer="copper1" svgId="connector20pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector21" type="male" name="A1">
   <description>A1</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector21pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector21pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector21pin"/>
     <p layer="copper1" svgId="connector21pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector22" type="male" name="A2">
   <description>A2</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector22pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector22pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector22pin"/>
     <p layer="copper1" svgId="connector22pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector23" type="male" name="A3">
   <description>A3</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector23pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector23pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector23pin"/>
     <p layer="copper1" svgId="connector23pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector24" type="male" name="A4">
   <description>A4</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector24pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector24pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector24pin"/>
     <p layer="copper1" svgId="connector24pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector25" type="male" name="A5">
   <description>A5</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector25pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector25pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector25pin"/>
     <p layer="copper1" svgId="connector25pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector26" type="male" name="AREF">
   <description>AREF</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector26pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector26pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector26pin"/>
     <p layer="copper1" svgId="connector26pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector27" type="male" name="V33">
   <description>V33</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector27pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector27pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector27pin"/>
     <p layer="copper1" svgId="connector27pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector34" type="male" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector34pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector34pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector34pin"/>
     <p layer="copper1" svgId="connector34pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector35" type="male" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector35pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector35pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector35pin"/>
     <p layer="copper1" svgId="connector35pin"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
  <bus id="com">
   <nodeMember connectorId="connector19"/>
   <nodeMember connectorId="connector32"/>
   <nodeMember connectorId="connector60"/>
  </bus>
  <bus id="reset">
   <nodeMember connectorId="connector18"/>
   <nodeMember connectorId="connector33"/>
   <nodeMember connectorId="connector59"/>
  </bus>
  <bus id="d12/miso">
   <nodeMember connectorId="connector30"/>
   <nodeMember connectorId="connector55"/>
  </bus>
  <bus id="+5v">
   <nodeMember connectorId="connector34"/>
   <nodeMember connectorId="connector56"/>
  </bus>
  <bus id="d13/sck">
   <nodeMember connectorId="connector45"/>
   <nodeMember connectorId="connector57"/>
  </bus>
  <bus id="d11/mosi">
   <nodeMember connectorId="connector29"/>
   <nodeMember connectorId="connector58"/>
  </bus>
  <bus id="internal1">
   <nodeMember connectorId="connector13"/>
   <nodeMember connectorId="connector14"/>
   <nodeMember connectorId="connector28"/>
  </bus>
 </buses>
</module>
