<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="FreqCtrl-OSCILLATOR-3225">
<version>1</version>
<date>2014-08-04</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>3.2x2.5  oscillators</description>
<title>OSCILLATOR</title>
<tags>
<tag>CRYSTAL-SMD-3225</tag>
<tag>OSCILLATOR</tag>
<tag>3.2X2.5</tag>
</tags>
<properties>
<property name="package">crystal-smd-3.2x2.5</property>
<property name="family">sparkfun Oscillator</property>
<property name="variant">3225</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-freqctrl_crystal-smd-5x3_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/freqctrl_oscillator3225_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/freqctrl_crystal-smd-3.2x2.5_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/sparkfun-freqctrl_crystal-smd-5x3_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector0" name="Pad 1" type="male">
<description>Pad 1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="Pad2" type="male">
<description>Pad 2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>