<?xml version='1.0' encoding='UTF-8'?>
<module referenceFile="powerbutton_adafruit.fzp" moduleId="powerpushbutton_adafruit" fritzingVersion="0.9.2b">
 <version>1</version>
 <author>Fabian Althaus</author>
 <title>Adafruit Push-button Power Switch Breakout</title>
 <url>https://www.adafruit.com/product/1400 </url>
 <label>Btn</label>
 <date>Mo Jul 20 2015</date>
  <tags>
    <tag>Powerbutton</tag>
    <tag>push</tag>
    <tag>breakout</tag>
    <tag>Switch</tag>
    <tag>Adafruit</tag>
    <tag>Pushbutton</tag>
    <tag>Power</tag>
  </tags>
 <properties>
    <property name="family">Button</property>
    <property name="package">THT</property>
    <property name="variant">Adafruit Power Switch</property>
 </properties>
 <description>The Adafruit Push-button Power Switch is a tidy little design that lets you control a DC power source using an everyday tactile button. The breakout uses a latching analog circuit that is triggered by a push of the button. Press once to turn on, then press again to turn off. The circuit uses a 3A P-FET to connect and disconnect the IN pin to the OUT pin. Works great from 3V to 14VDC and up to 3A (although the FET gets a little toasty at continuous 3A draw) yet has only 0.5uA quiescent current draw.</description>
 <views>
  <iconView>
   <layers image="icon/powerpushbutton_adafruit_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/powerpushbutton_adafruit_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView fliphorizontal="true">
   <layers image="schematic/powerpushbutton_adafruit_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/powerpushbutton_adafruit_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
    <connector name="IN" id="connector0" type="male">
     <description>(pin 1) Vcc IN</description>
     <views>
      <breadboardView>
       <p layer="breadboard" svgId="connector0pin"/>
      </breadboardView>
      <schematicView>
       <p terminalId="connector0terminal" layer="schematic" svgId="connector0pin"/>
      </schematicView>
      <pcbView>
       <p layer="copper0" svgId="connector0pin"/>
       <p layer="copper1" svgId="connector0pin"/>
      </pcbView>
     </views>
    </connector>
    <connector name="OUT" id="connector1" type="male">
     <description>(pin 2) OUT</description>
     <views>
      <breadboardView>
       <p layer="breadboard" svgId="connector1pin"/>
      </breadboardView>
      <schematicView>
       <p terminalId="connector1terminal" layer="schematic" svgId="connector1pin"/>
      </schematicView>
      <pcbView>
       <p layer="copper0" svgId="connector1pin"/>
       <p layer="copper1" svgId="connector1pin"/>
      </pcbView>
     </views>
    </connector>
    <connector name="GND" id="connector2" type="male">
     <description>(pin 3) Ground</description>
     <views>
      <breadboardView>
       <p layer="breadboard" svgId="connector2pin"/>
      </breadboardView>
      <schematicView>
       <p terminalId="connector2terminal" layer="schematic" svgId="connector2pin"/>
      </schematicView>
      <pcbView>
       <p layer="copper0" svgId="connector2pin"/>
       <p layer="copper1" svgId="connector2pin"/>
      </pcbView>
     </views>
    </connector>
    <connector name="OFF" id="connector3" type="male">
     <description>(pin 4) off</description>
     <views>
      <breadboardView>
       <p layer="breadboard" svgId="connector3pin"/>
      </breadboardView>
      <schematicView>
       <p terminalId="connector3terminal" layer="schematic" svgId="connector3pin"/>
      </schematicView>
      <pcbView>
       <p layer="copper0" svgId="connector3pin"/>
       <p layer="copper1" svgId="connector3pin"/>
      </pcbView>
     </views>
    </connector>
    <connector name="IN" id="connector4" type="male">
     <description>(pin 5) Vcc IN</description>
     <views>
      <breadboardView>
       <p layer="breadboard" svgId="connector4pin"/>
      </breadboardView>
      <schematicView>
       <p terminalId="connector4terminal" layer="schematic" svgId="connector4pin"/>
      </schematicView>
      <pcbView>
       <p layer="copper0" svgId="connector4pin"/>
       <p layer="copper1" svgId="connector4pin"/>
      </pcbView>
     </views>
    </connector>
    <connector name="OUT" id="connector5" type="male">
     <description>(pin 6) OUT</description>
     <views>
      <breadboardView>
       <p layer="breadboard" svgId="connector5pin"/>
      </breadboardView>
      <schematicView>
       <p terminalId="connector5terminal" layer="schematic" svgId="connector5pin"/>
      </schematicView>
      <pcbView>
       <p layer="copper0" svgId="connector5pin"/>
       <p layer="copper1" svgId="connector5pin"/>
      </pcbView>
     </views>
    </connector>
    <connector name="GND" id="connector6" type="male">
     <description>(pin 7) Ground</description>
     <views>
      <breadboardView>
       <p layer="breadboard" svgId="connector6pin"/>
      </breadboardView>
      <schematicView>
       <p terminalId="connector6terminal" layer="schematic" svgId="connector6pin"/>
      </schematicView>
      <pcbView>
       <p layer="copper0" svgId="connector6pin"/>
       <p layer="copper1" svgId="connector6pin"/>
      </pcbView>
     </views>
    </connector>
    <connector name="OFF" id="connector7" type="male">
     <description>(pin 8) Off</description>
     <views>
      <breadboardView>
       <p layer="breadboard" svgId="connector7pin"/>
      </breadboardView>
      <schematicView>
       <p terminalId="connector7terminal" layer="schematic" svgId="connector7pin"/>
      </schematicView>
      <pcbView>
       <p layer="copper0" svgId="connector7pin"/>
       <p layer="copper1" svgId="connector7pin"/>
      </pcbView>
     </views>
    </connector>
 </connectors>
    <buses>
    <bus id="IN">
     <nodeMember connectorId="connector0"/>
     <nodeMember connectorId="connector4"/>
    </bus>
    <bus id="OUT">
     <nodeMember connectorId="connector1"/>
     <nodeMember connectorId="connector5"/>
    </bus>
    <bus id="GND">
     <nodeMember connectorId="connector2"/>
     <nodeMember connectorId="connector6"/>
    </bus>
    <bus id="Off">
     <nodeMember connectorId="connector3"/>
     <nodeMember connectorId="connector7"/>
    </bus>
 </buses>
</module>