<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.3.17b.04.07.4081" moduleId="81591c6c31ccf12f0f3ccec5f150df2d">
    <version>4</version>
    <author>andre</author>
    <title>Wiring USB Adapter</title>
    <label>USB</label>
    <date>2010-04-11</date>
    <tags>
        <tag>Wiring Mini</tag>
        <tag>USB</tag>
        <tag>FTDI</tag>
        <tag>Serial</tag>
    </tags>
    <properties>
        <property name="family">USB-to-Serial Adapter</property>
        <property name="type">Wiring USB Adapter</property>
    </properties>
    <description>The Wiring USB Adapter connects the Wiring Mini to a host computer. It uses an FTDI FT232R to convert between USB and RS-232 serial commands.</description>
    <views>
        <iconView>
            <layers image="icon/controller_wiring.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/controller_wiring_usb_adapter.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/controller_wiring_usb_adapter.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/wiringmini_usb-adapter.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="keepout"/>
                <layer layerId="soldermask"/>
                <layer layerId="outline"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector type="male" id="connector15" name="RESET">
            <description>Reset</description>
            <views>
                <breadboardView>
                    <p svgId="connector15pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector15pin" layer="schematic" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector15pin" layer="copper0"/>
                    <p svgId="connector15pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector7" name="RX">
            <description>Receive Asynchronous Data</description>
            <views>
                <breadboardView>
                    <p svgId="connector7pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector7pin" layer="copper0"/>
                    <p svgId="connector7pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector16" name="OSCI">
            <description>Oscillator Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector16pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector16pin" layer="schematic" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector16pin" layer="copper0"/>
                    <p svgId="connector16pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector8" name="5V">
            <description>Power Out</description>
            <views>
                <breadboardView>
                    <p svgId="connector8pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector8pin" layer="copper0"/>
                    <p svgId="connector8pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector17" name="OSCO">
            <description>Oscillator Output</description>
            <views>
                <breadboardView>
                    <p svgId="connector17pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector17pin" layer="schematic" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector17pin" layer="copper0"/>
                    <p svgId="connector17pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector9" name="GND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector9pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector9pin" layer="copper0"/>
                    <p svgId="connector9pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector0" name="DTR">
            <description>Data Terminal Ready</description>
            <views>
                <breadboardView>
                    <p svgId="connector0pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector0pin" layer="copper0"/>
                    <p svgId="connector0pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector1" name="RTS">
            <description>Request To Send</description>
            <views>
                <breadboardView>
                    <p svgId="connector1pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1pin" layer="copper0"/>
                    <p svgId="connector1pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector10" name="GND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector10pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector10pin" layer="copper0"/>
                    <p svgId="connector10pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector2" name="RI">
            <description>Ring Indicator</description>
            <views>
                <breadboardView>
                    <p svgId="connector2pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2pin" layer="copper0"/>
                    <p svgId="connector2pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector3" name="DSR">
            <description>Data Set Ready</description>
            <views>
                <breadboardView>
                    <p svgId="connector3pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3pin" layer="copper0"/>
                    <p svgId="connector3pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector11" name="3.3V">
            <description>Power Out</description>
            <views>
                <breadboardView>
                    <p svgId="connector11pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector11pin" layer="copper0"/>
                    <p svgId="connector11pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector4" name="DCD">
            <description>Data Carrier Detect</description>
            <views>
                <breadboardView>
                    <p svgId="connector4pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector4pin" layer="copper0"/>
                    <p svgId="connector4pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector12" name="CBUS3">
            <description>Configurable CBUS</description>
            <views>
                <breadboardView>
                    <p svgId="connector12pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector12pin" layer="copper0"/>
                    <p svgId="connector12pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector5" name="CTS">
            <description>Clear To Send</description>
            <views>
                <breadboardView>
                    <p svgId="connector5pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector5pin" layer="copper0"/>
                    <p svgId="connector5pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector13" name="CBUS2">
            <description>Configurable CBUS</description>
            <views>
                <breadboardView>
                    <p svgId="connector13pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector13pin" layer="copper0"/>
                    <p svgId="connector13pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector14" name="CBUS4">
            <description>Configurable CBUS</description>
            <views>
                <breadboardView>
                    <p svgId="connector14pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector14pin" layer="schematic" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector14pin" layer="copper0"/>
                    <p svgId="connector14pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector6" name="TX">
            <description>Transmit Asynchronous Data</description>
            <views>
                <breadboardView>
                    <p svgId="connector6pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector6pin" layer="copper0"/>
                    <p svgId="connector6pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
