<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='Arduino-Ethernet-v11'>
<version>4</version>
<date>2011-11-29</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;strong&gt;Description:&lt;/strong&gt; Ever wonder what would happen if you stacked an Ethernet shield on an Arduino Pro microcontroller and ran over it with a steam roller? Well, it would probably just break. But in a cartoon world it might turn into the Ethernet Pro! The Ethernet Pro is an Arduino-sized, shield-compatible microcontroller with all of the functionality of the Ethernet shield built right in!&lt;/p&gt;
&lt;p&gt;
The Ethernet Pro is based on the same hardware as the Ethernet shield (Wiznet W5100) in the same configuration so it is a drop-in replacement for the &amp;quot;Arduino/Ethernet double-stack,&amp;quot; and works with all of the existing Ethernet shield libraries and code. This board features the &amp;#39;Optiboot&amp;#39; bootloader, so be sure to select &amp;quot;Arduino Uno&amp;quot; in the Arduino IDE when you program it. The board can be programmed using either an FTDI Basic or the ATmega8U2 breakout (w/ USB-to-Serial firmware).&lt;/p&gt;
&lt;p&gt;
	&lt;strong&gt;Documents: &lt;/strong&gt;&lt;/p&gt;
&lt;ul&gt;
	&lt;li&gt;
		&lt;a href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Dev/Arduino/Boards/Arduino-Ethernet-v112pg.pdf&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;
	&lt;li&gt;
		&lt;a href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Dev/Arduino/Boards/Arduino-Ethernet-v11.zip&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;
	&lt;li&gt;
		&lt;a href=&quot;http://www.sparkfun.com/datasheets/DevTools/Arduino/W5100_Datasheet_v1_1_6.pdf&quot; target=&quot;_blank&quot;&gt;Datasheet&lt;/a&gt; (W5100)&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://arduino.cc/en/Main/ArduinoEthernetShield&quot; target=&quot;_blank&quot;&gt;Arduino EthernetShield Page&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;</description>
<title>Ethernet Pro</title>
<url>http://www.sparkfun.com/products/10536</url>
<tags>
<tag>Arduino</tag>
<tag>Ethernet, Internet</tag>
<tag>Compatible</tag>
</tags>
<properties>
<property name='family'>Arduino</property>
<property name='Voltage'>5V</property>
<property name='Digital Pins'>14</property>
<property name='Analog Pins'>6</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/Arduino-Ethernet-v11_breadboard.svg'>
<layer layerId='breadboardbreadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/Arduino-Ethernet-v11_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/Arduino-Ethernet-v11_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/Arduino-Ethernet-v11_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector0' type='female' name='AD0'>
<description>AD0</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector0pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector0pin' terminalId='connector0terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector0pad'/><p layer='copper1' svgId='connector0pad'/></pcbView>
</views>
</connector>
<connector id='connector1' type='female' name='AD1'>
<description>AD1</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector1pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector1pin' terminalId='connector1terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector1pad'/><p layer='copper1' svgId='connector1pad'/></pcbView>
</views>
</connector>
<connector id='connector2' type='female' name='AD2'>
<description>AD2</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector2pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector2pin' terminalId='connector2terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector2pad'/><p layer='copper1' svgId='connector2pad'/></pcbView>
</views>
</connector>
<connector id='connector3' type='female' name='AD3'>
<description>AD3</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector3pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector3pin' terminalId='connector3terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector3pad'/><p layer='copper1' svgId='connector3pad'/></pcbView>
</views>
</connector>
<connector id='connector4' type='female' name='AD4'>
<description>AD4</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector4pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector4pin' terminalId='connector4terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector4pad'/><p layer='copper1' svgId='connector4pad'/></pcbView>
</views>
</connector>
<connector id='connector5' type='female' name='AD5'>
<description>AD5</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector5pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector5pin' terminalId='connector5terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector5pad'/><p layer='copper1' svgId='connector5pad'/></pcbView>
</views>
</connector>
<connector id='connector68' type='female' name='IO8'>
<description>IO8</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector68pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector68pin' terminalId='connector68terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector68pad'/><p layer='copper1' svgId='connector68pad'/></pcbView>
</views>
</connector>
<connector id='connector69' type='female' name='IO9'>
<description>IO9</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector69pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector69pin' terminalId='connector69terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector69pad'/><p layer='copper1' svgId='connector69pad'/></pcbView>
</views>
</connector>
<connector id='connector70' type='female' name='*CS'>
<description>*CS</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector70pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector70pin' terminalId='connector70terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector70pad'/><p layer='copper1' svgId='connector70pad'/></pcbView>
</views>
</connector>
<connector id='connector71' type='female' name='MOSI'>
<description>MOSI</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector71pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector71pin' terminalId='connector71terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector71pad'/><p layer='copper1' svgId='connector71pad'/></pcbView>
</views>
</connector>
<connector id='connector72' type='female' name='MISO'>
<description>MISO</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector72pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector72pin' terminalId='connector72terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector72pad'/><p layer='copper1' svgId='connector72pad'/></pcbView>
</views>
</connector>
<connector id='connector73' type='female' name='SCLK'>
<description>SCLK</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector73pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector73pin' terminalId='connector73terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector73pad'/><p layer='copper1' svgId='connector73pad'/></pcbView>
</views>
</connector>
<connector id='connector74' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector74pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector74pin' terminalId='connector74terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector74pad'/><p layer='copper1' svgId='connector74pad'/></pcbView>
</views>
</connector>
<connector id='connector75' type='female' name='AREF'>
<description>AREF</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector75pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector75pin' terminalId='connector75terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector75pad'/><p layer='copper1' svgId='connector75pad'/></pcbView>
</views>
</connector>
<connector id='connector76' type='female' name='IO0'>
<description>IO0</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector76pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector76pin' terminalId='connector76terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector76pad'/><p layer='copper1' svgId='connector76pad'/></pcbView>
</views>
</connector>
<connector id='connector77' type='female' name='IO1'>
<description>IO1</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector77pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector77pin' terminalId='connector77terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector77pad'/><p layer='copper1' svgId='connector77pad'/></pcbView>
</views>
</connector>
<connector id='connector78' type='female' name='IO2'>
<description>IO2</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector78pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector78pin' terminalId='connector78terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector78pad'/><p layer='copper1' svgId='connector78pad'/></pcbView>
</views>
</connector>
<connector id='connector79' type='female' name='IO3'>
<description>IO3</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector79pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector79pin' terminalId='connector79terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector79pad'/><p layer='copper1' svgId='connector79pad'/></pcbView>
</views>
</connector>
<connector id='connector80' type='female' name='IO4'>
<description>IO4</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector80pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector80pin' terminalId='connector80terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector80pad'/><p layer='copper1' svgId='connector80pad'/></pcbView>
</views>
</connector>
<connector id='connector81' type='female' name='IO5'>
<description>IO5</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector81pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector81pin' terminalId='connector81terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector81pad'/><p layer='copper1' svgId='connector81pad'/></pcbView>
</views>
</connector>
<connector id='connector82' type='female' name='IO6'>
<description>IO6</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector82pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector82pin' terminalId='connector82terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector82pad'/><p layer='copper1' svgId='connector82pad'/></pcbView>
</views>
</connector>
<connector id='connector83' type='female' name='IO7'>
<description>IO7</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector83pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector83pin' terminalId='connector83terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector83pad'/><p layer='copper1' svgId='connector83pad'/></pcbView>
</views>
</connector>
<connector id='connector98' type='female' name='MISO'>
<description>MISO</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector98pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector98pin' terminalId='connector98terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector98pad'/><p layer='copper1' svgId='connector98pad'/></pcbView>
</views>
</connector>
<connector id='connector99' type='female' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector99pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector99pin' terminalId='connector99terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector99pad'/><p layer='copper1' svgId='connector99pad'/></pcbView>
</views>
</connector>
<connector id='connector100' type='female' name='SCLK'>
<description>SCLK</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector100pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector100pin' terminalId='connector100terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector100pad'/><p layer='copper1' svgId='connector100pad'/></pcbView>
</views>
</connector>
<connector id='connector101' type='female' name='MOSI'>
<description>MOSI</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector101pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector101pin' terminalId='connector101terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector101pad'/><p layer='copper1' svgId='connector101pad'/></pcbView>
</views>
</connector>
<connector id='connector102' type='female' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector102pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector102pin' terminalId='connector102terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector102pad'/><p layer='copper1' svgId='connector102pad'/></pcbView>
</views>
</connector>
<connector id='connector103' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector103pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector103pin' terminalId='connector103terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector103pad'/><p layer='copper1' svgId='connector103pad'/></pcbView>
</views>
</connector>
<connector id='connector128' type='female' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector128pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector128pin' terminalId='connector128terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector128pad'/><p layer='copper1' svgId='connector128pad'/></pcbView>
</views>
</connector>
<connector id='connector129' type='female' name='3.3V'>
<description>3.3V</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector129pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector129pin' terminalId='connector129terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector129pad'/><p layer='copper1' svgId='connector129pad'/></pcbView>
</views>
</connector>
<connector id='connector130' type='female' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector130pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector130pin' terminalId='connector130terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector130pad'/><p layer='copper1' svgId='connector130pad'/></pcbView>
</views>
</connector>
<connector id='connector131' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector131pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector131pin' terminalId='connector131terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector131pad'/><p layer='copper1' svgId='connector131pad'/></pcbView>
</views>
</connector>
<connector id='connector132' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector132pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector132pin' terminalId='connector132terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector132pad'/><p layer='copper1' svgId='connector132pad'/></pcbView>
</views>
</connector>
<connector id='connector133' type='female' name='VIN'>
<description>VIN</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector133pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector133pin' terminalId='connector133terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector133pad'/><p layer='copper1' svgId='connector133pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='miso'>
<nodeMember connectorId='connector72'/>
<nodeMember connectorId='connector98'/>
</bus>
<bus id='sclk'>
<nodeMember connectorId='connector73'/>
<nodeMember connectorId='connector100'/>
</bus>
<bus id='mosi'>
<nodeMember connectorId='connector71'/>
<nodeMember connectorId='connector101'/>
</bus>
<bus id='gnd'>
<nodeMember connectorId='connector74'/>
<nodeMember connectorId='connector103'/>
<nodeMember connectorId='connector131'/>
<nodeMember connectorId='connector132'/>
</bus>
<bus id='reset'>
<nodeMember connectorId='connector102'/>
<nodeMember connectorId='connector128'/>
</bus>
<bus id='5v'>
<nodeMember connectorId='connector99'/>
<nodeMember connectorId='connector130'/>
</bus>
</buses>
</module>
