<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.5.4b.05.18.4914" moduleId="d4d5af9700923b8a114f57961f29a8a0">
    <version>4</version>
    <author>stefanhermann</author>
    <title>RGB LED (com. cathode, rgb)</title>
    <label>LED</label>
    <date>2011-06-11</date>
    <tags>
        <tag>RGB LED</tag>
        <tag>full color</tag>
        <tag>indicator</tag>
    </tags>
    <properties>
        <property name="package">5 mm [THT]</property>
        <property name="family">LED</property>
        <property name="pin order">rgb</property>
        <property name="polarity">common cathode</property>
        <property name="current"></property>
        <property name="rgb">RGB</property>
        <property name="part number"></property>
    </properties>
    <description>A 5mm tri-color LED with red, green and blue inside.</description>
    <views>
        <iconView>
            <layers image="icon/led-rgb-4pin-anode.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/led-rgb-4pin-anode-leg.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/led-rgb-4pin-cathode.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/LED-TRICOLOR-THROUGHHOLE_SparkFun.svg">
                <layer layerId="copper0"/>
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" type="male" name="red anode">
            <description>anode pin for red LED</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" legId="connector0leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pad"/>
                    <p layer="copper1" svgId="connector0pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="common cathode">
            <description>cathode pin for every color, connect to GND</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"  legId="connector1leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pad"/>
                    <p layer="copper1" svgId="connector1pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="male" name="green anode">
            <description>anode pin for green LED</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"  legId="connector2leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pad"/>
                    <p layer="copper1" svgId="connector2pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" type="male" name="blue anode">
            <description>anode pin for blue LED</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" legId="connector3leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pad"/>
                    <p layer="copper1" svgId="connector3pad"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
