<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='SparkFun_CAN-Bus_Shield'>
<version>4</version>
<date>2015-10-31</date>
<author>f.althaus</author>
<description>This shield gives the Arduino CAN-Bus capability. It uses the Microchip MCP2515 CAN controller with MCP2551 CAN transceiver. CAN connection is via a standard 9-way sub-D for use with OBD-II cable. Ideal for automative CAN application. The shield also has a uSD card holder, serial LCD connector and connector for an EM406 GPS module. Making this shield ideal for data logging application.

</description>
<title>CAN-Bus Shield</title>
<url>https://www.sparkfun.com/products/10039</url>
<tags>
<tag>Shield</tag>
<tag>CAN</tag>
<tag>BUS</tag>
<tag>Sparkfun</tag>
</tags>
<properties>
<property name='version'>v13</property>
<property name='family'>Sparkfun Shield</property>
<property name='variant'>CAN BUS</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/SparkFun_CAN-Bus_Shield_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/SparkFun_CAN-Bus_Shield_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/SparkFun_CAN-Bus_Shield_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/SparkFun_CAN-Bus_Shield_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector36' type='female' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector36pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector36pin' terminalId='connector36terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector36pad'/><p layer='copper1' svgId='connector36pad'/></pcbView>
</views>
</connector>
<connector id='connector37' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector37pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector37pin' terminalId='connector37terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector37pad'/><p layer='copper1' svgId='connector37pad'/></pcbView>
</views>
</connector>
<connector id='connector38' type='female' name='CANH'>
<description>CANH</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector38pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector38pin' terminalId='connector38terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector38pad'/><p layer='copper1' svgId='connector38pad'/></pcbView>
</views>
</connector>
<connector id='connector39' type='female' name='CANL'>
<description>CANL</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector39pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector39pin' terminalId='connector39terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector39pad'/><p layer='copper1' svgId='connector39pad'/></pcbView>
</views>
</connector>
<connector id='connector91' type='female' name='3.3V'>
<description>3.3V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector91pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector91pin' terminalId='connector91terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector91pad'/><p layer='copper1' svgId='connector91pad'/></pcbView>
</views>
</connector>
<connector id='connector92' type='female' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector92pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector92pin' terminalId='connector92terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector92pad'/><p layer='copper1' svgId='connector92pad'/></pcbView>
</views>
</connector>
<connector id='connector93' type='female' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector93pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector93pin' terminalId='connector93terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector93pad'/><p layer='copper1' svgId='connector93pad'/></pcbView>
</views>
</connector>
<connector id='connector94' type='female' name='JOY-UP'>
<description>JOY-UP</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector94pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector94pin' terminalId='connector94terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector94pad'/><p layer='copper1' svgId='connector94pad'/></pcbView>
</views>
</connector>
<connector id='connector95' type='female' name='JOY-LEFT'>
<description>JOY-LEFT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector95pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector95pin' terminalId='connector95terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector95pad'/><p layer='copper1' svgId='connector95pad'/></pcbView>
</views>
</connector>
<connector id='connector96' type='female' name='JOY-DOWN'>
<description>JOY-DOWN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector96pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector96pin' terminalId='connector96terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector96pad'/><p layer='copper1' svgId='connector96pad'/></pcbView>
</views>
</connector>
<connector id='connector97' type='female' name='JOY-CLICK'>
<description>JOY-CLICK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector97pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector97pin' terminalId='connector97terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector97pad'/><p layer='copper1' svgId='connector97pad'/></pcbView>
</views>
</connector>
<connector id='connector98' type='female' name='JOY-RIGHT'>
<description>JOY-RIGHT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector98pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector98pin' terminalId='connector98terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector98pad'/><p layer='copper1' svgId='connector98pad'/></pcbView>
</views>
</connector>
<connector id='connector99' type='female' name='AREF'>
<description>AREF</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector99pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector99pin' terminalId='connector99terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector99pad'/><p layer='copper1' svgId='connector99pad'/></pcbView>
</views>
</connector>
<connector id='connector100' type='female' name='CAN_INT'>
<description>CAN_INT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector100pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector100pin' terminalId='connector100terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector100pad'/><p layer='copper1' svgId='connector100pad'/></pcbView>
</views>
</connector>
<connector id='connector101' type='female' name='D3'>
<description>D3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector101pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector101pin' terminalId='connector101terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector101pad'/><p layer='copper1' svgId='connector101pad'/></pcbView>
</views>
</connector>
<connector id='connector102' type='female' name='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector102pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector102pin' terminalId='connector102terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector102pad'/><p layer='copper1' svgId='connector102pad'/></pcbView>
</views>
</connector>
<connector id='connector103' type='female' name='D5'>
<description>D5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector103pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector103pin' terminalId='connector103terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector103pad'/><p layer='copper1' svgId='connector103pad'/></pcbView>
</views>
</connector>
<connector id='connector104' type='female' name='LCD'>
<description>LCD</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector104pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector104pin' terminalId='connector104terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector104pad'/><p layer='copper1' svgId='connector104pad'/></pcbView>
</views>
</connector>
<connector id='connector105' type='female' name='LED2'>
<description>LED2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector105pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector105pin' terminalId='connector105terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector105pad'/><p layer='copper1' svgId='connector105pad'/></pcbView>
</views>
</connector>
<connector id='connector106' type='female' name='LED1'>
<description>LED1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector106pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector106pin' terminalId='connector106terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector106pad'/><p layer='copper1' svgId='connector106pad'/></pcbView>
</views>
</connector>
<connector id='connector107' type='female' name='SD_CS'>
<description>SD_CS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector107pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector107pin' terminalId='connector107terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector107pad'/><p layer='copper1' svgId='connector107pad'/></pcbView>
</views>
</connector>
<connector id='connector108' type='female' name='CAN_CS'>
<description>CAN_CS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector108pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector108pin' terminalId='connector108terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector108pad'/><p layer='copper1' svgId='connector108pad'/></pcbView>
</views>
</connector>
<connector id='connector109' type='female' name='MOSI'>
<description>MOSI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector109pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector109pin' terminalId='connector109terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector109pad'/><p layer='copper1' svgId='connector109pad'/></pcbView>
</views>
</connector>
<connector id='connector110' type='female' name='MISO'>
<description>MISO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector110pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector110pin' terminalId='connector110terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector110pad'/><p layer='copper1' svgId='connector110pad'/></pcbView>
</views>
</connector>
<connector id='connector111' type='female' name='SCK'>
<description>SCK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector111pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector111pin' terminalId='connector111terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector111pad'/><p layer='copper1' svgId='connector111pad'/></pcbView>
</views>
</connector>
<connector id='connector112' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector112pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector112pin' terminalId='connector112terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector112pad'/><p layer='copper1' svgId='connector112pad'/></pcbView>
</views>
</connector>
<connector id='connector113' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector113pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector113pin' terminalId='connector113terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector113pad'/><p layer='copper1' svgId='connector113pad'/></pcbView>
</views>
</connector>
<connector id='connector114' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector114pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector114pin' terminalId='connector114terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector114pad'/><p layer='copper1' svgId='connector114pad'/></pcbView>
</views>
</connector>
<connector id='connector115' type='female' name='IOREF'>
<description>IOREF</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector115pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector115pin' terminalId='connector115terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector115pad'/><p layer='copper1' svgId='connector115pad'/></pcbView>
</views>
</connector>
<connector id='connector116' type='female' name='NC'>
<description>NC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector116pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector116pin' terminalId='connector116terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector116pad'/><p layer='copper1' svgId='connector116pad'/></pcbView>
</views>
</connector>
<connector id='connector117' type='female' name='RS'>
<description>RS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector117pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector117pin' terminalId='connector117terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector117pad'/><p layer='copper1' svgId='connector117pad'/></pcbView>
</views>
</connector>
<connector id='connector118' type='female' name='RX'>
<description>RX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector118pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector118pin' terminalId='connector118terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector118pad'/><p layer='copper1' svgId='connector118pad'/></pcbView>
</views>
</connector>
<connector id='connector119' type='female' name='SCL'>
<description>SCL</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector119pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector119pin' terminalId='connector119terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector119pad'/><p layer='copper1' svgId='connector119pad'/></pcbView>
</views>
</connector>
<connector id='connector120' type='female' name='SDA'>
<description>SDA</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector120pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector120pin' terminalId='connector120terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector120pad'/><p layer='copper1' svgId='connector120pad'/></pcbView>
</views>
</connector>
<connector id='connector121' type='female' name='TX'>
<description>TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector121pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector121pin' terminalId='connector121terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector121pad'/><p layer='copper1' svgId='connector121pad'/></pcbView>
</views>
</connector>
<connector id='connector122' type='female' name='12V'>
<description>12V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector122pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector122pin' terminalId='connector122terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector122pad'/><p layer='copper1' svgId='connector122pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='5v'>
<nodeMember connectorId='connector36'/>
<nodeMember connectorId='connector92'/>
</bus>
<bus id='gnd'>
<nodeMember connectorId='connector37'/>
<nodeMember connectorId='connector112'/>
<nodeMember connectorId='connector113'/>
<nodeMember connectorId='connector114'/>
</bus>
</buses>
</module>
