<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="PC847X_7eb43b60a64029b53561d2a746e15e5e_1" fritzingVersion="0.9.0b">
 <version>5</version>
 <author>ThomDietrich</author>
 <title>Sharp PC847X</title>
 <label>U</label>
 <date>Do Jun 23 2016</date>
 <tags>
  <tag>isolator</tag>
  <tag>IC</tag>
  <tag>optocoupler</tag>
 </tags>
 <properties>
  <property name="part">PC847X</property>
  <property name="family">Optocoupler</property>
  <property name="package">THT</property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">&#xd;
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">&#xd;
p, li { white-space: pre-wrap; }&#xd;
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt; font-weight:400; font-style:normal;">&#xd;
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">Optocoupler with four channels on one chip (without sensititvity pins)&lt;/p>&#xd;
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">PC847X / 4x 817X / LTV 847&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/PC847X_5.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/PC847X_5.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/PC847X_5.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/PC847X_5.svg">
    <layer layerId="copper0"/>
    <layer layerId="keepout"/>
    <layer layerId="soldermask"/>
    <layer layerId="silkscreen"/>
    <layer layerId="outline"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector3" type="male" name="Pin 4">
   <description>Cathode</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard" terminalId="connector3terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper0"/>
     <p svgId="connector3pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector4" type="male" name="Pin 5">
   <description>Anode</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard" terminalId="connector4terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper0"/>
     <p svgId="connector4pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector5" type="male" name="Pin 6">
   <description>Cathode</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard" terminalId="connector5terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper0"/>
     <p svgId="connector5pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector0" type="male" name="Pin 1">
   <description>Anode</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" type="male" name="Pin 2">
   <description>Cathode</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" type="male" name="Pin 3">
   <description>Anode</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector7" type="male" name="Pin 7">
   <description>Anode</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper0"/>
     <p svgId="connector7pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector8" type="male" name="Pin 8">
   <description>Cathode</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper0"/>
     <p svgId="connector8pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector9" type="male" name="Pin 9">
   <description>Emitter</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper0"/>
     <p svgId="connector9pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector10" type="male" name="Pin 10">
   <description>Collector</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper0"/>
     <p svgId="connector10pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector11" type="male" name="Pin 11">
   <description>Emitter</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper0"/>
     <p svgId="connector11pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector12" type="male" name="Pin 12">
   <description>Collector</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper0"/>
     <p svgId="connector12pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector13" type="male" name="Pin 13">
   <description>Emitter</description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector13pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pin" layer="copper0"/>
     <p svgId="connector13pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector14" type="male" name="Pin 14">
   <description>Collector</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pin" layer="copper0"/>
     <p svgId="connector14pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector15" type="male" name="Pin 15">
   <description>Emitter</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pin" layer="copper0"/>
     <p svgId="connector15pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector16" type="male" name="Pin 16">
   <description>Collector</description>
   <views>
    <breadboardView>
     <p svgId="connector16pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector16pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector16pin" layer="copper0"/>
     <p svgId="connector16pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <url>http://www.sharpsma.com/download/pc847x-epdf</url>
</module>
