<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="capacitor_elko_goldcap_4.0F_92eef0d1d2f548b9db9918a1769107d3_2" fritzingVersion="0.2.1223" referenceFile="capacitor_electrolytic_large.fzp">
 <version>4</version>
 <author>Christoph Wempe</author>
 <title>Electrolytic Capacitor</title>
 <label>C</label>
 <date>Di Jan 16 2018</date>
 <tags>
  <tag>Electrolytic</tag>
  <tag>Supercap</tag>
  <tag>Capacitor</tag>
  <tag>Goldcap</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="family">capacitor [unidirectional]</property>
  <property name="variant">variant 1</property>
  <property name="part number"></property>
  <property name="voltage"></property>
  <property name="layer"></property>
  <property name="capacitance">4.0F</property>
  <property name="package">2cm H-Type</property>
 </properties>
 <taxonomy>discreteParts.capacitor.electrolytic</taxonomy>
 <description>1000µF electrolytic capacitor</description>
 <spice>
  <line>C{instanceTitle} {net connector0} {net connector1} {capacitance} IC=0</line>
 </spice>
 <views>
  <iconView>
   <layers image="icon/capacitor_elko_goldcap_4.0F_8647a5c11c9b485c095f1ac7ddec049d_2_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView flipvertical="true" fliphorizontal="true">
   <layers image="breadboard/capacitor_elko_goldcap_4.0F_8647a5c11c9b485c095f1ac7ddec049d_2_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/capacitor_elko_goldcap_4.0F_8647a5c11c9b485c095f1ac7ddec049d_2_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/capacitor_elko_goldcap_4.0F_8647a5c11c9b485c095f1ac7ddec049d_2_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="male" id="connector0" name="-">
   <description>- side</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard" legId="connector0leg"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector1" name="+">
   <description>+ side</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard" legId="connector1leg"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>
