<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="JST-VHR-3N" fritzingVersion="0.9.3.b">
 <version>5</version>
 <author>Stephen G. Parry</author>
 <title>JST-VHR-3N</title>
 <label>J</label>
 <date>Thu Jun 16 2016</date>
 <tags>
  <tag>VH</tag>
  <tag>JST</tag>
 </tags>
 <properties>
  <property name="family">JST VH Pin Header</property>
  <property name="variant">- Female 3 pin connector</property>
  <property name="hole size"></property>
  <property name="part number">JST-VHR-3N</property>
  <property name="Pin Spacing">0.156in (3.96mm)</property>
  <property name="Form">♀ (female)</property>
  <property name="Pins">3</property>
  <property name="layer"></property>
  <property name="package">THT</property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">JST-VHR-3N&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'Oxygen-Sans'; font-size:10pt;">Female 3 pin connector receptacle from JST VH series&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'Oxygen-Sans'; font-size:10pt;">This plug is used on Dagu motors in their robots. It is designed to mate with the JST-B3P-VH male header.&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'Oxygen-Sans'; font-size:10pt;">Note that because of the difference in alignment and spacing, the rear connection and front connection holes are represented as different connectors, with an internal connection between. When plugging onto the male header, ensure that the correct connectors have located.&lt;/span>&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:'Oxygen-Sans'; font-size:10pt;">&lt;br />&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/JST-VHR-3N_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/JST-VHR-3N_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView fliphorizontal="true">
   <layers image="schematic/JST-VHR-3N_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/JST-VHR-3N_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector name="pin1" id="connector1" type="male">
   <description>pin 1</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector name="pin2" id="connector0" type="male">
   <description>pin 2</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector name="pin3" id="connector2" type="male">
   <description>pin 3</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector name="pin 4" id="connector4" type="female">
   <description>pin 4</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" terminalId="connector3terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" terminalId="connector3terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="unknown" hybrid="yes" />
    </pcbView>
   </views>
  </connector>
  <connector name="pin 5" id="connector3" type="female">
   <description>pin 5</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" terminalId="connector4terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" terminalId="connector4terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="unknown" hybrid="yes" />
    </pcbView>
   </views>
  </connector>
  <connector name="pin 6" id="connector5" type="female">
   <description>pin 6</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" terminalId="connector5terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" terminalId="connector5terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="unknown" hybrid="yes" />
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
  <bus id="internal1">
   <nodeMember connectorId="connector0"/>
   <nodeMember connectorId="connector3"/>
  </bus>
  <bus id="internal2">
   <nodeMember connectorId="connector1"/>
   <nodeMember connectorId="connector4"/>
  </bus>
  <bus id="internal3">
   <nodeMember connectorId="connector2"/>
   <nodeMember connectorId="connector5"/>
  </bus>
 </buses>
</module>
