<?xml version='1.0' encoding='UTF-8'?>
<module referenceFile="mcp3008.fzp" fritzingVersion="0.7.2b" moduleId="mcp3008">
 <version>1</version>
 <date>Sat Mar 31 2018</date>
 <label>ADC</label>
 <author>ravi.csin@gmail.com</author>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'Ubuntu'; font-size:11pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">2.7V 4-Channel/8-Channel 10-Bit A/D Converters with SPI Serial Interface&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">The Microchip Technology Inc. MCP3004/3008&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">devices are successive approximation 10-bit Analog-&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">to-Digital (A/D) converters with on-board sample and&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">hold circuitry. The MCP3004 is programmable to&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">provide two pseudo-differential input pairs or four&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">single-ended inputs. The MCP3008 is programmable&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">to provide four pseudo-differential input pairs or eight&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">single-ended inputs. Differential Nonlinearity (DNL)&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">and Integral Nonlinearity (INL) are specified at ±1 LSB.&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">Communication with the devices is accomplished using&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">a simple serial interface compatible with the SPI&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">protocol. The devices are capable of conversion rates&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">of up to 200 ksps. The MCP3004/3008 devices operate&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">over a broad voltage range (2.7V - 5.5V). Low-current&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">design permits operation with typical standby currents&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">of only 5 nA and typical active currents of 320 μA. The&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">MCP3004 is offered in 14-pin PDIP, 150 mil SOIC and&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">TSSOP packages, while the MCP3008 is offered in 16-&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">pin PDIP and SOIC packages.&lt;/p>&lt;/body>&lt;/html></description>
 <title>MCP3008</title>
 <tags>
  <tag>MCP3008</tag>
  <tag>DIL16</tag>
  <tag>DIP</tag>
 </tags>
 <properties>
  <property name="family">Generic A2D</property>
  <property name="variant">variant 1</property>
  <property name="bit resolution">10</property>
  <property name="layer"></property>
  <property name="sampling rate">200 ksps max. sampling rate at V DD = 5V/75 ksps max. sampling rate at V DD = 2.7V</property>
  <property name="channels">8</property>
  <property name="package">dil16</property>
  <property name="part number"></property>
  <property name="interface ">SPI</property>
  <property name="chip">MCP3008</property>
  <property name="interface">SPI</property>
 </properties>
 <views>
  <breadboardView>
   <layers image="breadboard/mcp3008.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/mcp3008.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/mcp3008.svg">
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/mcp3008.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector type="male" name="CS/SHDN" id="connector9">
   <description>Select Logic</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector9pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector9terminal" svgId="connector9pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector9pad"/>
     <p layer="copper1" svgId="connector9pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="DGND" id="connector8">
   <description>Digital Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector8pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector8terminal" svgId="connector8pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector8pad"/>
     <p layer="copper1" svgId="connector8pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="CH7" id="connector7">
   <description>Input Channel 7</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector7pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector7terminal" svgId="connector7pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector7pad"/>
     <p layer="copper1" svgId="connector7pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="CH5" id="connector5">
   <description>Input Channel 5</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector5pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector5terminal" svgId="connector5pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector5pad"/>
     <p layer="copper1" svgId="connector5pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="VDD" id="connector15">
   <description>Voltage</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector15pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector15terminal" svgId="connector15pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector15pad"/>
     <p layer="copper1" svgId="connector15pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="CH6" id="connector6">
   <description>Input Channel 6</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector6pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector6terminal" svgId="connector6pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector6pad"/>
     <p layer="copper1" svgId="connector6pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="CLK" id="connector12">
   <description>Clock</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector12pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector12pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector12pad"/>
     <p layer="copper1" svgId="connector12pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="Dout" id="connector11">
   <description>Digital Out</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector11pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector11terminal" svgId="connector11pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector11pad"/>
     <p layer="copper1" svgId="connector11pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="AGND" id="connector13">
   <description>Analog Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector13pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector13terminal" svgId="connector13pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector13pad"/>
     <p layer="copper1" svgId="connector13pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="VREF" id="connector14">
   <description>Voltage Reference</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector14pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector14terminal" svgId="connector14pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector14pad"/>
     <p layer="copper1" svgId="connector14pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="Din" id="connector10">
   <description>Digital In</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector10pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector10terminal" svgId="connector10pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector10pad"/>
     <p layer="copper1" svgId="connector10pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="CH2" id="connector2">
   <description>Input Channel 2</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector2terminal" svgId="connector2pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector2pad"/>
     <p layer="copper1" svgId="connector2pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="CH0" id="connector0">
   <description>Input Channel 0</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pad"/>
     <p layer="copper1" svgId="connector0pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="CH4" id="connector4">
   <description>Input Channel 4</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector4pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector4terminal" svgId="connector4pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector4pad"/>
     <p layer="copper1" svgId="connector4pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="CH1" id="connector1">
   <description>Input Channel 1</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector1terminal" svgId="connector1pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pad"/>
     <p layer="copper1" svgId="connector1pad"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" name="CH3" id="connector3">
   <description>Input Channel 3</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" terminalId="connector3terminal" svgId="connector3pin"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector3pad"/>
     <p layer="copper1" svgId="connector3pad"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses/>
</module>
