<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.6.5b.01.02.5717" moduleId="e3afbdaad7b1e3e1408df3c505763145">
    <version replacedby="AVR_SPI_PROG-PTH">4</version>
    <author>Fritzing Part-o-matic</author>
    <title>avr isp 10 pin</title>
    <label>ISP</label>
    <date>2009-10-23</date>
    <tags>
        <tag>avr</tag>
        <tag>isp</tag>
    </tags>
    <properties>
        <property name="package">THT</property>
        <property name="family">//obsolete//Pin Header</property>
        <property name="form">♂ (shrouded male)</property>
        <property name="part number"></property>
        <property name="pin spacing">0.1in (2.54mm)</property>
        <property name="pins">10</property>
    </properties>
    <description>Generic shrouded header</description>
    <views>
        <iconView>
            <layers image="icon/avr_isp_10_pin_icon.svg">
                <layer layerId="breadboard"/>
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/avr_isp_10_pin_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <pcbView>
            <layers image="pcb/avr_isp_10_pin_pcb.svg">
                <layer layerId="copper1"/>
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
        <schematicView>
            <layers image="schematic/avr_isp_10_pin_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
    </views>
    <connectors>
        <connector id="connector3" type="male" name="sck" replacedby="connector6">
            <description>sck-pin 4</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pin"/>
                    <p layer="copper0" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" type="male" name="miso" replacedby="connector8">
            <description>miso-pin 5</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pin"/>
                    <p layer="copper0" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" type="male" name="gnd"  replacedby="connector9" >
            <description>pin 6</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" terminalId="connector5terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector5pin"/>
                    <p layer="copper0" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" type="male" name="gnd"  replacedby="connector7">
            <description>pin 7</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin" terminalId="connector6terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector6pin"/>
                    <p layer="copper0" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" type="male" name="rxd" replacedby="connector5">
            <description>pin 8</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin" terminalId="connector7terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector7pin"/>
                    <p layer="copper0" svgId="connector7pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" type="male" name="txd" replacedby="connector3">
            <description>pin 9</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin" terminalId="connector8terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector8pin"/>
                    <p layer="copper0" svgId="connector8pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" type="male" name="vcc" replacedby="connector1">
            <description>pin 10</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin" terminalId="connector9terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector9pin"/>
                    <p layer="copper0" svgId="connector9pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" type="male" name="mosi" replacedby="connector0">
            <description>mosi-pin 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin"/>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="not connected" replacedby="connector2">
            <description>pin 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="male" name="/reset"  replacedby="connector4">
            <description>reset-pin 3</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pin"/>
                    <p layer="copper0" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
