<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Electromechanical-FKIT-RIBBON_CONNECTOR--2MM_R_REV2">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Electromechanical' FKIT-RIBBON_CONNECTOR -2MM_R_REV2 -->
<version>4</version>
<date>2013-02-13</date>
<label>J</label>
<author>www.fritzing.org</author>
<description>&lt;h3&gt;fabrick.it Conductive Ribbon Connector&lt;/h3&gt;</description>
<title>FKIT-RIBBON_CONNECTOR</title>
<tags>
<tag>FKIT-RIBBON_CONNECTOR_03_2MM_R</tag>
<tag>FKIT-RIBBON_CONNECTOR</tag>
<tag>-2MM_R_REV2</tag>
</tags>
<properties>
<property name="package">fkit-ribbon_connector_03_2mm_r</property>
<property name="family">sparkfun E-Textiles Connector</property>
<property name="function">Ribbon</property>
<property name="variant">-2mm_r_rev2</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-electromechanical_fkit-ribbon_connector_03_2mm_r_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-electromechanical_fkit-connector_cond_03_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-electromechanical_fkit-ribbon_connector_03_2mm_r_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
<layer layerId="copper0"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/FKIT-RIBBON_CONNECTOR_03_2MM_R.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector2" name="P$1" type="male">
<description>P$1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector2pad"/>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="P$2" type="male">
<description>P$2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector5pad"/>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="P$3" type="male">
<description>P$3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector8pad"/>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>