<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='SHT1x-Breakout'>
<version>4</version>
<date>2015-10-04</date>
<author>f.althaus</author>
<description>The SHT15 Breakout is an easy to use, highly accurate, digital temperature and humidity sensor. This board has been fully calibrated and offers high precision and excellent long-term stability at low cost. The digital CMOSens® technology integrates two sensors and readout circuitry on one single chip. All you need is two lines for 2-wire communication, and you’ll have relative humidity and temperature readings to help you sense the world around you!



The two sensors built into the SHT15 have been seamlessly coupled to a 14bit analog to digital converter and a serial interface circuit resulting in superior signal quality, fast response time, and a strong resistance to external disturbances. Additionally, the on board SHT15 features a 0-100% RH measurement range with a temperature accuracy of +/- 0.3°C @ 25°C. There are only four pins that need to be hooked up in order to start using this sensor in a project. One for VCC, one for GND, and the two data lines SDA and SCL.</description>
<title>SHT1x-Breakout</title>
<url>https://www.sparkfun.com/products/13683</url>
<tags>
<tag>Breakout</tag>
<tag>SHT1x</tag>
<tag>SHT1</tag>
<tag>Sparkfun</tag>
</tags>
<properties>
<property name='version'>v14</property>
<property name='family'>Sparkfun Breakout</property>
<property name='variant'>SHT15</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/SHT1x-Breakout_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/SHT1x-Breakout_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/SHT1x-Breakout_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/SHT1x-Breakout_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector4' type='female' name='SCK'>
<description>SCK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector4pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector4pin' terminalId='connector4terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector4pad'/><p layer='copper1' svgId='connector4pad'/></pcbView>
</views>
</connector>
<connector id='connector5' type='female' name='DATA'>
<description>DATA</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector5pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector5pin' terminalId='connector5terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector5pad'/><p layer='copper1' svgId='connector5pad'/></pcbView>
</views>
</connector>
<connector id='connector6' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector6pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector6pin' terminalId='connector6terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector6pad'/><p layer='copper1' svgId='connector6pad'/></pcbView>
</views>
</connector>
<connector id='connector7' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector7pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector7pin' terminalId='connector7terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector7pad'/><p layer='copper1' svgId='connector7pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
