<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.9.0b.04.10.5970" moduleId="Raspberry Pi B+" referenceFile="Raspberry_Pi_B+.fzp">
 <version>5</version>
 <author>Fabian Althaus</author>
 <title>Raspberry Pi B+</title>
 <label>Raspberry Pi</label>
 <date>Aug 13 2014</date>
 <url>http://www.raspberrypi.org/</url>
 <tags>
  <tag>Raspberry</tag>
  <tag>Raspberry Pi</tag>
  <tag>RPi</tag>
  <tag>B+</tag>
 </tags>
 <properties>
  <property name="family">CPU Board (Raspberry Pi)</property>
  <property name="processor">Broadcom SoC BCM2835 ARMv6</property>
  <property name="variant">Raspberry Pi B+</property>
    <property name="revision">RPI-BPLUS-V1.2</property>
 </properties>
 <description>The awesome Raspberry Pi ARM Board with 40 pin GPIO. Ready for special designed Raspberry Pi B+ Hat (Hardware attached (on) top)</description>
 <views>
  <iconView>
   <layers image="icon/Raspberry_Pi_b+_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/raspberry_pi_b+_breadboard.svg">
    <layer layerId="breadboardbreadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/raspberry_pi_b+_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/Raspberry_Pi_b+_pcb.svg">
    <layer layerId="copper0"/>
	
    <layer layerId="copper1"/>
	  <layer layerId="silkscreen"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
   <connector id="connector0" name="3v3" type="male">
   <description>power - 3.3V</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector0pin" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pin"/>
    <p layer="copper1" svgId="connector0pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector1" name="GPIO2" type="male">
   <description>SDA1 I2C</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector1pin" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pin"/>
    <p layer="copper1" svgId="connector1pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector2" name="GPIO3" type="male">
   <description>SCL1 I2C</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector2pin" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector2pin"/>
    <p layer="copper1" svgId="connector2pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector3" name="GPIO4" type="male">
   <description>GPIO4</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector3pin" terminalId="connector3terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector3pin"/>
    <p layer="copper1" svgId="connector3pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector4" name="GND" type="male">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector4pin" terminalId="connector4terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector4pin"/>
    <p layer="copper1" svgId="connector4pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector5" name="GPIO17" type="male">
   <description>GPIO17</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector5pin" terminalId="connector5terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector5pin"/>
    <p layer="copper1" svgId="connector5pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector6" name="GPIO27" type="male">
   <description>GPIO27</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector6pin" terminalId="connector6terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector6pin"/>
    <p layer="copper1" svgId="connector6pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector7" name="GPIO22" type="male">
   <description>GPIO22</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector7pin" terminalId="connector7terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector7pin"/>
    <p layer="copper1" svgId="connector7pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector8" name="3V3" type="male">
   <description>power - 3.3V</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector8pin" terminalId="connector8terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector8pin"/>
    <p layer="copper1" svgId="connector8pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector9" name="GPIO10" type="male">
   <description>SPI0_MOSI - GPIO10</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector9pin" terminalId="connector9terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector9pin"/>
    <p layer="copper1" svgId="connector9pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector10" name="GPIO9" type="male">
   <description>SPI0_MISO - GPIO9</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector10pin" terminalId="connector10terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector10pin"/>
    <p layer="copper1" svgId="connector10pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector11" name="GPIO11" type="male">
   <description>SPI0_SCLK - GPIO11</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector11pin" terminalId="connector11terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector11pin"/>
    <p layer="copper1" svgId="connector11pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector12" name="GND" type="male">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector12pin" terminalId="connector12terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector12pin"/>
    <p layer="copper1" svgId="connector12pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector13" name="ID_SD" type="male">
   <description>I2C ID EEPROM</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector13pin" terminalId="connector13terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector13pin"/>
    <p layer="copper1" svgId="connector13pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector14" name="GPIO5" type="male">
   <description>GPIO5</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector14pin" terminalId="connector14terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector14pin"/>
    <p layer="copper1" svgId="connector14pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector15" name="GPIO6" type="male">
   <description>GPIO6</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector15pin" terminalId="connector15terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector15pin"/>
    <p layer="copper1" svgId="connector15pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector16" name="GPIO13" type="male">
   <description>GPIO13</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector16pin" terminalId="connector16terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector16pin"/>
    <p layer="copper1" svgId="connector16pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector17" name="GPIO19" type="male">
   <description>GPIO19</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector17pin" terminalId="connector17terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector17pin"/>
    <p layer="copper1" svgId="connector17pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector18" name="GPIO26" type="male">
   <description>GPIO26</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector18pin" terminalId="connector18terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector18pin"/>
    <p layer="copper1" svgId="connector18pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector19" name="GND" type="male">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector19pin" terminalId="connector19terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector19pin"/>
    <p layer="copper1" svgId="connector19pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector20" name="GPIO21" type="male">
   <description>GPIO21</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector20pin" terminalId="connector20terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector20pin"/>
    <p layer="copper1" svgId="connector20pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector21" name="GPIO20" type="male">
   <description>GPIO20</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector21pin" terminalId="connector21terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector21pin"/>
    <p layer="copper1" svgId="connector21pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector22" name="GPIO16" type="male">
   <description>GPIO16</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector22pin" terminalId="connector22terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector22pin"/>
    <p layer="copper1" svgId="connector22pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector23" name="GND" type="male">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector23pin" terminalId="connector23terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector23pin"/>
    <p layer="copper1" svgId="connector23pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector24" name="GPIO12" type="male">
   <description>GPIO12</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector24pin" terminalId="connector24terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector24pin" terminalId="connector24terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector24pin"/>
    <p layer="copper1" svgId="connector24pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector25" name="GND" type="male">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector25pin" terminalId="connector25terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector25pin" terminalId="connector25terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector25pin"/>
    <p layer="copper1" svgId="connector25pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector26" name="ID_SC" type="male">
   <description>I2C ID EEPROM</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector26pin" terminalId="connector26terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector26pin" terminalId="connector26terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector26pin"/>
    <p layer="copper1" svgId="connector26pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector27" name="GPIO7" type="male">
   <description>SPI0_CE1_N - GPIO7</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector27pin" terminalId="connector27terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector27pin" terminalId="connector27terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector27pin"/>
    <p layer="copper1" svgId="connector27pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector28" name="GPIO8" type="male">
   <description>SPI0_CE0_N - GPIO8</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector28pin" terminalId="connector28terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector28pin" terminalId="connector28terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector28pin"/>
    <p layer="copper1" svgId="connector28pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector29" name="GPIO25" type="male">
   <description>GPIO25</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector29pin" terminalId="connector29terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector29pin" terminalId="connector29terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector29pin"/>
    <p layer="copper1" svgId="connector29pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector30" name="GND" type="male">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector30pin" terminalId="connector30terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector30pin" terminalId="connector30terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector30pin"/>
    <p layer="copper1" svgId="connector30pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector31" name="GPIO24" type="male">
   <description>GPIO24</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector31pin" terminalId="connector31terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector31pin" terminalId="connector31terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector31pin"/>
    <p layer="copper1" svgId="connector31pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector32" name="GPIO23" type="male">
   <description>GPIO23</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector32pin" terminalId="connector32terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector32pin" terminalId="connector32terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector32pin"/>
    <p layer="copper1" svgId="connector32pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector33" name="GND" type="male">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector33pin" terminalId="connector33terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector33pin" terminalId="connector33terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector33pin"/>
    <p layer="copper1" svgId="connector33pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector34" name="GPIO18" type="male">
   <description>PCM_CLK - GPIO18</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector34pin" terminalId="connector34terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector34pin" terminalId="connector34terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector34pin"/>
    <p layer="copper1" svgId="connector34pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector35" name="GPIO15" type="male">
   <description>UART0_RXD - GPIO15</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector35pin" terminalId="connector35terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector35pin" terminalId="connector35terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector35pin"/>
    <p layer="copper1" svgId="connector35pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector36" name="GPIO14" type="male">
   <description>UART0_TXD - GPIO14</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector36pin" terminalId="connector36terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector36pin" terminalId="connector36terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector36pin"/>
    <p layer="copper1" svgId="connector36pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector37" name="GND" type="male">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector37pin" terminalId="connector37terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector37pin" terminalId="connector37terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector37pin"/>
    <p layer="copper1" svgId="connector37pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector38" name="5V" type="male">
   <description>power - 5V</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector38pin" terminalId="connector38terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector38pin" terminalId="connector38terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector38pin"/>
    <p layer="copper1" svgId="connector38pin"/></pcbView>
   </views>
  </connector>
    <connector id="connector39" name="5V" type="male">
   <description>power - 5V</description>
   <views>
    <breadboardView>
     <p layer="breadboardbreadboard" svgId="connector39pin" terminalId="connector39terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector39pin" terminalId="connector39terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector39pin"/>
    <p layer="copper1" svgId="connector39pin"/></pcbView>
   </views>
  </connector>
  </connectors>
  <buses>
  <bus id="5V">
   <nodeMember connectorId="connector38"/>
   <nodeMember connectorId="connector39"/>
  </bus>
  <bus id="3V3">
   <nodeMember connectorId="connector0"/>
   <nodeMember connectorId="connector8"/>
  </bus>
    <bus id="GND">
   <nodeMember connectorId="connector4"/>
   <nodeMember connectorId="connector12"/>
      <nodeMember connectorId="connector19"/>
   <nodeMember connectorId="connector23"/>
   <nodeMember connectorId="connector25"/>
      <nodeMember connectorId="connector30"/>
         <nodeMember connectorId="connector33"/>
            <nodeMember connectorId="connector37"/>
  </bus>
 </buses>
</module>
