<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Passives-RESISTOR-2512-ResistorModuleID">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Passives' RESISTOR 2512 -->
<version>4</version>
<date>2013-02-13</date>
<label>R</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;Resistor&lt;/b&gt;
Basic schematic elements and footprints for 0603, 1206, and PTH resistors.</description>
<title>Resistor</title>
<tags>
<tag>R2512</tag>
<tag>2512</tag>
<tag>RESISTOR</tag>
</tags>
<properties>
<property name="package">2512 [SMD]</property>
<property name="family">Resistor</property>
        <property name="Resistance" showInLabel="yes">220</property>
      <property name="power" showInLabel="yes"/>
      <property name="tolerance" showInLabel="yes">&#177;5%</property>

</properties>
<views>
<breadboardView>
<layers image="breadboard/resistor_220.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/resistor.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-passives_r2512_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/resistor_icon_220.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector0" name="Pin 0" type="male">
<description>Pin0</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin" legId="connector0leg"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="Pin 1" type="male">
<description>Pin 1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"  legId="connector1leg"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>