<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='Arduino Voice Shield-v16'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Description: &lt;/span&gt;The VoiceBox Shield can be mounted on top of your &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=666&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;Arduino USB Board&lt;/a&gt; or &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9219&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;Pro&lt;/a&gt;, to give it access to all capabilities of the &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9578&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;SpeakJet&lt;/a&gt; voice and sound synthesizer. &lt;span class=&quot;description&quot;&gt;The Voice Box Shield uses the SpeakJet chip to convert serial commands into a great robot-sounding voice.&lt;/span&gt;&lt;br /&gt;


	&lt;br /&gt;


	Populated on the VoiceBox Shield are the 18-DIP SpeakJet IC and a two stage audio amplifier with a potentiometer to set the gain. You can connect a speaker directly to the &amp;#39;SPK+/-&amp;#39; pins, and get your Arduino-bot talking with very minimal work!&lt;br /&gt;


	&lt;br /&gt;


	You can control the SpeakJet through either its serial line, or the eight event input lines which are connected to digital pins 5-12. A 3-way jumper allows you to connect either the software (D2) or hardware (D1) TX pin of the Arduino to the SpeakJet&amp;#39;s serial input.&lt;br /&gt;


	&lt;br /&gt;


	Also included on the shield are a 13x7 grid of 0.1&amp;quot; pitch through-holes for prototyping, the Arduino&amp;#39;s reset button. Headers are not included, we recommend the &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9280&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;6&lt;/a&gt; and &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9279&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;8-pin stackable headers&lt;/a&gt;.&lt;br /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/DevTools/Arduino/Arduino%20Voice%20Shield-v13.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/Code/SpeakJet_Sample.zip&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Example Code&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.youtube.com/watch?v=Eo3hEKAOxeg&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Listen to the SpeakJet!&lt;/a&gt; (YouTube)&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/tutorial_info.php?tutorials_id=158&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Talking Wireless Server Tutorial&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Components/General/speakjet-usermanual.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;SpeakJet User&amp;#39;s Guide&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Components/General/SpeakJet-dictionary.zip&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;SpeakJet Dictionary&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/commerce/tutorial_info.php?tutorials_id=166&quot; target=&quot;_blank&quot;&gt;Tutorial &lt;/a&gt;on adding the TTS256 text to speech IC to the shield&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;strong&gt;Replaces: &lt;/strong&gt;&lt;a href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9624&quot; target=&quot;_self&quot;&gt;DEV-09624&lt;/a&gt;&lt;/p&gt;</description>
<title>Arduino Voicebox Shield (Stephen Hawking in a box)</title>
<url>http://www.sparkfun.com/products/9799</url>
<tags>
<tag>Voice</tag>
<tag>Voicebox</tag>
<tag>Synthesizer</tag>
<tag>Speakjet</tag>
</tags>
<properties>
<property name='family'>Voice Shield</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/Arduino Voice Shield-v16_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/Arduino Voice Shield-v16_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/Arduino Voice Shield-v16_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/Arduino Voice Shield-v16_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector35' type='male' name='AUDIO'>
<description>AUDIO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector35pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector35pin' terminalId='connector35terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector35pad'/><p layer='copper1' svgId='connector35pad'/></pcbView>
</views>
</connector>
<connector id='connector36' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector36pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector36pin' terminalId='connector36terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector36pad'/><p layer='copper1' svgId='connector36pad'/></pcbView>
</views>
</connector>
<connector id='connector79' type='female' name='3.3V'>
<description>3.3V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector79pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector79pin' terminalId='connector79terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector79pad'/><p layer='copper1' svgId='connector79pad'/></pcbView>
</views>
</connector>
<connector id='connector80' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector80pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector80pin' terminalId='connector80terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector80pad'/><p layer='copper1' svgId='connector80pad'/></pcbView>
</views>
</connector>
<connector id='connector81' type='female' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector81pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector81pin' terminalId='connector81terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector81pad'/><p layer='copper1' svgId='connector81pad'/></pcbView>
</views>
</connector>
<connector id='connector82' type='female' name='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector82pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector82pin' terminalId='connector82terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector82pad'/><p layer='copper1' svgId='connector82pad'/></pcbView>
</views>
</connector>
<connector id='connector83' type='female' name='A2'>
<description>A2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector83pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector83pin' terminalId='connector83terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector83pad'/><p layer='copper1' svgId='connector83pad'/></pcbView>
</views>
</connector>
<connector id='connector84' type='female' name='A3'>
<description>A3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector84pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector84pin' terminalId='connector84terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector84pad'/><p layer='copper1' svgId='connector84pad'/></pcbView>
</views>
</connector>
<connector id='connector85' type='female' name='A4'>
<description>A4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector85pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector85pin' terminalId='connector85terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector85pad'/><p layer='copper1' svgId='connector85pad'/></pcbView>
</views>
</connector>
<connector id='connector86' type='female' name='A5'>
<description>A5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector86pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector86pin' terminalId='connector86terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector86pad'/><p layer='copper1' svgId='connector86pad'/></pcbView>
</views>
</connector>
<connector id='connector87' type='female' name='AREF'>
<description>AREF</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector87pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector87pin' terminalId='connector87terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector87pad'/><p layer='copper1' svgId='connector87pad'/></pcbView>
</views>
</connector>
<connector id='connector88' type='female' name='D-TX'>
<description>D-TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector88pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector88pin' terminalId='connector88terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector88pad'/><p layer='copper1' svgId='connector88pad'/></pcbView>
</views>
</connector>
<connector id='connector89' type='female' name='RST'>
<description>RST</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector89pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector89pin' terminalId='connector89terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector89pad'/><p layer='copper1' svgId='connector89pad'/></pcbView>
</views>
</connector>
<connector id='connector90' type='female' name='SPK'>
<description>SPK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector90pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector90pin' terminalId='connector90terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector90pad'/><p layer='copper1' svgId='connector90pad'/></pcbView>
</views>
</connector>
<connector id='connector91' type='female' name='E0'>
<description>E0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector91pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector91pin' terminalId='connector91terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector91pad'/><p layer='copper1' svgId='connector91pad'/></pcbView>
</views>
</connector>
<connector id='connector92' type='female' name='E1'>
<description>E1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector92pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector92pin' terminalId='connector92terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector92pad'/><p layer='copper1' svgId='connector92pad'/></pcbView>
</views>
</connector>
<connector id='connector93' type='female' name='E2'>
<description>E2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector93pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector93pin' terminalId='connector93terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector93pad'/><p layer='copper1' svgId='connector93pad'/></pcbView>
</views>
</connector>
<connector id='connector94' type='female' name='E3'>
<description>E3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector94pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector94pin' terminalId='connector94terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector94pad'/><p layer='copper1' svgId='connector94pad'/></pcbView>
</views>
</connector>
<connector id='connector95' type='female' name='E4'>
<description>E4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector95pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector95pin' terminalId='connector95terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector95pad'/><p layer='copper1' svgId='connector95pad'/></pcbView>
</views>
</connector>
<connector id='connector96' type='female' name='E5'>
<description>E5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector96pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector96pin' terminalId='connector96terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector96pad'/><p layer='copper1' svgId='connector96pad'/></pcbView>
</views>
</connector>
<connector id='connector97' type='female' name='E6'>
<description>E6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector97pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector97pin' terminalId='connector97terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector97pad'/><p layer='copper1' svgId='connector97pad'/></pcbView>
</views>
</connector>
<connector id='connector98' type='female' name='E7'>
<description>E7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector98pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector98pin' terminalId='connector98terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector98pad'/><p layer='copper1' svgId='connector98pad'/></pcbView>
</views>
</connector>
<connector id='connector99' type='female' name='RDY'>
<description>RDY</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector99pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector99pin' terminalId='connector99terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector99pad'/><p layer='copper1' svgId='connector99pad'/></pcbView>
</views>
</connector>
<connector id='connector100' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector100pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector100pin' terminalId='connector100terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector100pad'/><p layer='copper1' svgId='connector100pad'/></pcbView>
</views>
</connector>
<connector id='connector101' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector101pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector101pin' terminalId='connector101terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector101pad'/><p layer='copper1' svgId='connector101pad'/></pcbView>
</views>
</connector>
<connector id='connector102' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector102pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector102pin' terminalId='connector102terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector102pad'/><p layer='copper1' svgId='connector102pad'/></pcbView>
</views>
</connector>
<connector id='connector103' type='female' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector103pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector103pin' terminalId='connector103terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector103pad'/><p layer='copper1' svgId='connector103pad'/></pcbView>
</views>
</connector>
<connector id='connector104' type='female' name='RX'>
<description>RX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector104pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector104pin' terminalId='connector104terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector104pad'/><p layer='copper1' svgId='connector104pad'/></pcbView>
</views>
</connector>
<connector id='connector105' type='female' name='TX'>
<description>TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector105pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector105pin' terminalId='connector105terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector105pad'/><p layer='copper1' svgId='connector105pad'/></pcbView>
</views>
</connector>
<connector id='connector106' type='female' name='VIN'>
<description>VIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector106pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector106pin' terminalId='connector106terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector106pad'/><p layer='copper1' svgId='connector106pad'/></pcbView>
</views>
</connector>
<connector id='connector125' type='female' name='N$16'>
<description>N$16</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector125pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector125pin' terminalId='connector125terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector125pad' hybrid='yes' /><p layer='copper1' svgId='connector125pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector126' type='female' name='N$17'>
<description>N$17</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector126pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector126pin' terminalId='connector126terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector126pad' hybrid='yes' /><p layer='copper1' svgId='connector126pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector127' type='female' name='N$18'>
<description>N$18</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector127pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector127pin' terminalId='connector127terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector127pad' hybrid='yes' /><p layer='copper1' svgId='connector127pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector128' type='female' name='N$19'>
<description>N$19</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector128pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector128pin' terminalId='connector128terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector128pad' hybrid='yes' /><p layer='copper1' svgId='connector128pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector129' type='female' name='N$20'>
<description>N$20</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector129pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector129pin' terminalId='connector129terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector129pad' hybrid='yes' /><p layer='copper1' svgId='connector129pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector130' type='female' name='N$21'>
<description>N$21</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector130pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector130pin' terminalId='connector130terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector130pad' hybrid='yes' /><p layer='copper1' svgId='connector130pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector131' type='female' name='N$22'>
<description>N$22</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector131pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector131pin' terminalId='connector131terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector131pad' hybrid='yes' /><p layer='copper1' svgId='connector131pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector132' type='female' name='N$23'>
<description>N$23</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector132pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector132pin' terminalId='connector132terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector132pad' hybrid='yes' /><p layer='copper1' svgId='connector132pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector133' type='female' name='N$24'>
<description>N$24</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector133pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector133pin' terminalId='connector133terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector133pad' hybrid='yes' /><p layer='copper1' svgId='connector133pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector134' type='female' name='N$25'>
<description>N$25</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector134pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector134pin' terminalId='connector134terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector134pad' hybrid='yes' /><p layer='copper1' svgId='connector134pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector135' type='female' name='N$26'>
<description>N$26</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector135pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector135pin' terminalId='connector135terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector135pad' hybrid='yes' /><p layer='copper1' svgId='connector135pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector136' type='female' name='N$27'>
<description>N$27</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector136pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector136pin' terminalId='connector136terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector136pad' hybrid='yes' /><p layer='copper1' svgId='connector136pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector137' type='female' name='N$28'>
<description>N$28</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector137pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector137pin' terminalId='connector137terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector137pad' hybrid='yes' /><p layer='copper1' svgId='connector137pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector138' type='female' name='N$29'>
<description>N$29</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector138pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector138pin' terminalId='connector138terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector138pad' hybrid='yes' /><p layer='copper1' svgId='connector138pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector139' type='female' name='N$30'>
<description>N$30</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector139pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector139pin' terminalId='connector139terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector139pad' hybrid='yes' /><p layer='copper1' svgId='connector139pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector140' type='female' name='N$31'>
<description>N$31</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector140pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector140pin' terminalId='connector140terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector140pad' hybrid='yes' /><p layer='copper1' svgId='connector140pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector141' type='female' name='N$32'>
<description>N$32</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector141pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector141pin' terminalId='connector141terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector141pad' hybrid='yes' /><p layer='copper1' svgId='connector141pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector142' type='female' name='N$33'>
<description>N$33</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector142pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector142pin' terminalId='connector142terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector142pad' hybrid='yes' /><p layer='copper1' svgId='connector142pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector143' type='female' name='N$34'>
<description>N$34</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector143pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector143pin' terminalId='connector143terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector143pad' hybrid='yes' /><p layer='copper1' svgId='connector143pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector144' type='female' name='N$35'>
<description>N$35</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector144pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector144pin' terminalId='connector144terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector144pad' hybrid='yes' /><p layer='copper1' svgId='connector144pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector145' type='female' name='N$36'>
<description>N$36</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector145pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector145pin' terminalId='connector145terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector145pad' hybrid='yes' /><p layer='copper1' svgId='connector145pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector146' type='female' name='N$37'>
<description>N$37</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector146pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector146pin' terminalId='connector146terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector146pad' hybrid='yes' /><p layer='copper1' svgId='connector146pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector147' type='female' name='N$38'>
<description>N$38</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector147pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector147pin' terminalId='connector147terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector147pad' hybrid='yes' /><p layer='copper1' svgId='connector147pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector148' type='female' name='N$39'>
<description>N$39</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector148pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector148pin' terminalId='connector148terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector148pad' hybrid='yes' /><p layer='copper1' svgId='connector148pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector149' type='female' name='N$40'>
<description>N$40</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector149pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector149pin' terminalId='connector149terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector149pad' hybrid='yes' /><p layer='copper1' svgId='connector149pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector150' type='female' name='N$41'>
<description>N$41</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector150pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector150pin' terminalId='connector150terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector150pad' hybrid='yes' /><p layer='copper1' svgId='connector150pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector151' type='female' name='N$42'>
<description>N$42</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector151pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector151pin' terminalId='connector151terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector151pad' hybrid='yes' /><p layer='copper1' svgId='connector151pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector152' type='female' name='N$43'>
<description>N$43</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector152pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector152pin' terminalId='connector152terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector152pad' hybrid='yes' /><p layer='copper1' svgId='connector152pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector153' type='female' name='N$44'>
<description>N$44</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector153pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector153pin' terminalId='connector153terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector153pad' hybrid='yes' /><p layer='copper1' svgId='connector153pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector154' type='female' name='N$45'>
<description>N$45</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector154pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector154pin' terminalId='connector154terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector154pad' hybrid='yes' /><p layer='copper1' svgId='connector154pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector155' type='female' name='N$46'>
<description>N$46</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector155pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector155pin' terminalId='connector155terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector155pad' hybrid='yes' /><p layer='copper1' svgId='connector155pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector156' type='female' name='N$47'>
<description>N$47</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector156pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector156pin' terminalId='connector156terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector156pad' hybrid='yes' /><p layer='copper1' svgId='connector156pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector157' type='female' name='N$48'>
<description>N$48</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector157pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector157pin' terminalId='connector157terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector157pad' hybrid='yes' /><p layer='copper1' svgId='connector157pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector158' type='female' name='N$49'>
<description>N$49</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector158pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector158pin' terminalId='connector158terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector158pad' hybrid='yes' /><p layer='copper1' svgId='connector158pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector159' type='female' name='N$50'>
<description>N$50</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector159pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector159pin' terminalId='connector159terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector159pad' hybrid='yes' /><p layer='copper1' svgId='connector159pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector160' type='female' name='N$51'>
<description>N$51</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector160pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector160pin' terminalId='connector160terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector160pad' hybrid='yes' /><p layer='copper1' svgId='connector160pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector161' type='female' name='N$52'>
<description>N$52</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector161pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector161pin' terminalId='connector161terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector161pad' hybrid='yes' /><p layer='copper1' svgId='connector161pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector162' type='female' name='N$53'>
<description>N$53</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector162pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector162pin' terminalId='connector162terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector162pad' hybrid='yes' /><p layer='copper1' svgId='connector162pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector163' type='female' name='N$54'>
<description>N$54</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector163pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector163pin' terminalId='connector163terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector163pad' hybrid='yes' /><p layer='copper1' svgId='connector163pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector164' type='female' name='N$55'>
<description>N$55</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector164pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector164pin' terminalId='connector164terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector164pad' hybrid='yes' /><p layer='copper1' svgId='connector164pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector165' type='female' name='N$56'>
<description>N$56</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector165pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector165pin' terminalId='connector165terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector165pad' hybrid='yes' /><p layer='copper1' svgId='connector165pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector166' type='female' name='N$57'>
<description>N$57</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector166pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector166pin' terminalId='connector166terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector166pad' hybrid='yes' /><p layer='copper1' svgId='connector166pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector167' type='female' name='N$58'>
<description>N$58</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector167pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector167pin' terminalId='connector167terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector167pad' hybrid='yes' /><p layer='copper1' svgId='connector167pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector168' type='female' name='N$59'>
<description>N$59</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector168pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector168pin' terminalId='connector168terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector168pad' hybrid='yes' /><p layer='copper1' svgId='connector168pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector169' type='female' name='N$60'>
<description>N$60</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector169pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector169pin' terminalId='connector169terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector169pad' hybrid='yes' /><p layer='copper1' svgId='connector169pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector170' type='female' name='N$61'>
<description>N$61</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector170pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector170pin' terminalId='connector170terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector170pad' hybrid='yes' /><p layer='copper1' svgId='connector170pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector171' type='female' name='N$62'>
<description>N$62</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector171pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector171pin' terminalId='connector171terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector171pad' hybrid='yes' /><p layer='copper1' svgId='connector171pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector172' type='female' name='N$63'>
<description>N$63</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector172pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector172pin' terminalId='connector172terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector172pad' hybrid='yes' /><p layer='copper1' svgId='connector172pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector173' type='female' name='N$64'>
<description>N$64</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector173pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector173pin' terminalId='connector173terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector173pad' hybrid='yes' /><p layer='copper1' svgId='connector173pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector174' type='female' name='N$65'>
<description>N$65</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector174pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector174pin' terminalId='connector174terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector174pad' hybrid='yes' /><p layer='copper1' svgId='connector174pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector175' type='female' name='N$66'>
<description>N$66</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector175pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector175pin' terminalId='connector175terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector175pad' hybrid='yes' /><p layer='copper1' svgId='connector175pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector176' type='female' name='N$67'>
<description>N$67</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector176pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector176pin' terminalId='connector176terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector176pad' hybrid='yes' /><p layer='copper1' svgId='connector176pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector177' type='female' name='N$68'>
<description>N$68</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector177pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector177pin' terminalId='connector177terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector177pad' hybrid='yes' /><p layer='copper1' svgId='connector177pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector178' type='female' name='N$69'>
<description>N$69</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector178pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector178pin' terminalId='connector178terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector178pad' hybrid='yes' /><p layer='copper1' svgId='connector178pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector179' type='female' name='N$70'>
<description>N$70</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector179pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector179pin' terminalId='connector179terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector179pad' hybrid='yes' /><p layer='copper1' svgId='connector179pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector180' type='female' name='N$75'>
<description>N$75</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector180pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector180pin' terminalId='connector180terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector180pad' hybrid='yes' /><p layer='copper1' svgId='connector180pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector181' type='female' name='N$76'>
<description>N$76</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector181pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector181pin' terminalId='connector181terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector181pad' hybrid='yes' /><p layer='copper1' svgId='connector181pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector182' type='female' name='N$77'>
<description>N$77</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector182pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector182pin' terminalId='connector182terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector182pad' hybrid='yes' /><p layer='copper1' svgId='connector182pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector183' type='female' name='N$78'>
<description>N$78</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector183pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector183pin' terminalId='connector183terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector183pad' hybrid='yes' /><p layer='copper1' svgId='connector183pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector184' type='female' name='N$79'>
<description>N$79</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector184pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector184pin' terminalId='connector184terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector184pad' hybrid='yes' /><p layer='copper1' svgId='connector184pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector185' type='female' name='N$80'>
<description>N$80</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector185pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector185pin' terminalId='connector185terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector185pad' hybrid='yes' /><p layer='copper1' svgId='connector185pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector186' type='female' name='N$81'>
<description>N$81</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector186pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector186pin' terminalId='connector186terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector186pad' hybrid='yes' /><p layer='copper1' svgId='connector186pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector187' type='female' name='N$82'>
<description>N$82</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector187pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector187pin' terminalId='connector187terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector187pad' hybrid='yes' /><p layer='copper1' svgId='connector187pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector188' type='female' name='N$83'>
<description>N$83</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector188pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector188pin' terminalId='connector188terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector188pad' hybrid='yes' /><p layer='copper1' svgId='connector188pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector189' type='female' name='N$84'>
<description>N$84</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector189pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector189pin' terminalId='connector189terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector189pad' hybrid='yes' /><p layer='copper1' svgId='connector189pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector190' type='female' name='N$89'>
<description>N$89</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector190pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector190pin' terminalId='connector190terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector190pad' hybrid='yes' /><p layer='copper1' svgId='connector190pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector191' type='female' name='N$90'>
<description>N$90</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector191pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector191pin' terminalId='connector191terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector191pad' hybrid='yes' /><p layer='copper1' svgId='connector191pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector192' type='female' name='N$91'>
<description>N$91</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector192pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector192pin' terminalId='connector192terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector192pad' hybrid='yes' /><p layer='copper1' svgId='connector192pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector193' type='female' name='N$92'>
<description>N$92</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector193pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector193pin' terminalId='connector193terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector193pad' hybrid='yes' /><p layer='copper1' svgId='connector193pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector194' type='female' name='N$93'>
<description>N$93</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector194pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector194pin' terminalId='connector194terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector194pad' hybrid='yes' /><p layer='copper1' svgId='connector194pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector195' type='female' name='N$94'>
<description>N$94</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector195pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector195pin' terminalId='connector195terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector195pad' hybrid='yes' /><p layer='copper1' svgId='connector195pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector196' type='female' name='N$95'>
<description>N$95</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector196pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector196pin' terminalId='connector196terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector196pad' hybrid='yes' /><p layer='copper1' svgId='connector196pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector197' type='female' name='N$96'>
<description>N$96</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector197pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector197pin' terminalId='connector197terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector197pad' hybrid='yes' /><p layer='copper1' svgId='connector197pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector198' type='female' name='N$101'>
<description>N$101</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector198pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector198pin' terminalId='connector198terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector198pad' hybrid='yes' /><p layer='copper1' svgId='connector198pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector199' type='female' name='N$102'>
<description>N$102</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector199pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector199pin' terminalId='connector199terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector199pad' hybrid='yes' /><p layer='copper1' svgId='connector199pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector200' type='female' name='N$103'>
<description>N$103</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector200pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector200pin' terminalId='connector200terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector200pad' hybrid='yes' /><p layer='copper1' svgId='connector200pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector201' type='female' name='N$104'>
<description>N$104</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector201pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector201pin' terminalId='connector201terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector201pad' hybrid='yes' /><p layer='copper1' svgId='connector201pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector202' type='female' name='N$105'>
<description>N$105</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector202pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector202pin' terminalId='connector202terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector202pad' hybrid='yes' /><p layer='copper1' svgId='connector202pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector203' type='female' name='N$106'>
<description>N$106</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector203pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector203pin' terminalId='connector203terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector203pad' hybrid='yes' /><p layer='copper1' svgId='connector203pad' hybrid='yes' /></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector36'/>
<nodeMember connectorId='connector100'/>
<nodeMember connectorId='connector101'/>
<nodeMember connectorId='connector102'/>
</bus>
</buses>
</module>
