<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.1.1201" moduleId="1099ABDE24_ST-2leadbutton-horizon">
 <version replacedby="20A9BBEE34_ST-2leadbutton-horizon">1</version>
 <title>Pushbutton</title>
 <date>2008-09-16</date>
 <label>S</label>
 <tags>
  <tag>Pushbutton</tag>
  <tag>button</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="Default State">Normally Open</property>
  <property name="family">//obsolete//Switch - 2 pin</property>
  <property name="Switching Circuit">SPST</property>
 <property name="package">THT</property></properties>
 <taxonomy>discreteParts.switches.pushbutton</taxonomy>
 <description>A generic pushbutton.</description>
 <views>
  <iconView>
   <layers image="icon/basic_pbutton_2leg_horizon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/basic_pbutton_2leg_horizon.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
   <schematicView fliphorizontal="true" flipvertical="true">
   <layers image="schematic/pushbutton.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/axial_lay_300mil.svg">
     <layer layerId="copper0"/>
	<layer layerId="silkscreen"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="leg0" type="male">
   <description>leg</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" name="leg1" type="male">
   <description>leg</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pad"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>