<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='Arduino Nano3'>
<version replacedby='Arduino Nano3(fix)'>5</version>
<date>2013-04-11</date>
<author>Althaus</author>
<description>The Arduino Nano is a small, complete, and breadboard-friendly board based on the ATmega328 (Arduino Nano 3.0) or ATmega168 (Arduino Nano 2.x). It has more or less the same functionality of the Arduino Duemilanove, but in a different package. It lacks only a DC power jack, and works with a Mini-B USB cable instead of a standard one. The Nano was designed and is being produced by Gravitech.

</description>
<title>Arduino Nano (Rev3.0)</title>
<url>http://arduino.cc/en/Main/ArduinoBoardNano</url>
<tags>
<tag>Arduino Nano</tag>
<tag>ATmega328V</tag>
<tag>microcontrollerboard</tag>
</tags>
<properties>
<property name='family'>//obsolete//microcontroller board (arduino)</property>
<property name='type'>Arduino Nano (3.0)</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/Arduino Nano3_breadboard.svg'>
<layer layerId='breadboardbreadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/Arduino Nano3_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/Arduino Nano3_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/Arduino Nano3_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector55' type='male' name='D12/MISO' replacedby="connector30">
<description>D12/MISO</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector55pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector55pin' terminalId='connector55terminal'/></schematicView>
<pcbView>
<p layer='unknown' svgId='connector55pad'/></pcbView>
</views>
</connector>
<connector id='connector56' type='male' name='5V' replacedby="connector56">
<description>5V</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector56pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector56pin' terminalId='connector56terminal'/></schematicView>
<pcbView>
<p layer='unknown' svgId='connector56pad'/></pcbView>
</views>
</connector>
<connector id='connector57' type='male' name='D13/SCK' replacedby="connector45">
<description>D13/SCK</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector57pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector57pin' terminalId='connector57terminal'/></schematicView>
<pcbView>
<p layer='unknown' svgId='connector57pad'/></pcbView>
</views>
</connector>
<connector id='connector58' type='male' name='D11/MOSI' replacedby="connector58">
<description>D11/MOSI</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector58pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector58pin' terminalId='connector58terminal'/></schematicView>
<pcbView>
<p layer='unknown' svgId='connector58pad'/></pcbView>
</views>
</connector>
<connector id='connector59' type='male' name='RESET' replacedby="connector59">
<description>RESET</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector59pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector59pin' terminalId='connector59terminal'/></schematicView>
<pcbView>
<p layer='unknown' svgId='connector59pad'/></pcbView>
</views>
</connector>
<connector id='connector60' type='male' name='GND' replacedby="connector60">
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector60pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector60pin' terminalId='connector60terminal'/></schematicView>
<pcbView>
<p layer='unknown' svgId='connector60pad'/></pcbView>
</views>
</connector>
<connector id='connector16' type='male' name='D1/TX' replacedby="connector16">
<description>D1/TX</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector16pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector16pin' terminalId='connector16terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector16pad'/><p layer='copper1' svgId='connector16pad'/></pcbView>
</views>
</connector>
<connector id='connector17' type='male' name='D0/RX' replacedby="connector17">
<description>D0/RX</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector17pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector17pin' terminalId='connector17terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector17pad'/><p layer='copper1' svgId='connector17pad'/></pcbView>
</views>
</connector>
<connector id='connector18' type='male' name='RESET' replacedby="connector18">
<description>RESET</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector18pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector18pin' terminalId='connector18terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector18pad'/><p layer='copper1' svgId='connector18pad'/></pcbView>
</views>
</connector>
<connector id='connector19' type='male' name='GND' replacedby="connector19">
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector19pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector19pin' terminalId='connector19terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector19pad'/><p layer='copper1' svgId='connector19pad'/></pcbView>
</views>
</connector>
<connector id='connector20' type='male' name='D2' replacedby="connector20">
<description>D2</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector20pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector20pin' terminalId='connector20terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector20pad'/><p layer='copper1' svgId='connector20pad'/></pcbView>
</views>
</connector>
<connector id='connector21' type='male' name='D3' replacedby="connector21">
<description>D3</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector21pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector21pin' terminalId='connector21terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector21pad'/><p layer='copper1' svgId='connector21pad'/></pcbView>
</views>
</connector>
<connector id='connector22' type='male' name='D4' replacedby="connector22">
<description>D4</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector22pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector22pin' terminalId='connector22terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector22pad'/><p layer='copper1' svgId='connector22pad'/></pcbView>
</views>
</connector>
<connector id='connector23' type='male' name='D5' replacedby="connector23">
<description>D5</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector23pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector23pin' terminalId='connector23terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector23pad'/><p layer='copper1' svgId='connector23pad'/></pcbView>
</views>
</connector>
<connector id='connector24' type='male' name='D6' replacedby="connector24">
<description>D6</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector24pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector24pin' terminalId='connector24terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector24pad'/><p layer='copper1' svgId='connector24pad'/></pcbView>
</views>
</connector>
<connector id='connector25' type='male' name='D7' replacedby="connector25">
<description>D7</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector25pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector25pin' terminalId='connector25terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector25pad'/><p layer='copper1' svgId='connector25pad'/></pcbView>
</views>
</connector>
<connector id='connector26' type='male' name='D8' replacedby="connector26">
<description>D8</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector26pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector26pin' terminalId='connector26terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector26pad'/><p layer='copper1' svgId='connector26pad'/></pcbView>
</views>
</connector>
<connector id='connector27' type='male' name='D9' replacedby="connector27">
<description>D9</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector27pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector27pin' terminalId='connector27terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector27pad'/><p layer='copper1' svgId='connector27pad'/></pcbView>
</views>
</connector>
<connector id='connector28' type='male' name='D10' replacedby="connector28">
<description>D10</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector28pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector28pin' terminalId='connector28terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector28pad'/><p layer='copper1' svgId='connector28pad'/></pcbView>
</views>
</connector>
<connector id='connector29' type='male' name='D11/MOSI' replacedby="connector29">
<description>D11/MOSI</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector29pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector29pin' terminalId='connector29terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector29pad'/><p layer='copper1' svgId='connector29pad'/></pcbView>
</views>
</connector>
<connector id='connector30' type='male' name='D12/MISO' replacedby="connector30">
<description>D12/MISO</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector30pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector30pin' terminalId='connector30terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector30pad'/><p layer='copper1' svgId='connector30pad'/></pcbView>
</views>
</connector>
<connector id='connector31' type='male' name='VIN' replacedby="connector31">
<description>VIN</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector31pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector31pin' terminalId='connector31terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector31pad'/><p layer='copper1' svgId='connector31pad'/></pcbView>
</views>
</connector>
<connector id='connector32' type='male' name='GND' replacedby="connector32">
<description>GND</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector32pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector32pin' terminalId='connector32terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector32pad'/><p layer='copper1' svgId='connector32pad'/></pcbView>
</views>
</connector>
<connector id='connector33' type='male' name='RESET' replacedby="connector33">
<description>RESET</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector33pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector33pin' terminalId='connector33terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector33pad'/><p layer='copper1' svgId='connector33pad'/></pcbView>
</views>
</connector>
<connector id='connector34' type='male' name='5V' replacedby="connector34">
<description>5V</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector34pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector34pin' terminalId='connector34terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector34pad'/><p layer='copper1' svgId='connector34pad'/></pcbView>
</views>
</connector>
<connector id='connector35' type='male' name='A7' replacedby="connector35">
<description>A7</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector35pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector35pin' terminalId='connector35terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector35pad'/><p layer='copper1' svgId='connector35pad'/></pcbView>
</views>
</connector>
<connector id='connector36' type='male' name='A6' replacedby="connector36">
<description>A6</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector36pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector36pin' terminalId='connector36terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector36pad'/><p layer='copper1' svgId='connector36pad'/></pcbView>
</views>
</connector>
<connector id='connector37' type='male' name='A5' replacedby="connector37">
<description>A5</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector37pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector37pin' terminalId='connector37terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector37pad'/><p layer='copper1' svgId='connector37pad'/></pcbView>
</views>
</connector>
<connector id='connector38' type='male' name='A4' replacedby="connector38">
<description>A4</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector38pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector38pin' terminalId='connector38terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector38pad'/><p layer='copper1' svgId='connector38pad'/></pcbView>
</views>
</connector>
<connector id='connector39' type='male' name='A3' replacedby="connector39">
<description>A3</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector39pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector39pin' terminalId='connector39terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector39pad'/><p layer='copper1' svgId='connector39pad'/></pcbView>
</views>
</connector>
<connector id='connector40' type='male' name='A2' replacedby="connector40">
<description>A2</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector40pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector40pin' terminalId='connector40terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector40pad'/><p layer='copper1' svgId='connector40pad'/></pcbView>
</views>
</connector>
<connector id='connector41' type='male' name='A1' replacedby="connector41">
<description>A1</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector41pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector41pin' terminalId='connector41terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector41pad'/><p layer='copper1' svgId='connector41pad'/></pcbView>
</views>
</connector>
<connector id='connector42' type='male' name='A0' replacedby="connector42">
<description>A0</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector42pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector42pin' terminalId='connector42terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector42pad'/><p layer='copper1' svgId='connector42pad'/></pcbView>
</views>
</connector>
<connector id='connector43' type='male' name='AREF' replacedby="connector43">
<description>AREF</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector43pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector43pin' terminalId='connector43terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector43pad'/><p layer='copper1' svgId='connector43pad'/></pcbView>
</views>
</connector>
<connector id='connector44' type='male' name='3V3' replacedby="connector44">
<description>3V3</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector44pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector44pin' terminalId='connector44terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector44pad'/><p layer='copper1' svgId='connector44pad'/></pcbView>
</views>
</connector>
<connector id='connector45' type='male' name='D13/SCK' replacedby="connector45">
<description>D13/SCK</description><views>
<breadboardView>
<p layer='breadboardbreadboard' svgId='connector45pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector45pin' terminalId='connector45terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector45pad'/><p layer='copper1' svgId='connector45pad'/></pcbView>
</views>
</connector>

</connectors>
<buses>
<bus id='com'>
<nodeMember connectorId='connector19'/>
<nodeMember connectorId='connector32'/>
<nodeMember connectorId='connector60'/>
</bus>
<bus id='reset'>
<nodeMember connectorId='connector18'/>
<nodeMember connectorId='connector33'/>
<nodeMember connectorId='connector59'/>
</bus>
<bus id='d12/miso'>
<nodeMember connectorId='connector30'/>
<nodeMember connectorId='connector55'/>
</bus>
<bus id='+5v'>
<nodeMember connectorId='connector34'/>
<nodeMember connectorId='connector56'/>
</bus>
<bus id='d13/sck'>
<nodeMember connectorId='connector45'/>
<nodeMember connectorId='connector57'/>
</bus>
<bus id='d11/mosi'>
<nodeMember connectorId='connector29'/>
<nodeMember connectorId='connector58'/>
</bus>
</buses>
</module>
