<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="usb_3.0_female_fix" fritzingVersion="0.9.3b">
 <!-- generated from Sparkfun Eagle Library 'SparkFun-Connectors' USB -A-SMD -->
 <version>5</version>
 <date>Fri Oct 23 2015</date>
 <label>X</label>
 <author>www.fritzing.org, f.althaus</author>
 <description>&lt;b>USB Connectors&lt;/b>&#xd;
&lt;p>USB-B-PTH is fully proven SKU : PRT-00139&#xd;
&lt;p>USB-miniB is fully proven SKU : PRT-00587&#xd;
&lt;p>USB-A-PCB is untested.&#xd;
&lt;p>USB-A-H is throughly reviewed, but untested. Spark Fun Electronics SKU : PRT-00437&#xd;
&lt;p>USB-B-SMT is throughly reviewed, but untested. Needs silkscreen touching up.&#xd;
&lt;p>USB-A-S has not been used/tested&#xd;
&lt;p>USB-MB-H has not been used/tested</description>
 <title>USB Connectors</title>
 <tags>
  <tag>USB</tag>
  <tag>USB-A-S-NOSILK-FEMALE</tag>
  <tag>-A-SMD</tag>
 </tags>
 <properties>
  <property name="package">usb3 - female</property>
  <property name="target"></property>
  <property name="family">sparkfun usb connector</property>
  <property name="variant">usb3 female</property>
  <property name="layer"/>
  <property name="part number"/>
 </properties>
 <views>
  <breadboardView>
   <layers image="breadboard/usb_3.0_female_fix_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/usb_3.0_female_fix_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/usb_3.0_female_fix_pcb.svg">
    <layer layerId="copper1"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
   </layers>
  </pcbView>
  <iconView>
   <layers image="icon/usb_3.0_female_fix_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
 </views>
 <connectors>
  <connector id="connector2" type="male" name="D+">
   <description>D+</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" terminalId="connector3terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pad" layer="copper0"/>
     <p svgId="connector2pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector3" type="male" name="D-">
   <description>D-</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" terminalId="connector2terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pad" layer="copper0"/>
     <p svgId="connector3pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector4" type="male" name="GND">
   <description>GND</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" terminalId="connector5terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pad" layer="copper0"/>
     <p svgId="connector4pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector5" type="male" name="VBUS">
   <description>VBUS</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" terminalId="connector4terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pad" layer="copper0"/>
     <p svgId="connector5pad" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector6" type="male" name="SSRX-">
   <description>pin 6</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper0"/>
     <p svgId="connector6pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector7" type="male" name="GND_DRAIN">
   <description>pin 7</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper0"/>
     <p svgId="connector7pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector8" type="male" name="SSRX+">
   <description>pin 8</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper0"/>
     <p svgId="connector8pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector9" type="male" name="SSTX-">
   <description>pin 9</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper0"/>
     <p svgId="connector9pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector10" type="male" name="SSTX+">
   <description>pin 10</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper0"/>
     <p svgId="connector10pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector11" type="male" name="NC">
   <description>pin 11</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper0"/>
     <p svgId="connector11pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector12" type="male" name="NC">
   <description>pin 12</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper0"/>
     <p svgId="connector12pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses/>
</module>
