<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.1.1255" moduleId="TMP36_THT">
 <version>4</version>
 <author>Jonathan Cohen</author>
 <title>TMP36 Temperature Sensor</title>
 <label>T</label>
 <date>2011-08-08</date>
 <tags>
  <tag>NPN</tag>
  <tag>temperature</tag>
  <tag>sensor</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="package">TO92 [THT]</property>
  <property name="type">solid state</property>
  <property name="family">temperature sensor</property>
  <property name="variant">TMP36</property>
 </properties>
 <description>A TMP36 temperature sensor with a range from -40°C to 150°C.</description>
 <views>
  <iconView>
   <layers image="icon/tmp36icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/tmp36.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView fliphorizontal="true" flipvertical="true">
   <layers image="schematic/tmp36_schem.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/TO92_3_100mil_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
   <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="+Vs" type="male">
   <description>input voltage</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin"  legId="connector0leg"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector2pin"/>
    <p layer="copper1" svgId="connector2pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" name="Vout" type="male">
   <description>output voltage</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin"  legId="connector1leg"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pin"/>
    <p layer="copper1" svgId="connector1pin"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" name="GND" type="male">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector2pin" legId="connector2leg"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pin"/>
    <p layer="copper1" svgId="connector0pin"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>
