<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.4.1b.07.17.4356" moduleId="atlas-sientific_ENV-32X" referenceFile="atlas-sientific_ENV-32X.fzp">
 <author>Atlas Scientific </author>
 <title>ENV-32X Flash Memory Data Logger</title>
 <label>ENV-32X Flash Memory Data Logger</label>
 <date>Thu Jul 18 2013</date>
 <tags/>
 <properties>
  <property name="family">Memory</property>
  <property name="variant">V1</property>
  <property name="layer"></property>
  <property name="part number"></property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">As computer power increases with each passing year, so too, does computer memory. Now, 32 gigabytes of flash memory so cheap, it's disposable. However, for the embedded systems engineer 32 gigabytes of flash memory is simply useless over kill. An 8 bit computer system is simply not designed to efficiently manage 32,000,000,000 bytes of memory.&lt;/span>&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-size:8pt;">&lt;br />&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">Atlas Scientific has designed a memory system specifically designed to hold small strings of data no larger than 128 bytes long, a perfect size for holding sensor data. The ENV-32X Embedded Data Logger has been designed, like all other Atlas Scientific products, to be easy to use and easy to implement. The ENV-32X Embedded Data Logger requires no additional hardware and no drivers to operate. Simply output the string to be stored and the ENV-32X Embedded Data Logger takes care of the rest.&lt;/span>&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-size:8pt;">&lt;br />&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• 32Mb flash memory&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• No drivers required&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Specifically designed to hold strings of up to 128 characters long&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Read/ Write/Erase 32,760 individual strings&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Fast operation read/write a 128 byte string in just 3ms&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Write to memory confirmation&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Two different organized read back methods&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• 20 year data retention&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Up to 3,276,000,000 program/erase cycles&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Simple asynchronous serial connectivity (voltage swing 0-VCC)&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Simple instruction set consisting of only 7 commands&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Debugging LED's&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• 3.3 volt operation&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Low power consumption&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Well suited for airborne applications weighing only 1.53 grams&lt;/span>&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/atlas-sientific_ENV-32X_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <schematicView>
   <layers image="schematic/atlas-sientific_ENV-32X_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <breadboardView>
   <layers image="breadboard/atlas-sientific_ENV-32X_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <pcbView>
   <layers image="pcb/atlas-sientific_ENV-32X_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="male" id="connector0" name="TX">
   <description>Data Out</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper1"/>
     <p svgId="connector0pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector1" name="RX">
   <description>Data In</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper1"/>
     <p svgId="connector1pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector2" name="Vcc">
   <description>Supply Voltage</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper1"/>
     <p svgId="connector2pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector3" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper1"/>
     <p svgId="connector3pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <url>https://www.atlas-scientific.com/product_pages/embedded/env-32x.html</url>
</module>
