<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="Dagu_DGServo_9g_Pan_and_tilt" referenceFile="servo.fzp" fritzingVersion="0.12.34">
 <version>4</version>
 <author>Stephen Parry</author>
 <title>Dagu DGServo 9g (Pan and tilt)</title>
 <label>M</label>
 <date>Mon Jun 6 2016</date>
 <tags>
  <tag>Dagu</tag>
  <tag>servo</tag>
 </tags>
 <properties>
  <property name="variant">- Top view with turning circle for pan and tilt</property>
  <property name="family">Dagu DGServo 9g</property>
  <property name="view">top</property>
  <property name="part number">RS001B</property>
  <property name="layer"></property>
  <property name="turning circle">yes</property>
 </properties>
 <taxonomy>discreteParts.servo</taxonomy>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'Oxygen-Sans'; font-size:10pt;">Dagu DGServo 9g (Pan and tilt)&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">The breadboard view is rendered as non-perspective top projection for layout on stripboard or similar.&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">The inner circle indicates the turning circle of the base of the pan and tilt frame at about 16mm above board level if you fully recess the motor, 33mm if not.&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">The outer circle indicates the turning circle of the tilt part of the frame when at its greatest extent (41mm) at about 50mm if recessed, 67mm if not.&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">Further allowances will need to be made for any electronics mounted to the tilt frame.&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">The female header connector normally attached to end of the servo wires, exists in Fritzing as a separate part in the Dagu bin. Simply plug the connector onto whichever header pins you are using, then attach the wires to the connector.&lt;/span>&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;br />&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/Dagu_DGServo_9g_Pan_and_tilt_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/Dagu_DGServo_9g_Pan_and_tilt_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/Dagu_DGServo_9g_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/Dagu_DGServo_9g_pcb.svg">
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="gnd" type="male">
   <description>ground</description>
   <views>
    <breadboardView>
     <p legId="connector0leg" svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector0terminal" svgId="connector0pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" name="vcc" type="male">
   <description>vcc</description>
   <views>
    <breadboardView>
     <p legId="connector1leg" svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector1terminal" svgId="connector1pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" name="pulse" type="male">
   <description>pulse</description>
   <views>
    <breadboardView>
     <p legId="connector2leg" svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p terminalId="connector2terminal" svgId="connector2pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>
