<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.7.1b.03.10.5908" moduleId="PCF8574">
    <version replacedby='PCF8574A_f92705dc5bbcb278fb8f55ff08c7872a_1'>4</version>
    <author>D&amp;C</author>
    <title>PCF8574</title>
    <label>U</label>
    <date>2012-04-07</date>
    <tags>
        <tag>DIP</tag>
        <tag>I2C</tag>
        <tag>Expander Port</tag>
    </tags>
    <properties>
        <property name="package">DIP16 [THT]</property>
        <property name="family">PCF8574</property>
        <property name="type">PCF8574</property>
        <property name="part number"></property>
    </properties>
    <description>8-bit parallel-load shift registers</description>
    <views>
        <pcbView>
            <layers image="pcb/dip_16_300mil_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
        <iconView>
            <layers image="icon/PCF8574.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/PCF8574.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/PCF8574.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
    </views>
    <connectors>
        <connector id="connector15" type="male" name="VCC">
            <description>Positive supply voltage</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin" terminalId="connector15terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector15pin"/>
                    <p layer="copper0" svgId="connector15pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" type="male" name="P0">
            <description>Output pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pin"/>
                    <p layer="copper0" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" type="male" name="P1">
            <description>Output pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pin"/>
                    <p layer="copper0" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" type="male" name="P2">
            <description>Output pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" terminalId="connector5terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector5pin"/>
                    <p layer="copper0" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" type="male" name="P3">
            <description>Output pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin" terminalId="connector6terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector6pin"/>
                    <p layer="copper0" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" type="male" name="GND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin" terminalId="connector7terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector7pin"/>
                    <p layer="copper0" svgId="connector7pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" type="male" name="P4">
            <description>Output pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin" terminalId="connector8terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector8pin"/>
                    <p layer="copper0" svgId="connector8pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" type="male" name="P5">
            <description>Output pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin" terminalId="connector9terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector9pin"/>
                    <p layer="copper0" svgId="connector9pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" type="male" name="P6">
            <description>Output pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin" terminalId="connector10terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector10pin"/>
                    <p layer="copper0" svgId="connector10pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" type="male" name="P7">
            <description>Output pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin" terminalId="connector11terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector11pin"/>
                    <p layer="copper0" svgId="connector11pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector12" type="male" name="INT">
            <description>Interrupt pin, (active low)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin" terminalId="connector12terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector12pin"/>
                    <p layer="copper0" svgId="connector12pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" type="male" name="A0">
            <description>Address pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin"/>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="A1">
            <description>Address pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector13" type="male" name="SCL">
            <description>Serial Clock pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin" terminalId="connector13terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector13pin"/>
                    <p layer="copper0" svgId="connector13pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector14" type="male" name="SDA">
            <description>Serial Data pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin" terminalId="connector14terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector14pin"/>
                    <p layer="copper0" svgId="connector14pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="male" name="A3">
            <description>Output Pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pin"/>
                    <p layer="copper0" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
