<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.4.1b.07.17.4356" moduleId="ESP8266_module_antenna">
<version>2</version>
 <author>YDonnelly fixed f.althaus</author>
 <title>ESP8266 WiFi Module</title>
 <label>U</label>
 <date>Apr 18 2017</date>
 <tags>
  <tag>ESP201</tag>
  <tag>ESP8266</tag>
  <tag>breakout</tag>
  <tag>radio</tag>
  <tag>wifi</tag>
  <tag>module</tag>
 </tags>
 <properties>
  <property name="family">ESP8266</property>
  <property name="variant">variant 201</property>
  <property name="layer"></property>
  <property name="part number">ESP8266</property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'Ubuntu'; font-size:11pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">Generic WiFi Module based on the ESP8266 with onboard PCB antenna and UART communications&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/ESP8266_module_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <schematicView>
   <layers image="schematic/ESP8266_module_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <breadboardView>
   <layers image="breadboard/ESP8266_module_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <pcbView>
   <layers image="pcb/ESP8266_module_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="male" id="connector1" name="IO0">
   <description>General-Purpose IO 0 (Active-low flash enable; pull high)</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper1"/>
     <p svgId="connector1pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector2" name="IO2">
   <description>General-Purpose IO 2</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper1"/>
     <p svgId="connector2pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector3" name="D2">
   <description>Data line 2</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper1"/>
     <p svgId="connector3pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector4" name="CLK">
   <description>Data clock</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper1"/>
     <p svgId="connector4pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector5" name="CMD">
   <description>Data command</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper1"/>
     <p svgId="connector5pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector6" name="D0">
   <description>Data line 0</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper1"/>
     <p svgId="connector6pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector7" name="D1">
   <description>Data line 1</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper1"/>
     <p svgId="connector7pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector8" name="D3">
   <description>Data line 3</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper1"/>
     <p svgId="connector8pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector9" name="IO4">
   <description>General-Purpose IO 4</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper1"/>
     <p svgId="connector9pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector10" name="3.3V">
   <description>+3.3V Supply</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper1"/>
     <p svgId="connector10pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector11" name="3.3V">
   <description>+3.3V Supply</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper1"/>
     <p svgId="connector11pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector12" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper1"/>
     <p svgId="connector12pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector13" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pin" layer="copper1"/>
     <p svgId="connector13pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector14" name="IO5">
   <description>General-Purpose IO 5</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" layer="schematic" terminalId="connector14terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pin" layer="copper1"/>
     <p svgId="connector14pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector15" name="T_OUT">
   <description>Analog-Digital Converter</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" layer="schematic" terminalId="connector15terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pin" layer="copper1"/>
     <p svgId="connector15pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector16" name="RST">
   <description>Active-low reset</description>
   <views>
    <breadboardView>
     <p svgId="connector16pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector16pin" layer="schematic" terminalId="connector16terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector16pin" layer="copper1"/>
     <p svgId="connector16pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector17" name="CHIP_EN">
   <description>Chip enable</description>
   <views>
    <breadboardView>
     <p svgId="connector17pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector17pin" layer="schematic" terminalId="connector17terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector17pin" layer="copper1"/>
     <p svgId="connector17pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector18" name="XPD">
   <description>Deep-sleep wakeup</description>
   <views>
    <breadboardView>
     <p svgId="connector18pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector18pin" layer="schematic" terminalId="connector18terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector18pin" layer="copper1"/>
     <p svgId="connector18pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector19" name="IO14">
   <description>General-Purpose IO 14</description>
   <views>
    <breadboardView>
     <p svgId="connector19pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector19pin" layer="schematic" terminalId="connector19terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector19pin" layer="copper1"/>
     <p svgId="connector19pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector20" name="IO12">
   <description>General-Purpose IO 12</description>
   <views>
    <breadboardView>
     <p svgId="connector20pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector20pin" layer="schematic" terminalId="connector20terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector20pin" layer="copper1"/>
     <p svgId="connector20pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector21" name="IO13">
   <description>General-Purpose IO 13</description>
   <views>
    <breadboardView>
     <p svgId="connector21pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector21pin" layer="schematic" terminalId="connector21terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector21pin" layer="copper1"/>
     <p svgId="connector21pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector22" name="IO15">
   <description>General-Purpose IO 15 (Pull high)</description>
   <views>
    <breadboardView>
     <p svgId="connector22pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector22pin" layer="schematic" terminalId="connector22terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector22pin" layer="copper1"/>
     <p svgId="connector22pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector23" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector23pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector23pin" layer="schematic" terminalId="connector23terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector23pin" layer="copper1"/>
     <p svgId="connector23pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector24" name="TX">
   <description>UART Transmit</description>
   <views>
    <breadboardView>
     <p svgId="connector24pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector24pin" layer="schematic" terminalId="connector24terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector24pin" layer="copper1"/>
     <p svgId="connector24pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector25" name="RX">
   <description>UART Receive</description>
   <views>
    <breadboardView>
     <p svgId="connector25pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector25pin" layer="schematic" terminalId="connector25terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector25pin" layer="copper1"/>
     <p svgId="connector25pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector26" name="3.3V">
   <description>+3.3V Supply</description>
   <views>
    <breadboardView>
     <p svgId="connector26pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector26pin" layer="schematic" terminalId="connector26terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector26pin" layer="copper1"/>
     <p svgId="connector26pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <url>http://www.esp8266.com</url>
</module>
