<?xml version='1.0' encoding='UTF-8'?>
<module moduleId="LDH-45-350B" fritzingVersion="0.12.34">
 <version>4</version>
 <author>F.Althaus</author>
 <title>LDH-45-350B</title>
 <label>LDH-45-350B</label>
 <date>Mi Nov 15 2017</date>
 <tags>
  <tag>LED Driver</tag>
  <tag>LDH-45-350B</tag>
  <tag>Mean Well</tag>
 </tags>
 <properties>
  <property name="family">LED Driver</property>
  <property name="package">THT</property>
  <property name="pins">7</property>
  <property name="chip label">LDH-45B-350</property>
  <property name="part number"></property>
 </properties>
 <description>DC-DC Stepup Converter</description>
 <views>
  <iconView>
   <layers image="icon/LDH-45-350B_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/LDH-45-350B_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/LDH-45-350B_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/LDH-45-350B_pcb.svg">
    <layer layerId="silkscreen"/>
    <layer layerId="copper0"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector name="Vin+" type="male" id="connector0">
   <description>pin 1</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" terminalId="connector0terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" terminalId="connector0terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector name="Vin-" type="male" id="connector1">
   <description>pin 2</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" terminalId="connector1terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" terminalId="connector1terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector name="DIM-" type="male" id="connector2">
   <description>pin 3</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" terminalId="connector2terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" terminalId="connector2terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector name="Analog DIM" type="male" id="connector3">
   <description>pin 4</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" terminalId="connector3terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" terminalId="connector3terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper0"/>
     <p svgId="connector3pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector name="PWM DIM" type="male" id="connector4">
   <description>pin 5</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" terminalId="connector4terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" terminalId="connector4terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper0"/>
     <p svgId="connector4pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector name="Vout-" type="male" id="connector5">
   <description>pin 6</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" terminalId="connector5terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" terminalId="connector5terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper0"/>
     <p svgId="connector5pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector name="Vout+" type="male" id="connector6">
   <description>pin 7</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" terminalId="connector6terminal" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" terminalId="connector6terminal" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper0"/>
     <p svgId="connector6pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  </connectors>
</module>
