<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.4.1b.07.17.4356" moduleId="fa3e296736059e8c25d88ac262af999a">
    <version>4</version>
    <author>tigoe</author>
    <title>Basic Flex Resistor</title>
    <label>R</label>
    <date>2010-07-17</date>
    <tags>
       <tag>FSR</tag>
       <tag>Felx Sensor</tag>
       <tag>force sensitive resistor</tag>
      <tag>user part</tag>
       <tag>fritzing core</tag>
  </tags>
    <properties>
        <property name="family">FSR</property>
        <property name="Sensing Area Diameter">6 &quot;</property>
    </properties>
    <description>A generic Flex resistor</description>
    <views>
        <breadboardView>
            <layers image="breadboard/Basic_Force_Sensing_Resistor_(FSR)__a4ff.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/basic_fsr.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/jumper_2_100mil_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
        <iconView>
            <layers image="icon/Basic_Force_Sensing_Resistor_(FSR)__a4ff.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
    </views>
    <connectors>
        <connector id="connector0" name="Pin 2" type="male">
            <description>Pin 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                    <p layer="copper1" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" name="pin 1" type="male">
            <description>Pin 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>