<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='PWM-Shield-v12'>
<version>4</version>
<date>2011-11-29</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;strong&gt;Description:&lt;/strong&gt; This is the Arduino shield version of our TLC5940 Breakout. The PWM Shield will allow you to generate up to 16 PWM signals from your Arduino by utilizing the power of the TLC5940 IC. All 16 PWM channels are broken out to standard 0.1&amp;quot; headers, which run alongside convenient voltage and ground rails. Because the IC can be daisy-chained, output headers are broken out on one side of the shield and can be connected to our TLC5940 Breakout to further expand your PWM capabilities.&amp;nbsp;&lt;/p&gt;


&lt;p&gt;


	Use this board to increase the number of PWM pins available to your microcontroller for applications such as monocolor, multicolor or full-color LED displays, LED signboards, display backlighting, servo control, or any other project where a large number of PWM drivers are necessary.&lt;/p&gt;


&lt;p&gt;


	&lt;strong&gt;Note: &lt;/strong&gt;While each 3-pin PWM header is 0.1&amp;quot; spaced, the space between each header is slightly larger in order to accommodate servo connections. In order to make this board suitable for use with servos, 2.2k pull-up resistors have been included on each output as well. Finally, the 2.2k resistor on the Iref pin sets the output current to 17.8mA but a parallel through-hole connection is provided for an additional resistor to increase the current if necessary. To determine the resistor value you need for a given output check the equations provided on the schematic below.&lt;/p&gt;


&lt;p&gt;


	&lt;strong&gt;Documents:&lt;/strong&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Dev/Arduino/Shields/PWM-Shield-v12.pdf&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Dev/Arduino/Shields/PWM-Shield-v12.zip&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/datasheets/Components/General/tlc5940.pdf&quot; target=&quot;_blank&quot;&gt;Datasheet&lt;/a&gt; (TLC5940)&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://code.google.com/p/tlc5940arduino/&quot; target=&quot;_blank&quot;&gt;Arduino Library&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.arduino.cc/playground/Learning/TLC5940&quot; target=&quot;_blank&quot;&gt;Arduino Example&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;</description>
<title>PWM Shield</title>
<url>http://www.sparkfun.com/products/10615</url>
<tags>
<tag>PWM</tag>
<tag>Shield</tag>
<tag>Pulse Width Modulation</tag>
<tag>Analog Write</tag>
</tags>
<properties>
<property name='Steps'>4096</property>
<property name='family'>PWM</property>
<property name='Max LED Supply Voltage'>17V</property>
<property name='Channels'>16</property>
<property name='Operating Voltage'>3V-5.5V</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/PWM-Shield-v12_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/PWM-Shield-v12_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/PWM-Shield-v12_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/PWM-Shield-v12_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector6' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector6pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector6pin' terminalId='connector6terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector6pad'/><p layer='copper1' svgId='connector6pad'/></pcbView>
</views>
</connector>
<connector id='connector7' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector7pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector7pin' terminalId='connector7terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector7pad'/><p layer='copper1' svgId='connector7pad'/></pcbView>
</views>
</connector>
<connector id='connector8' type='female' name='OUT9'>
<description>OUT9</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector8pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector8pin' terminalId='connector8terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector8pad'/><p layer='copper1' svgId='connector8pad'/></pcbView>
</views>
</connector>
<connector id='connector9' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector9pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector9pin' terminalId='connector9terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector9pad'/><p layer='copper1' svgId='connector9pad'/></pcbView>
</views>
</connector>
<connector id='connector10' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector10pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector10pin' terminalId='connector10terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector10pad'/><p layer='copper1' svgId='connector10pad'/></pcbView>
</views>
</connector>
<connector id='connector11' type='female' name='OUT0'>
<description>OUT0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector11pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector11pin' terminalId='connector11terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector11pad'/><p layer='copper1' svgId='connector11pad'/></pcbView>
</views>
</connector>
<connector id='connector12' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector12pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector12pin' terminalId='connector12terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector12pad'/><p layer='copper1' svgId='connector12pad'/></pcbView>
</views>
</connector>
<connector id='connector13' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector13pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector13pin' terminalId='connector13terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector13pad'/><p layer='copper1' svgId='connector13pad'/></pcbView>
</views>
</connector>
<connector id='connector14' type='female' name='OUT1'>
<description>OUT1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector14pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector14pin' terminalId='connector14terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector14pad'/><p layer='copper1' svgId='connector14pad'/></pcbView>
</views>
</connector>
<connector id='connector15' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector15pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector15pin' terminalId='connector15terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector15pad'/><p layer='copper1' svgId='connector15pad'/></pcbView>
</views>
</connector>
<connector id='connector16' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector16pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector16pin' terminalId='connector16terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector16pad'/><p layer='copper1' svgId='connector16pad'/></pcbView>
</views>
</connector>
<connector id='connector17' type='female' name='OUT2'>
<description>OUT2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector17pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector17pin' terminalId='connector17terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector17pad'/><p layer='copper1' svgId='connector17pad'/></pcbView>
</views>
</connector>
<connector id='connector18' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector18pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector18pin' terminalId='connector18terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector18pad'/><p layer='copper1' svgId='connector18pad'/></pcbView>
</views>
</connector>
<connector id='connector19' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector19pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector19pin' terminalId='connector19terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector19pad'/><p layer='copper1' svgId='connector19pad'/></pcbView>
</views>
</connector>
<connector id='connector20' type='female' name='OUT3'>
<description>OUT3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector20pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector20pin' terminalId='connector20terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector20pad'/><p layer='copper1' svgId='connector20pad'/></pcbView>
</views>
</connector>
<connector id='connector21' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector21pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector21pin' terminalId='connector21terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector21pad'/><p layer='copper1' svgId='connector21pad'/></pcbView>
</views>
</connector>
<connector id='connector22' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector22pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector22pin' terminalId='connector22terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector22pad'/><p layer='copper1' svgId='connector22pad'/></pcbView>
</views>
</connector>
<connector id='connector23' type='female' name='OUT4'>
<description>OUT4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector23pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector23pin' terminalId='connector23terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector23pad'/><p layer='copper1' svgId='connector23pad'/></pcbView>
</views>
</connector>
<connector id='connector24' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector24pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector24pin' terminalId='connector24terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector24pad'/><p layer='copper1' svgId='connector24pad'/></pcbView>
</views>
</connector>
<connector id='connector25' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector25pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector25pin' terminalId='connector25terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector25pad'/><p layer='copper1' svgId='connector25pad'/></pcbView>
</views>
</connector>
<connector id='connector26' type='female' name='OUT5'>
<description>OUT5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector26pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector26pin' terminalId='connector26terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector26pad'/><p layer='copper1' svgId='connector26pad'/></pcbView>
</views>
</connector>
<connector id='connector27' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector27pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector27pin' terminalId='connector27terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector27pad'/><p layer='copper1' svgId='connector27pad'/></pcbView>
</views>
</connector>
<connector id='connector28' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector28pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector28pin' terminalId='connector28terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector28pad'/><p layer='copper1' svgId='connector28pad'/></pcbView>
</views>
</connector>
<connector id='connector29' type='female' name='OUT6'>
<description>OUT6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector29pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector29pin' terminalId='connector29terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector29pad'/><p layer='copper1' svgId='connector29pad'/></pcbView>
</views>
</connector>
<connector id='connector30' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector30pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector30pin' terminalId='connector30terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector30pad'/><p layer='copper1' svgId='connector30pad'/></pcbView>
</views>
</connector>
<connector id='connector31' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector31pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector31pin' terminalId='connector31terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector31pad'/><p layer='copper1' svgId='connector31pad'/></pcbView>
</views>
</connector>
<connector id='connector32' type='female' name='OUT7'>
<description>OUT7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector32pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector32pin' terminalId='connector32terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector32pad'/><p layer='copper1' svgId='connector32pad'/></pcbView>
</views>
</connector>
<connector id='connector33' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector33pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector33pin' terminalId='connector33terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector33pad'/><p layer='copper1' svgId='connector33pad'/></pcbView>
</views>
</connector>
<connector id='connector34' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector34pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector34pin' terminalId='connector34terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector34pad'/><p layer='copper1' svgId='connector34pad'/></pcbView>
</views>
</connector>
<connector id='connector35' type='female' name='OUT8'>
<description>OUT8</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector35pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector35pin' terminalId='connector35terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector35pad'/><p layer='copper1' svgId='connector35pad'/></pcbView>
</views>
</connector>
<connector id='connector36' type='female' name='GSCLK'>
<description>GSCLK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector36pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector36pin' terminalId='connector36terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector36pad'/><p layer='copper1' svgId='connector36pad'/></pcbView>
</views>
</connector>
<connector id='connector37' type='female' name='XLAT'>
<description>XLAT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector37pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector37pin' terminalId='connector37terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector37pad'/><p layer='copper1' svgId='connector37pad'/></pcbView>
</views>
</connector>
<connector id='connector38' type='female' name='BLANK'>
<description>BLANK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector38pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector38pin' terminalId='connector38terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector38pad'/><p layer='copper1' svgId='connector38pad'/></pcbView>
</views>
</connector>
<connector id='connector39' type='female' name='SOUT'>
<description>SOUT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector39pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector39pin' terminalId='connector39terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector39pad'/><p layer='copper1' svgId='connector39pad'/></pcbView>
</views>
</connector>
<connector id='connector40' type='female' name='SCLK'>
<description>SCLK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector40pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector40pin' terminalId='connector40terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector40pad'/><p layer='copper1' svgId='connector40pad'/></pcbView>
</views>
</connector>
<connector id='connector41' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector41pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector41pin' terminalId='connector41terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector41pad'/><p layer='copper1' svgId='connector41pad'/></pcbView>
</views>
</connector>
<connector id='connector42' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector42pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector42pin' terminalId='connector42terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector42pad'/><p layer='copper1' svgId='connector42pad'/></pcbView>
</views>
</connector>
<connector id='connector43' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector43pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector43pin' terminalId='connector43terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector43pad'/><p layer='copper1' svgId='connector43pad'/></pcbView>
</views>
</connector>
<connector id='connector44' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector44pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector44pin' terminalId='connector44terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector44pad'/><p layer='copper1' svgId='connector44pad'/></pcbView>
</views>
</connector>
<connector id='connector45' type='female' name='OUT10'>
<description>OUT10</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector45pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector45pin' terminalId='connector45terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector45pad'/><p layer='copper1' svgId='connector45pad'/></pcbView>
</views>
</connector>
<connector id='connector46' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector46pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector46pin' terminalId='connector46terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector46pad'/><p layer='copper1' svgId='connector46pad'/></pcbView>
</views>
</connector>
<connector id='connector47' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector47pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector47pin' terminalId='connector47terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector47pad'/><p layer='copper1' svgId='connector47pad'/></pcbView>
</views>
</connector>
<connector id='connector48' type='female' name='OUT11'>
<description>OUT11</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector48pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector48pin' terminalId='connector48terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector48pad'/><p layer='copper1' svgId='connector48pad'/></pcbView>
</views>
</connector>
<connector id='connector49' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector49pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector49pin' terminalId='connector49terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector49pad'/><p layer='copper1' svgId='connector49pad'/></pcbView>
</views>
</connector>
<connector id='connector50' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector50pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector50pin' terminalId='connector50terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector50pad'/><p layer='copper1' svgId='connector50pad'/></pcbView>
</views>
</connector>
<connector id='connector51' type='female' name='OUT12'>
<description>OUT12</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector51pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector51pin' terminalId='connector51terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector51pad'/><p layer='copper1' svgId='connector51pad'/></pcbView>
</views>
</connector>
<connector id='connector52' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector52pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector52pin' terminalId='connector52terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector52pad'/><p layer='copper1' svgId='connector52pad'/></pcbView>
</views>
</connector>
<connector id='connector53' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector53pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector53pin' terminalId='connector53terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector53pad'/><p layer='copper1' svgId='connector53pad'/></pcbView>
</views>
</connector>
<connector id='connector54' type='female' name='OUT13'>
<description>OUT13</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector54pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector54pin' terminalId='connector54terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector54pad'/><p layer='copper1' svgId='connector54pad'/></pcbView>
</views>
</connector>
<connector id='connector55' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector55pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector55pin' terminalId='connector55terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector55pad'/><p layer='copper1' svgId='connector55pad'/></pcbView>
</views>
</connector>
<connector id='connector56' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector56pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector56pin' terminalId='connector56terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector56pad'/><p layer='copper1' svgId='connector56pad'/></pcbView>
</views>
</connector>
<connector id='connector57' type='female' name='OUT14'>
<description>OUT14</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector57pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector57pin' terminalId='connector57terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector57pad'/><p layer='copper1' svgId='connector57pad'/></pcbView>
</views>
</connector>
<connector id='connector58' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector58pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector58pin' terminalId='connector58terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector58pad'/><p layer='copper1' svgId='connector58pad'/></pcbView>
</views>
</connector>
<connector id='connector59' type='female' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector59pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector59pin' terminalId='connector59terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector59pad'/><p layer='copper1' svgId='connector59pad'/></pcbView>
</views>
</connector>
<connector id='connector60' type='female' name='OUT15'>
<description>OUT15</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector60pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector60pin' terminalId='connector60terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector60pad'/><p layer='copper1' svgId='connector60pad'/></pcbView>
</views>
</connector>
<connector id='connector61' type='female' name='VIN'>
<description>VIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector61pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector61pin' terminalId='connector61terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector61pad'/><p layer='copper1' svgId='connector61pad'/></pcbView>
</views>
</connector>
<connector id='connector62' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector62pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector62pin' terminalId='connector62terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector62pad'/><p layer='copper1' svgId='connector62pad'/></pcbView>
</views>
</connector>
<connector id='connector63' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector63pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector63pin' terminalId='connector63terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector63pad'/><p layer='copper1' svgId='connector63pad'/></pcbView>
</views>
</connector>
<connector id='connector64' type='female' name='VIN'>
<description>VIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector64pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector64pin' terminalId='connector64terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector64pad'/><p layer='copper1' svgId='connector64pad'/></pcbView>
</views>
</connector>
<connector id='connector65' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector65pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector65pin' terminalId='connector65terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector65pad'/><p layer='copper1' svgId='connector65pad'/></pcbView>
</views>
</connector>
<connector id='connector66' type='female' name='VIN'>
<description>VIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector66pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector66pin' terminalId='connector66terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector66pad'/><p layer='copper1' svgId='connector66pad'/></pcbView>
</views>
</connector>
<connector id='connector122' type='female' name='3.3V'>
<description>3.3V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector122pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector122pin' terminalId='connector122terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector122pad'/><p layer='copper1' svgId='connector122pad'/></pcbView>
</views>
</connector>
<connector id='connector123' type='female' name='5V_A'>
<description>5V_A</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector123pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector123pin' terminalId='connector123terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector123pad'/><p layer='copper1' svgId='connector123pad'/></pcbView>
</views>
</connector>
<connector id='connector124' type='female' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector124pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector124pin' terminalId='connector124terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector124pad'/><p layer='copper1' svgId='connector124pad'/></pcbView>
</views>
</connector>
<connector id='connector125' type='female' name='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector125pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector125pin' terminalId='connector125terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector125pad'/><p layer='copper1' svgId='connector125pad'/></pcbView>
</views>
</connector>
<connector id='connector126' type='female' name='A2'>
<description>A2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector126pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector126pin' terminalId='connector126terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector126pad'/><p layer='copper1' svgId='connector126pad'/></pcbView>
</views>
</connector>
<connector id='connector127' type='female' name='A3'>
<description>A3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector127pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector127pin' terminalId='connector127terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector127pad'/><p layer='copper1' svgId='connector127pad'/></pcbView>
</views>
</connector>
<connector id='connector128' type='female' name='A4'>
<description>A4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector128pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector128pin' terminalId='connector128terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector128pad'/><p layer='copper1' svgId='connector128pad'/></pcbView>
</views>
</connector>
<connector id='connector129' type='female' name='A5'>
<description>A5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector129pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector129pin' terminalId='connector129terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector129pad'/><p layer='copper1' svgId='connector129pad'/></pcbView>
</views>
</connector>
<connector id='connector130' type='female' name='AREF'>
<description>AREF</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector130pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector130pin' terminalId='connector130terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector130pad'/><p layer='copper1' svgId='connector130pad'/></pcbView>
</views>
</connector>
<connector id='connector131' type='female' name='D2'>
<description>D2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector131pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector131pin' terminalId='connector131terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector131pad'/><p layer='copper1' svgId='connector131pad'/></pcbView>
</views>
</connector>
<connector id='connector132' type='female' name='GSCLK - D3'>
<description>GSCLK - D3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector132pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector132pin' terminalId='connector132terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector132pad'/><p layer='copper1' svgId='connector132pad'/></pcbView>
</views>
</connector>
<connector id='connector133' type='female' name='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector133pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector133pin' terminalId='connector133terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector133pad'/><p layer='copper1' svgId='connector133pad'/></pcbView>
</views>
</connector>
<connector id='connector134' type='female' name='D5'>
<description>D5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector134pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector134pin' terminalId='connector134terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector134pad'/><p layer='copper1' svgId='connector134pad'/></pcbView>
</views>
</connector>
<connector id='connector135' type='female' name='D6'>
<description>D6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector135pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector135pin' terminalId='connector135terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector135pad'/><p layer='copper1' svgId='connector135pad'/></pcbView>
</views>
</connector>
<connector id='connector136' type='female' name='D7'>
<description>D7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector136pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector136pin' terminalId='connector136terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector136pad'/><p layer='copper1' svgId='connector136pad'/></pcbView>
</views>
</connector>
<connector id='connector137' type='female' name='D8'>
<description>D8</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector137pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector137pin' terminalId='connector137terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector137pad'/><p layer='copper1' svgId='connector137pad'/></pcbView>
</views>
</connector>
<connector id='connector138' type='female' name='XLAT - D9'>
<description>XLAT - D9</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector138pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector138pin' terminalId='connector138terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector138pad'/><p layer='copper1' svgId='connector138pad'/></pcbView>
</views>
</connector>
<connector id='connector139' type='female' name='BLANK - D10'>
<description>BLANK - D10</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector139pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector139pin' terminalId='connector139terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector139pad'/><p layer='copper1' svgId='connector139pad'/></pcbView>
</views>
</connector>
<connector id='connector140' type='female' name='SIN - D11'>
<description>SIN - D11</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector140pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector140pin' terminalId='connector140terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector140pad'/><p layer='copper1' svgId='connector140pad'/></pcbView>
</views>
</connector>
<connector id='connector141' type='female' name='D12'>
<description>D12</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector141pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector141pin' terminalId='connector141terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector141pad'/><p layer='copper1' svgId='connector141pad'/></pcbView>
</views>
</connector>
<connector id='connector142' type='female' name='SCLK - D13'>
<description>SCLK - D13</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector142pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector142pin' terminalId='connector142terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector142pad'/><p layer='copper1' svgId='connector142pad'/></pcbView>
</views>
</connector>
<connector id='connector143' type='female' name='GND - GND@0'>
<description>GND - GND@0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector143pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector143pin' terminalId='connector143terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector143pad'/><p layer='copper1' svgId='connector143pad'/></pcbView>
</views>
</connector>
<connector id='connector144' type='female' name='GND - GND@1'>
<description>GND - GND@1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector144pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector144pin' terminalId='connector144terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector144pad'/><p layer='copper1' svgId='connector144pad'/></pcbView>
</views>
</connector>
<connector id='connector145' type='female' name='GND - GND@2'>
<description>GND - GND@2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector145pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector145pin' terminalId='connector145terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector145pad'/><p layer='copper1' svgId='connector145pad'/></pcbView>
</views>
</connector>
<connector id='connector146' type='female' name='RES'>
<description>RES</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector146pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector146pin' terminalId='connector146terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector146pad'/><p layer='copper1' svgId='connector146pad'/></pcbView>
</views>
</connector>
<connector id='connector147' type='female' name='RX'>
<description>RX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector147pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector147pin' terminalId='connector147terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector147pad'/><p layer='copper1' svgId='connector147pad'/></pcbView>
</views>
</connector>
<connector id='connector148' type='female' name='TX'>
<description>TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector148pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector148pin' terminalId='connector148terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector148pad'/><p layer='copper1' svgId='connector148pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector6'/>
<nodeMember connectorId='connector9'/>
<nodeMember connectorId='connector12'/>
<nodeMember connectorId='connector15'/>
<nodeMember connectorId='connector18'/>
<nodeMember connectorId='connector21'/>
<nodeMember connectorId='connector24'/>
<nodeMember connectorId='connector27'/>
<nodeMember connectorId='connector30'/>
<nodeMember connectorId='connector33'/>
<nodeMember connectorId='connector42'/>
<nodeMember connectorId='connector43'/>
<nodeMember connectorId='connector46'/>
<nodeMember connectorId='connector49'/>
<nodeMember connectorId='connector52'/>
<nodeMember connectorId='connector55'/>
<nodeMember connectorId='connector58'/>
<nodeMember connectorId='connector62'/>
<nodeMember connectorId='connector63'/>
<nodeMember connectorId='connector65'/>
<nodeMember connectorId='connector143'/>
<nodeMember connectorId='connector144'/>
<nodeMember connectorId='connector145'/>
</bus>
<bus id='vcc'>
<nodeMember connectorId='connector7'/>
<nodeMember connectorId='connector10'/>
<nodeMember connectorId='connector13'/>
<nodeMember connectorId='connector16'/>
<nodeMember connectorId='connector19'/>
<nodeMember connectorId='connector22'/>
<nodeMember connectorId='connector25'/>
<nodeMember connectorId='connector28'/>
<nodeMember connectorId='connector31'/>
<nodeMember connectorId='connector34'/>
<nodeMember connectorId='connector41'/>
<nodeMember connectorId='connector44'/>
<nodeMember connectorId='connector47'/>
<nodeMember connectorId='connector50'/>
<nodeMember connectorId='connector53'/>
<nodeMember connectorId='connector56'/>
<nodeMember connectorId='connector59'/>
</bus>
<bus id='vin'>
<nodeMember connectorId='connector61'/>
<nodeMember connectorId='connector64'/>
<nodeMember connectorId='connector66'/>
</bus>
<bus id='gsclk'>
<nodeMember connectorId='connector36'/>
<nodeMember connectorId='connector132'/>
</bus>
<bus id='xlat'>
<nodeMember connectorId='connector37'/>
<nodeMember connectorId='connector138'/>
</bus>
<bus id='blank'>
<nodeMember connectorId='connector38'/>
<nodeMember connectorId='connector139'/>
</bus>
<bus id='sclk'>
<nodeMember connectorId='connector40'/>
<nodeMember connectorId='connector142'/>
</bus>
</buses>
</module>
