<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='blueIOT_Rc1-final'>
<version>4</version>
<date>2014-10-03</date>
<author>joev</author>
<description>Painting the Internet of Things Blue. blueIOT is an tiny little board in the size of an SD Card which comes with latest sensors for

measuring acceleration (3 axis), humidity, altitude and temperature. The integrated Bluetooth Low Energy (BLE) module is certified 

and allows easy communication with smartphones and home gateways. All this runs with a single coin cell battery at 3V while consuming

in average 1uA in managed sleep mode. All this is a perfect basis for wearable, fitness tracker, beacons for in door navigation and 

more. Programming is supported with the Arduino IDE using an FTDI cable. For development there is an SD card slot for recording 

sensor data up to 32 GByte. For further extension blueIOT comes with exposed PINs for I2C bus, analog and digital I/Os. OLEDs 

from Adafruit with I2C bus are supported right away. Further details and sample projects can be found on www.Fab-Lab.eu</description>
<title>blueIOT core</title>
<tags>
<tag>Bluetooth</tag>
<tag>LowPower</tag>
<tag>IoT</tag>
<tag>BLE</tag>
<tag>wireless</tag>
<tag>Bluetooth Low Energy</tag>
<tag>shield</tag>
<tag>AtMega328</tag>
<tag>BLUETOOTH MODULE</tag>
<tag>BLE112-A-V1</tag>
<tag>BLUEGIGA</tag>
<tag>fab-lab.eu</tag>
<tag>HTU21D</tag>
<tag>BMP180</tag>
<tag>ADXL362</tag>
<tag>Internet of Things</tag>
<tag>Sensor</tag>
<tag>Fitness Tracker</tag>
<tag>Ultra-Low Power</tag>
<tag>MEMS</tag>
<tag>wearable</tag>
<tag>BLE112</tag>
<tag>Beacon</tag>
</tags>
<properties>
<property name='communication'>Bluetooth</property>
<property name='family'>microcontroller board (blueIOT)</property>
<property name='processor'>AtMega328</property>
<property name='compatible'>Arduino</property>
<property name='variant'>blueIOT core</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/blueIOT_Rc1-final_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/blueIOT_Rc1-final_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/blueIOT_Rc1-final_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/blueIOT_Rc1-final_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector56' type='male' name='D8'>
<description>D8</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector56pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector56pin' terminalId='connector56terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector56pad'/><p layer='copper1' svgId='connector56pad'/></pcbView>
</views>
</connector>
<connector id='connector57' type='male' name='D10'>
<description>D10</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector57pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector57pin' terminalId='connector57terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector57pad'/><p layer='copper1' svgId='connector57pad'/></pcbView>
</views>
</connector>
<connector id='connector58' type='male' name='MOSI'>
<description>MOSI</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector58pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector58pin' terminalId='connector58terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector58pad'/><p layer='copper1' svgId='connector58pad'/></pcbView>
</views>
</connector>
<connector id='connector59' type='male' name='SCK'>
<description>SCK</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector59pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector59pin' terminalId='connector59terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector59pad'/><p layer='copper1' svgId='connector59pad'/></pcbView>
</views>
</connector>
<connector id='connector60' type='male' name='MISO'>
<description>MISO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector60pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector60pin' terminalId='connector60terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector60pad'/><p layer='copper1' svgId='connector60pad'/></pcbView>
</views>
</connector>
<connector id='connector61' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector61pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector61pin' terminalId='connector61terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector61pad'/><p layer='copper1' svgId='connector61pad'/></pcbView>
</views>
</connector>
<connector id='connector62' type='male' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector62pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector62pin' terminalId='connector62terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector62pad'/><p layer='copper1' svgId='connector62pad'/></pcbView>
</views>
</connector>
<connector id='connector63' type='male' name='P21'>
<description>P21</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector63pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector63pin' terminalId='connector63terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector63pad'/><p layer='copper1' svgId='connector63pad'/></pcbView>
</views>
</connector>
<connector id='connector64' type='male' name='P22'>
<description>P22</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector64pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector64pin' terminalId='connector64terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector64pad'/><p layer='copper1' svgId='connector64pad'/></pcbView>
</views>
</connector>
<connector id='connector65' type='male' name='D5'>
<description>D5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector65pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector65pin' terminalId='connector65terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector65pad'/><p layer='copper1' svgId='connector65pad'/></pcbView>
</views>
</connector>
<connector id='connector66' type='male' name='TXD'>
<description>TXD</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector66pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector66pin' terminalId='connector66terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector66pad'/><p layer='copper1' svgId='connector66pad'/></pcbView>
</views>
</connector>
<connector id='connector67' type='male' name='D2'>
<description>D2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector67pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector67pin' terminalId='connector67terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector67pad'/><p layer='copper1' svgId='connector67pad'/></pcbView>
</views>
</connector>
<connector id='connector68' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector68pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector68pin' terminalId='connector68terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector68pad'/><p layer='copper1' svgId='connector68pad'/></pcbView>
</views>
</connector>
<connector id='connector69' type='male' name='RXD'>
<description>RXD</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector69pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector69pin' terminalId='connector69terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector69pad'/><p layer='copper1' svgId='connector69pad'/></pcbView>
</views>
</connector>
<connector id='connector70' type='male' name='A5'>
<description>A5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector70pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector70pin' terminalId='connector70terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector70pad'/><p layer='copper1' svgId='connector70pad'/></pcbView>
</views>
</connector>
<connector id='connector71' type='male' name='A4'>
<description>A4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector71pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector71pin' terminalId='connector71terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector71pad'/><p layer='copper1' svgId='connector71pad'/></pcbView>
</views>
</connector>
<connector id='connector72' type='male' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector72pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector72pin' terminalId='connector72terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector72pad'/><p layer='copper1' svgId='connector72pad'/></pcbView>
</views>
</connector>
<connector id='connector73' type='male' name='DTR'>
<description>DTR</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector73pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector73pin' terminalId='connector73terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector73pad'/><p layer='copper1' svgId='connector73pad'/></pcbView>
</views>
</connector>
<connector id='connector74' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector74pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector74pin' terminalId='connector74terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector74pad'/><p layer='copper1' svgId='connector74pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector68'/>
<nodeMember connectorId='connector74'/>
</bus>
</buses>
</module>
