<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='GPSShield-v15'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Description: &lt;/span&gt;Adding GPS to your Arduino has never been easier. The multiple GPS receivers attach easily to the shield, and with the &lt;a href=&quot;http://www.sparkfun.com/tutorial/GPSQuickStart/gps_parsing_v13.pde&quot;&gt;example sketch&lt;/a&gt;, you will be able to locate your exact position within a few meters. Here&amp;#39;s where &lt;a href=&quot;http://maps.google.com/maps?q=40.06477,+-105.20997&quot; target=&quot;_blank&quot;&gt;we are&lt;/a&gt;. GPS also gives you amazingly accurate time! A &lt;a href=&quot;http://www.sparkfun.com/commerce/tutorial_info.php?tutorials_id=173&quot;&gt;GPS quickstart guide&lt;/a&gt; is available for this product.&lt;/p&gt;


&lt;p&gt;


	With the GPS Shield you can add GPS functionality to your Arduino. A connector for the popular &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=465&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;EM-406&lt;/a&gt; GPS receiver is populated on the board, and footprints for &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=8288&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;EM-408&lt;/a&gt; and &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=8297&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;EB-85A&lt;/a&gt; connectors are also made available (connectors are not soldered on or included and can be found below in the related items). There is also a spot for the &lt;a href=&quot;http://www.sparkfun.com/products/9758&quot; target=&quot;_blank&quot;&gt;SUP500&lt;/a&gt; GPS module. The regular GPS pins (RX, TX, PPS, etc.) are also broken out to a 10-pin 0.1&amp;quot; pitch header, and a small protoyping area is also provided.&lt;/p&gt;


&lt;p&gt;


	The DLINE/UART switch switches the GPS module&amp;#39;s input/output between Arduino&amp;#39;s standard TX/RX pins or any digital pins on the Arduino (default setting uses pins 3 and 2 connected to TX and RX, respectively). The regular GPS pins (RX, TX, PPS, etc.) are broken out to a 10-pin 0.1&amp;quot; pitch header, and a small protoyping area is also provided. An ON/OFF switch is included which controls power to the GPS module. Additionally, the Arduino reset switch is also brought out.&lt;/p&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Note: &lt;/span&gt;The DLINE/UART switch must be set to DLINE in order to upload code through the Arduino IDE.&lt;/p&gt;


&lt;p&gt;


	The shield also includes the footprint for a &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=7948&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;12mm coin cell battery holder&lt;/a&gt; to provide battery backup to the optional EB-85A gps module.&lt;/p&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Note: &lt;/span&gt;GPS modules are not included with the GPS Shield, and only the EM-406 connector is populated. Headers are also not installed or included, we recommend the &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9280&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;6&lt;/a&gt; and &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9279&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;8-pin stackable headers&lt;/a&gt;.&lt;/p&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Features:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		EM-406 connector populated&lt;/li&gt;


	&lt;li&gt;


		EM-408 and EB-85A connector footprints provided and connected for optional use&lt;/li&gt;


	&lt;li&gt;


		SUP500 connector and footprint&lt;/li&gt;


	&lt;li&gt;


		Coin cell battery socket footprint provided and connected for optional battery backup of EB-85A GPS module&lt;/li&gt;


	&lt;li&gt;


		Standard Arduino sized shield&lt;/li&gt;


	&lt;li&gt;


		Prototyping area&lt;/li&gt;


	&lt;li&gt;


		GPS serial and PPS signals broken out to a 0.1&amp;quot; header for additional device connections&lt;/li&gt;


	&lt;li&gt;


		Arduino reset button&lt;/li&gt;


	&lt;li&gt;


		DLINE/UART switch controls serial communications&lt;/li&gt;


	&lt;li&gt;


		ON/OFF switch controls power to GPS module&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/commerce/tutorial_info.php?tutorials_id=173&quot;&gt;GPS Quickstart Guide&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/commerce/tutorial_info.php?tutorials_id=184&quot;&gt;Assembly Guide&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/tutorial/GPSQuickStart/gps_parsing_v13.pde&quot;&gt;Example Sketch&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/DevTools/Arduino/GPSShield-v14.pdf&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/DevTools/Arduino/GPSShield-v14.zip&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;strong&gt;Replaces: &lt;/strong&gt;&lt;a href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9487&quot; target=&quot;_blank&quot;&gt;GPS-09487&lt;/a&gt;&lt;/p&gt;</description>
<title>Arduino GPS Shield</title>
<url>http://www.sparkfun.com/products/10102</url>
<tags>
<tag>GPS</tag>
</tags>
<properties>
<property name='family'>GPS Shield</property>
<property name='Update Rate'>Selectable (Based on GPS Receiver)</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/GPSShield-v15_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/GPSShield-v15_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/GPSShield-v15_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/GPSShield-v15_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector9' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector9pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector9pin' terminalId='connector9terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector9pad'/><p layer='copper1' svgId='connector9pad'/></pcbView>
</views>
</connector>
<connector id='connector10' type='male' name='PSEL'>
<description>PSEL</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector10pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector10pin' terminalId='connector10terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector10pad'/><p layer='copper1' svgId='connector10pad'/></pcbView>
</views>
</connector>
<connector id='connector11' type='male' name='BATT'>
<description>BATT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector11pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector11pin' terminalId='connector11terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector11pad'/><p layer='copper1' svgId='connector11pad'/></pcbView>
</views>
</connector>
<connector id='connector12' type='male' name='PPS'>
<description>PPS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector12pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector12pin' terminalId='connector12terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector12pad'/><p layer='copper1' svgId='connector12pad'/></pcbView>
</views>
</connector>
<connector id='connector13' type='male' name='RX2'>
<description>RX2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector13pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector13pin' terminalId='connector13terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector13pad'/><p layer='copper1' svgId='connector13pad'/></pcbView>
</views>
</connector>
<connector id='connector14' type='male' name='TX2'>
<description>TX2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector14pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector14pin' terminalId='connector14terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector14pad'/><p layer='copper1' svgId='connector14pad'/></pcbView>
</views>
</connector>
<connector id='connector15' type='male' name='RX'>
<description>RX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector15pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector15pin' terminalId='connector15terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector15pad'/><p layer='copper1' svgId='connector15pad'/></pcbView>
</views>
</connector>
<connector id='connector16' type='male' name='TX'>
<description>TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector16pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector16pin' terminalId='connector16terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector16pad'/><p layer='copper1' svgId='connector16pad'/></pcbView>
</views>
</connector>
<connector id='connector17' type='male' name='EN'>
<description>EN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector17pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector17pin' terminalId='connector17terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector17pad'/><p layer='copper1' svgId='connector17pad'/></pcbView>
</views>
</connector>
<connector id='connector18' type='male' name='3.3V'>
<description>3.3V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector18pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector18pin' terminalId='connector18terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector18pad'/><p layer='copper1' svgId='connector18pad'/></pcbView>
</views>
</connector>
<connector id='connector19' type='male' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector19pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector19pin' terminalId='connector19terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector19pad'/><p layer='copper1' svgId='connector19pad'/></pcbView>
</views>
</connector>
<connector id='connector20' type='male' name='UART_RX'>
<description>UART_RX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector20pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector20pin' terminalId='connector20terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector20pad'/><p layer='copper1' svgId='connector20pad'/></pcbView>
</views>
</connector>
<connector id='connector21' type='male' name='UART_TX'>
<description>UART_TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector21pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector21pin' terminalId='connector21terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector21pad'/><p layer='copper1' svgId='connector21pad'/></pcbView>
</views>
</connector>
<connector id='connector22' type='male' name='D_RX'>
<description>D_RX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector22pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector22pin' terminalId='connector22terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector22pad'/><p layer='copper1' svgId='connector22pad'/></pcbView>
</views>
</connector>
<connector id='connector23' type='male' name='D_TX'>
<description>D_TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector23pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector23pin' terminalId='connector23terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector23pad'/><p layer='copper1' svgId='connector23pad'/></pcbView>
</views>
</connector>
<connector id='connector24' type='male' name='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector24pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector24pin' terminalId='connector24terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector24pad'/><p layer='copper1' svgId='connector24pad'/></pcbView>
</views>
</connector>
<connector id='connector25' type='male' name='D5'>
<description>D5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector25pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector25pin' terminalId='connector25terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector25pad'/><p layer='copper1' svgId='connector25pad'/></pcbView>
</views>
</connector>
<connector id='connector26' type='male' name='D6'>
<description>D6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector26pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector26pin' terminalId='connector26terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector26pad'/><p layer='copper1' svgId='connector26pad'/></pcbView>
</views>
</connector>
<connector id='connector27' type='male' name='D7'>
<description>D7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector27pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector27pin' terminalId='connector27terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector27pad'/><p layer='copper1' svgId='connector27pad'/></pcbView>
</views>
</connector>
<connector id='connector28' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector28pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector28pin' terminalId='connector28terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector28pad'/><p layer='copper1' svgId='connector28pad'/></pcbView>
</views>
</connector>
<connector id='connector29' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector29pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector29pin' terminalId='connector29terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector29pad'/><p layer='copper1' svgId='connector29pad'/></pcbView>
</views>
</connector>
<connector id='connector30' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector30pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector30pin' terminalId='connector30terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector30pad'/><p layer='copper1' svgId='connector30pad'/></pcbView>
</views>
</connector>
<connector id='connector31' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector31pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector31pin' terminalId='connector31terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector31pad'/><p layer='copper1' svgId='connector31pad'/></pcbView>
</views>
</connector>
<connector id='connector32' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector32pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector32pin' terminalId='connector32terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector32pad'/><p layer='copper1' svgId='connector32pad'/></pcbView>
</views>
</connector>
<connector id='connector33' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector33pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector33pin' terminalId='connector33terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector33pad'/><p layer='copper1' svgId='connector33pad'/></pcbView>
</views>
</connector>
<connector id='connector34' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector34pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector34pin' terminalId='connector34terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector34pad'/><p layer='copper1' svgId='connector34pad'/></pcbView>
</views>
</connector>
<connector id='connector37' type='male' name='D8'>
<description>D8</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector37pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector37pin' terminalId='connector37terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector37pad'/><p layer='copper1' svgId='connector37pad'/></pcbView>
</views>
</connector>
<connector id='connector38' type='male' name='D9'>
<description>D9</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector38pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector38pin' terminalId='connector38terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector38pad'/><p layer='copper1' svgId='connector38pad'/></pcbView>
</views>
</connector>
<connector id='connector39' type='male' name='D10'>
<description>D10</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector39pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector39pin' terminalId='connector39terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector39pad'/><p layer='copper1' svgId='connector39pad'/></pcbView>
</views>
</connector>
<connector id='connector40' type='male' name='D11'>
<description>D11</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector40pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector40pin' terminalId='connector40terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector40pad'/><p layer='copper1' svgId='connector40pad'/></pcbView>
</views>
</connector>
<connector id='connector41' type='male' name='D12'>
<description>D12</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector41pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector41pin' terminalId='connector41terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector41pad'/><p layer='copper1' svgId='connector41pad'/></pcbView>
</views>
</connector>
<connector id='connector42' type='male' name='D13'>
<description>D13</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector42pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector42pin' terminalId='connector42terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector42pad'/><p layer='copper1' svgId='connector42pad'/></pcbView>
</views>
</connector>
<connector id='connector59' type='female' name='3.3VIN'>
<description>3.3VIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector59pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector59pin' terminalId='connector59terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector59pad'/><p layer='copper1' svgId='connector59pad'/></pcbView>
</views>
</connector>
<connector id='connector60' type='female' name='5VIN'>
<description>5VIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector60pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector60pin' terminalId='connector60terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector60pad'/><p layer='copper1' svgId='connector60pad'/></pcbView>
</views>
</connector>
<connector id='connector61' type='female' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector61pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector61pin' terminalId='connector61terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector61pad'/><p layer='copper1' svgId='connector61pad'/></pcbView>
</views>
</connector>
<connector id='connector62' type='female' name='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector62pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector62pin' terminalId='connector62terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector62pad'/><p layer='copper1' svgId='connector62pad'/></pcbView>
</views>
</connector>
<connector id='connector63' type='female' name='A2'>
<description>A2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector63pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector63pin' terminalId='connector63terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector63pad'/><p layer='copper1' svgId='connector63pad'/></pcbView>
</views>
</connector>
<connector id='connector64' type='female' name='A3'>
<description>A3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector64pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector64pin' terminalId='connector64terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector64pad'/><p layer='copper1' svgId='connector64pad'/></pcbView>
</views>
</connector>
<connector id='connector65' type='female' name='A4'>
<description>A4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector65pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector65pin' terminalId='connector65terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector65pad'/><p layer='copper1' svgId='connector65pad'/></pcbView>
</views>
</connector>
<connector id='connector66' type='female' name='A5'>
<description>A5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector66pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector66pin' terminalId='connector66terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector66pad'/><p layer='copper1' svgId='connector66pad'/></pcbView>
</views>
</connector>
<connector id='connector67' type='female' name='AREF'>
<description>AREF</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector67pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector67pin' terminalId='connector67terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector67pad'/><p layer='copper1' svgId='connector67pad'/></pcbView>
</views>
</connector>
<connector id='connector68' type='female' name='D_RX'>
<description>D_RX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector68pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector68pin' terminalId='connector68terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector68pad'/><p layer='copper1' svgId='connector68pad'/></pcbView>
</views>
</connector>
<connector id='connector69' type='female' name='D_TX'>
<description>D_TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector69pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector69pin' terminalId='connector69terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector69pad'/><p layer='copper1' svgId='connector69pad'/></pcbView>
</views>
</connector>
<connector id='connector70' type='female' name='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector70pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector70pin' terminalId='connector70terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector70pad'/><p layer='copper1' svgId='connector70pad'/></pcbView>
</views>
</connector>
<connector id='connector71' type='female' name='D5'>
<description>D5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector71pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector71pin' terminalId='connector71terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector71pad'/><p layer='copper1' svgId='connector71pad'/></pcbView>
</views>
</connector>
<connector id='connector72' type='female' name='D6'>
<description>D6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector72pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector72pin' terminalId='connector72terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector72pad'/><p layer='copper1' svgId='connector72pad'/></pcbView>
</views>
</connector>
<connector id='connector73' type='female' name='D7'>
<description>D7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector73pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector73pin' terminalId='connector73terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector73pad'/><p layer='copper1' svgId='connector73pad'/></pcbView>
</views>
</connector>
<connector id='connector74' type='female' name='D8'>
<description>D8</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector74pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector74pin' terminalId='connector74terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector74pad'/><p layer='copper1' svgId='connector74pad'/></pcbView>
</views>
</connector>
<connector id='connector75' type='female' name='D9'>
<description>D9</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector75pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector75pin' terminalId='connector75terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector75pad'/><p layer='copper1' svgId='connector75pad'/></pcbView>
</views>
</connector>
<connector id='connector76' type='female' name='D10'>
<description>D10</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector76pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector76pin' terminalId='connector76terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector76pad'/><p layer='copper1' svgId='connector76pad'/></pcbView>
</views>
</connector>
<connector id='connector77' type='female' name='D11'>
<description>D11</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector77pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector77pin' terminalId='connector77terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector77pad'/><p layer='copper1' svgId='connector77pad'/></pcbView>
</views>
</connector>
<connector id='connector78' type='female' name='D12'>
<description>D12</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector78pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector78pin' terminalId='connector78terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector78pad'/><p layer='copper1' svgId='connector78pad'/></pcbView>
</views>
</connector>
<connector id='connector79' type='female' name='D13'>
<description>D13</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector79pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector79pin' terminalId='connector79terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector79pad'/><p layer='copper1' svgId='connector79pad'/></pcbView>
</views>
</connector>
<connector id='connector80' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector80pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector80pin' terminalId='connector80terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector80pad'/><p layer='copper1' svgId='connector80pad'/></pcbView>
</views>
</connector>
<connector id='connector81' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector81pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector81pin' terminalId='connector81terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector81pad'/><p layer='copper1' svgId='connector81pad'/></pcbView>
</views>
</connector>
<connector id='connector82' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector82pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector82pin' terminalId='connector82terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector82pad'/><p layer='copper1' svgId='connector82pad'/></pcbView>
</views>
</connector>
<connector id='connector83' type='female' name='RES'>
<description>RES</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector83pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector83pin' terminalId='connector83terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector83pad'/><p layer='copper1' svgId='connector83pad'/></pcbView>
</views>
</connector>
<connector id='connector84' type='female' name='UART_RX'>
<description>UART_RX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector84pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector84pin' terminalId='connector84terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector84pad'/><p layer='copper1' svgId='connector84pad'/></pcbView>
</views>
</connector>
<connector id='connector85' type='female' name='UART_TX'>
<description>UART_TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector85pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector85pin' terminalId='connector85terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector85pad'/><p layer='copper1' svgId='connector85pad'/></pcbView>
</views>
</connector>
<connector id='connector86' type='female' name='VIN'>
<description>VIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector86pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector86pin' terminalId='connector86terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector86pad'/><p layer='copper1' svgId='connector86pad'/></pcbView>
</views>
</connector>
<connector id='connector133' type='female' name='N$2'>
<description>N$2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector133pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector133pin' terminalId='connector133terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector133pad' hybrid='yes' /><p layer='copper1' svgId='connector133pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector134' type='female' name='N$4'>
<description>N$4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector134pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector134pin' terminalId='connector134terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector134pad' hybrid='yes' /><p layer='copper1' svgId='connector134pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector135' type='female' name='N$6'>
<description>N$6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector135pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector135pin' terminalId='connector135terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector135pad' hybrid='yes' /><p layer='copper1' svgId='connector135pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector136' type='female' name='N$7'>
<description>N$7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector136pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector136pin' terminalId='connector136terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector136pad' hybrid='yes' /><p layer='copper1' svgId='connector136pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector137' type='female' name='N$8'>
<description>N$8</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector137pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector137pin' terminalId='connector137terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector137pad' hybrid='yes' /><p layer='copper1' svgId='connector137pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector138' type='female' name='N$9'>
<description>N$9</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector138pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector138pin' terminalId='connector138terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector138pad' hybrid='yes' /><p layer='copper1' svgId='connector138pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector139' type='female' name='N$10'>
<description>N$10</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector139pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector139pin' terminalId='connector139terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector139pad' hybrid='yes' /><p layer='copper1' svgId='connector139pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector140' type='female' name='N$11'>
<description>N$11</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector140pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector140pin' terminalId='connector140terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector140pad' hybrid='yes' /><p layer='copper1' svgId='connector140pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector141' type='female' name='N$13'>
<description>N$13</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector141pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector141pin' terminalId='connector141terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector141pad' hybrid='yes' /><p layer='copper1' svgId='connector141pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector142' type='female' name='N$15'>
<description>N$15</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector142pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector142pin' terminalId='connector142terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector142pad' hybrid='yes' /><p layer='copper1' svgId='connector142pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector143' type='female' name='N$16'>
<description>N$16</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector143pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector143pin' terminalId='connector143terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector143pad' hybrid='yes' /><p layer='copper1' svgId='connector143pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector144' type='female' name='N$17'>
<description>N$17</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector144pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector144pin' terminalId='connector144terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector144pad' hybrid='yes' /><p layer='copper1' svgId='connector144pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector145' type='female' name='N$18'>
<description>N$18</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector145pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector145pin' terminalId='connector145terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector145pad' hybrid='yes' /><p layer='copper1' svgId='connector145pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector146' type='female' name='N$19'>
<description>N$19</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector146pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector146pin' terminalId='connector146terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector146pad' hybrid='yes' /><p layer='copper1' svgId='connector146pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector147' type='female' name='N$20'>
<description>N$20</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector147pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector147pin' terminalId='connector147terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector147pad' hybrid='yes' /><p layer='copper1' svgId='connector147pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector148' type='female' name='N$21'>
<description>N$21</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector148pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector148pin' terminalId='connector148terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector148pad' hybrid='yes' /><p layer='copper1' svgId='connector148pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector149' type='female' name='N$23'>
<description>N$23</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector149pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector149pin' terminalId='connector149terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector149pad' hybrid='yes' /><p layer='copper1' svgId='connector149pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector150' type='female' name='N$25'>
<description>N$25</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector150pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector150pin' terminalId='connector150terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector150pad' hybrid='yes' /><p layer='copper1' svgId='connector150pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector151' type='female' name='N$27'>
<description>N$27</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector151pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector151pin' terminalId='connector151terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector151pad' hybrid='yes' /><p layer='copper1' svgId='connector151pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector152' type='female' name='N$28'>
<description>N$28</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector152pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector152pin' terminalId='connector152terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector152pad' hybrid='yes' /><p layer='copper1' svgId='connector152pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector153' type='female' name='N$29'>
<description>N$29</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector153pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector153pin' terminalId='connector153terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector153pad' hybrid='yes' /><p layer='copper1' svgId='connector153pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector154' type='female' name='N$30'>
<description>N$30</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector154pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector154pin' terminalId='connector154terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector154pad' hybrid='yes' /><p layer='copper1' svgId='connector154pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector155' type='female' name='N$31'>
<description>N$31</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector155pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector155pin' terminalId='connector155terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector155pad' hybrid='yes' /><p layer='copper1' svgId='connector155pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector156' type='female' name='N$32'>
<description>N$32</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector156pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector156pin' terminalId='connector156terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector156pad' hybrid='yes' /><p layer='copper1' svgId='connector156pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector157' type='female' name='N$33'>
<description>N$33</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector157pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector157pin' terminalId='connector157terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector157pad' hybrid='yes' /><p layer='copper1' svgId='connector157pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector158' type='female' name='N$40'>
<description>N$40</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector158pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector158pin' terminalId='connector158terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector158pad' hybrid='yes' /><p layer='copper1' svgId='connector158pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector159' type='female' name='N$41'>
<description>N$41</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector159pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector159pin' terminalId='connector159terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector159pad' hybrid='yes' /><p layer='copper1' svgId='connector159pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector160' type='female' name='N$42'>
<description>N$42</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector160pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector160pin' terminalId='connector160terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector160pad' hybrid='yes' /><p layer='copper1' svgId='connector160pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector161' type='female' name='N$43'>
<description>N$43</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector161pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector161pin' terminalId='connector161terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector161pad' hybrid='yes' /><p layer='copper1' svgId='connector161pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector162' type='female' name='N$44'>
<description>N$44</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector162pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector162pin' terminalId='connector162terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector162pad' hybrid='yes' /><p layer='copper1' svgId='connector162pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector163' type='female' name='N$45'>
<description>N$45</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector163pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector163pin' terminalId='connector163terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector163pad' hybrid='yes' /><p layer='copper1' svgId='connector163pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector164' type='female' name='N$52'>
<description>N$52</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector164pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector164pin' terminalId='connector164terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector164pad' hybrid='yes' /><p layer='copper1' svgId='connector164pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector165' type='female' name='N$53'>
<description>N$53</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector165pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector165pin' terminalId='connector165terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector165pad' hybrid='yes' /><p layer='copper1' svgId='connector165pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector166' type='female' name='N$54'>
<description>N$54</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector166pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector166pin' terminalId='connector166terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector166pad' hybrid='yes' /><p layer='copper1' svgId='connector166pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector167' type='female' name='N$55'>
<description>N$55</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector167pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector167pin' terminalId='connector167terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector167pad' hybrid='yes' /><p layer='copper1' svgId='connector167pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector168' type='female' name='N$56'>
<description>N$56</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector168pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector168pin' terminalId='connector168terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector168pad' hybrid='yes' /><p layer='copper1' svgId='connector168pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector169' type='female' name='N$57'>
<description>N$57</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector169pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector169pin' terminalId='connector169terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector169pad' hybrid='yes' /><p layer='copper1' svgId='connector169pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector170' type='female' name='N$64'>
<description>N$64</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector170pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector170pin' terminalId='connector170terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector170pad' hybrid='yes' /><p layer='copper1' svgId='connector170pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector171' type='female' name='N$65'>
<description>N$65</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector171pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector171pin' terminalId='connector171terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector171pad' hybrid='yes' /><p layer='copper1' svgId='connector171pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector172' type='female' name='N$66'>
<description>N$66</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector172pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector172pin' terminalId='connector172terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector172pad' hybrid='yes' /><p layer='copper1' svgId='connector172pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector173' type='female' name='N$67'>
<description>N$67</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector173pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector173pin' terminalId='connector173terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector173pad' hybrid='yes' /><p layer='copper1' svgId='connector173pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector174' type='female' name='N$68'>
<description>N$68</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector174pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector174pin' terminalId='connector174terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector174pad' hybrid='yes' /><p layer='copper1' svgId='connector174pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector175' type='female' name='N$69'>
<description>N$69</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector175pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector175pin' terminalId='connector175terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector175pad' hybrid='yes' /><p layer='copper1' svgId='connector175pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector176' type='female' name='N$76'>
<description>N$76</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector176pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector176pin' terminalId='connector176terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector176pad' hybrid='yes' /><p layer='copper1' svgId='connector176pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector177' type='female' name='N$77'>
<description>N$77</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector177pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector177pin' terminalId='connector177terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector177pad' hybrid='yes' /><p layer='copper1' svgId='connector177pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector178' type='female' name='N$78'>
<description>N$78</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector178pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector178pin' terminalId='connector178terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector178pad' hybrid='yes' /><p layer='copper1' svgId='connector178pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector179' type='female' name='N$79'>
<description>N$79</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector179pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector179pin' terminalId='connector179terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector179pad' hybrid='yes' /><p layer='copper1' svgId='connector179pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector180' type='female' name='N$80'>
<description>N$80</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector180pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector180pin' terminalId='connector180terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector180pad' hybrid='yes' /><p layer='copper1' svgId='connector180pad' hybrid='yes' /></pcbView>
</views>
</connector>
<connector id='connector181' type='female' name='N$81'>
<description>N$81</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector181pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector181pin' terminalId='connector181terminal' hybrid='yes' /></schematicView>
<pcbView>
<p layer='copper0' svgId='connector181pad' hybrid='yes' /><p layer='copper1' svgId='connector181pad' hybrid='yes' /></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector9'/>
<nodeMember connectorId='connector28'/>
<nodeMember connectorId='connector29'/>
<nodeMember connectorId='connector30'/>
<nodeMember connectorId='connector31'/>
<nodeMember connectorId='connector32'/>
<nodeMember connectorId='connector33'/>
<nodeMember connectorId='connector34'/>
<nodeMember connectorId='connector80'/>
<nodeMember connectorId='connector81'/>
<nodeMember connectorId='connector82'/>
</bus>
<bus id='d_rx'>
<nodeMember connectorId='connector22'/>
<nodeMember connectorId='connector68'/>
</bus>
<bus id='d_tx'>
<nodeMember connectorId='connector23'/>
<nodeMember connectorId='connector69'/>
</bus>
<bus id='d4'>
<nodeMember connectorId='connector24'/>
<nodeMember connectorId='connector70'/>
</bus>
<bus id='d5'>
<nodeMember connectorId='connector25'/>
<nodeMember connectorId='connector71'/>
</bus>
<bus id='d6'>
<nodeMember connectorId='connector26'/>
<nodeMember connectorId='connector72'/>
</bus>
<bus id='d7'>
<nodeMember connectorId='connector27'/>
<nodeMember connectorId='connector73'/>
</bus>
<bus id='d8'>
<nodeMember connectorId='connector37'/>
<nodeMember connectorId='connector74'/>
</bus>
<bus id='d9'>
<nodeMember connectorId='connector38'/>
<nodeMember connectorId='connector75'/>
</bus>
<bus id='d10'>
<nodeMember connectorId='connector39'/>
<nodeMember connectorId='connector76'/>
</bus>
<bus id='d11'>
<nodeMember connectorId='connector40'/>
<nodeMember connectorId='connector77'/>
</bus>
<bus id='d12'>
<nodeMember connectorId='connector41'/>
<nodeMember connectorId='connector78'/>
</bus>
<bus id='d13'>
<nodeMember connectorId='connector42'/>
<nodeMember connectorId='connector79'/>
</bus>
<bus id='uart_rx'>
<nodeMember connectorId='connector20'/>
<nodeMember connectorId='connector84'/>
</bus>
<bus id='uart_tx'>
<nodeMember connectorId='connector21'/>
<nodeMember connectorId='connector85'/>
</bus>
</buses>
</module>
