<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.4.4b.10.03.4492" moduleId="teensy_3.1" referenceFile="Teensy_3.1.fzp">
 <author>Fabian Althaus modified by Ouinouin</author>
 <title>Teensy 3.1</title>
 <label>Teensy 3.1</label>
 <date>Mo Jan 20 2014</date>
 <tags>
  <tag>Wino</tag>
  <tag>Teensy 3.1</tag>
  <tag>microcontroller</tag>
  <tag>Freescale</tag>
  <tag>Low power</tag>
  <tag>Teensy</tag>
 </tags>
 <properties>
  <property name="family">microcontroller board (teensy)</property>
  <property name="variant">Teensy 3.1</property>
  <property name="input voltage">5.0 V</property>
  <property name="layer"></property>
  <property name="processor">MK20DX256</property>
  <property name="I/O voltage">output 3.3V , Input 5V tolerant</property>
  <property name="part number"></property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'Sans Serif'; font-size:9pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-family:'MS Shell Dlg 2'; font-size:8pt;">The Teensy is a complete USB-based microcontoller development system, in a very small footprint, capable of implementing many types of projects. All programming is done via the USB port. No special programmer is needed, only a standard micro-USB cable and a PC or Macintosh with a USB port. It has a USB keyboard/mouse/joystick emulation stack and can be programmed through Arduino IDE.&lt;/span>&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/teensy_3.1_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/teensy_3.1_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/teensy_3.1_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/teensy_3.1_pcb.svg">
    <layer layerId="copper1"/>
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="female" id="connector15" name="3V3">
   <description>3.3V Input</description>
   <views>
    <breadboardView>
     <p svgId="connector15pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector15pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector15pin" layer="copper0"/>
     <p svgId="connector15pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector7" name="D6">
   <description>Digital Inpout/Output and PWM</description>
   <views>
    <breadboardView>
     <p svgId="connector7pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector7pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector7pin" layer="copper0"/>
     <p svgId="connector7pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector16" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector16pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector16pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector16pin" layer="copper0"/>
     <p svgId="connector16pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector8" name="D7">
   <description>Digital Inpout/Output and RX3</description>
   <views>
    <breadboardView>
     <p svgId="connector8pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector8pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector8pin" layer="copper0"/>
     <p svgId="connector8pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector17" name="Program">
   <description>Program</description>
   <views>
    <breadboardView>
     <p svgId="connector17pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector17pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector17pin" layer="copper0"/>
     <p svgId="connector17pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector9" name="D8">
   <description>Digital Inpout/Output and TX3</description>
   <views>
    <breadboardView>
     <p svgId="connector9pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector9pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector9pin" layer="copper0"/>
     <p svgId="connector9pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector18" name="A14/DAC">
   <description>this is a real DAC, not a PWM one. this pin was previously the reset pin on T3.0.</description>
   <views>
    <breadboardView>
     <p svgId="connector18pin" layer="breadboard" terminalId="connector18terminal"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector18pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector18pin" layer="copper0"/>
     <p svgId="connector18pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector19" name="D13">
   <description>Digital I/O</description>
   <views>
    <breadboardView>
     <p svgId="connector19pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector19pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector19pin" layer="copper0"/>
     <p svgId="connector19pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector20" name="A0/D14">
   <description>Analog Input/Digital I/O</description>
   <views>
    <breadboardView>
     <p svgId="connector20pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector20pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector20pin" layer="copper0"/>
     <p svgId="connector20pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector21" name="A1/D15">
   <description>Analog Input/Digital I/O</description>
   <views>
    <breadboardView>
     <p svgId="connector21pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector21pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector21pin" layer="copper0"/>
     <p svgId="connector21pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector22" name="A2/D16">
   <description>Analog Input/Digital I/O</description>
   <views>
    <breadboardView>
     <p svgId="connector22pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector22pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector22pin" layer="copper0"/>
     <p svgId="connector22pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector23" name="A3/D17">
   <description>Analog Input/Digital I/O</description>
   <views>
    <breadboardView>
     <p svgId="connector23pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector23pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector23pin" layer="copper0"/>
     <p svgId="connector23pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector24" name="A4/D18">
   <description>Analog Input/Digital I/O - SDA</description>
   <views>
    <breadboardView>
     <p svgId="connector24pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector24pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector24pin" layer="copper0"/>
     <p svgId="connector24pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector25" name="A5/D19">
   <description>Analog Input/Digital I/O - SCL</description>
   <views>
    <breadboardView>
     <p svgId="connector25pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector25pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector25pin" layer="copper0"/>
     <p svgId="connector25pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector26" name="A6/D20">
   <description>Analog Input/Digital I/O, PWM</description>
   <views>
    <breadboardView>
     <p svgId="connector26pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector26pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector26pin" layer="copper0"/>
     <p svgId="connector26pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector27" name="A7/D21">
   <description>Analog Input/Digital I/O, PWM</description>
   <views>
    <breadboardView>
     <p svgId="connector27pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector27pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector27pin" layer="copper0"/>
     <p svgId="connector27pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector28" name="A8/D22">
   <description>Analog Input/Digital I/O, PWM</description>
   <views>
    <breadboardView>
     <p svgId="connector28pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector28pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector28pin" layer="copper0"/>
     <p svgId="connector28pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector29" name="A9/D23">
   <description>Analog Input/Digital I/O, PWM</description>
   <views>
    <breadboardView>
     <p svgId="connector29pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector29pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector29pin" layer="copper0"/>
     <p svgId="connector29pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector30" name="3V3">
   <description>+3.3V Input (100mA max)</description>
   <views>
    <breadboardView>
     <p svgId="connector30pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector30pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector30pin" layer="copper0"/>
     <p svgId="connector30pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector0" name="GND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector1" name="D0">
   <description>Digital I/O and RX1</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector10" name="D9">
   <description>Digital I/O, PWM and RX2</description>
   <views>
    <breadboardView>
     <p svgId="connector10pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector10pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector10pin" layer="copper0"/>
     <p svgId="connector10pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector2" name="D1">
   <description>Digital I/O and TX1</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector3" name="D2">
   <description>Digital I/O</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper0"/>
     <p svgId="connector3pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector11" name="D10">
   <description>Digital I/O, PWM and TX2</description>
   <views>
    <breadboardView>
     <p svgId="connector11pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector11pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector11pin" layer="copper0"/>
     <p svgId="connector11pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector4" name="D3">
   <description>Digital I/O and PWM</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper0"/>
     <p svgId="connector4pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector12" name="D11">
   <description>Digital I/O</description>
   <views>
    <breadboardView>
     <p svgId="connector12pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector12pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector12pin" layer="copper0"/>
     <p svgId="connector12pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector5" name="D4">
   <description>Digital I/O and PWM</description>
   <views>
    <breadboardView>
     <p svgId="connector5pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector5pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector5pin" layer="copper0"/>
     <p svgId="connector5pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector13" name="D12">
   <description>Digital I/O</description>
   <views>
    <breadboardView>
     <p svgId="connector13pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector13pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector13pin" layer="copper0" terminalId="connector13terminal"/>
     <p svgId="connector13pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector6" name="D5">
   <description>Digital I/O and PWM</description>
   <views>
    <breadboardView>
     <p svgId="connector6pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector6pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector6pin" layer="copper0"/>
     <p svgId="connector6pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector14" name="VBat">
   <description>Voltage Input, use 3V coin cell for real time clock</description>
   <views>
    <breadboardView>
     <p svgId="connector14pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector14pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector14pin" layer="copper0"/>
     <p svgId="connector14pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector31" name="AGND">
   <description>Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector31pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector31pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector31pin" layer="copper0"/>
     <p svgId="connector31pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector32" name="Vin">
   <description>3.7V to 5.5V </description>
   <views>
    <breadboardView>
     <p svgId="connector32pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector32pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector32pin" layer="copper0"/>
     <p svgId="connector32pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector33" name="A11">
   <description>Analog Input</description>
   <views>
    <breadboardView>
     <p svgId="connector33pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector33pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector33pin" layer="copper0"/>
     <p svgId="connector33pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector34" name="A10">
   <description>Analog Input</description>
   <views>
    <breadboardView>
     <p svgId="connector34pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector34pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector34pin" layer="copper0"/>
     <p svgId="connector34pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector35" name="AREF">
   <description>Aref</description>
   <views>
    <breadboardView>
     <p svgId="connector35pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector35pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector35pin" layer="copper0"/>
     <p svgId="connector35pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="female" id="connector36" name="VUSB">
   <description>VUSB</description>
   <views>
    <breadboardView>
     <p svgId="connector36pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector36pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector36pin" layer="copper0"/>
     <p svgId="connector36pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
  <bus id="GND"/>
  <bus id="3V3"/>
  <bus id="internal1"/>
  <bus id="internal2">
   <nodeMember connectorId="connector0"/>
   <nodeMember connectorId="connector16"/>
  </bus>
 </buses>
 <url>http://www.pjrc.com/teensy</url>
</module>
